{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Articles"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":2,"defined_names":9,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Articles","index":0,"n_rows":315,"n_cols":49,"rows_kept":315,"cut":false,"hidden":false,"merged":[]}
["code plomb","PLOMBERIE","Description plomb","Catégorie plomb","Taille plomb","PUV plomb","code elec","ELECTRICITE","Description elec","Catégorie elec","Taille elec","PUV elec","code carre","CARRELAGE","Description carre","Catégorie carre","Taille carre","PUV carre","code prest","PRESTATIONS","Description prest","Catégorie prest","Taille prest","PUV prest","code sani","SANITAIRE","Description sani","Catégorie sani","Taille sani","PUV sani","code plac","PLACARD","Description plac","Catégorie plac","Taille plac","PUV plac","code quinc","QUINCAILLERIE","Description  quinc","Catégorie quinc","Taille quinc","PUV quinc","code platre","PLATRERIE","Description platre","Catégorie platre","Taille platre","PUV platre"]
["WAV3025626","tuyau PVC 40 au ml","PVC 40","plomberie","Ml",2.4300000000000002,"SCH13392","mini coffret opale 4 pas ","coffret","électricité","u",8.49,"numcarre1","colle faience \"adesilex P22\"","colle","carrelage","U",30.05,"numprest1","achat de la cuisine meuble et plan de travail","cuisine","prestations","Mo",2313.14,"numsani1","lave mains HALL 50 X 25CM","lavabo","sanitaire","U",98.6,"numplac","faux plafond en lambris pvc blanc","lambris","placard","Mo",16.23,"numquinc1","chevilles placos 5 x 35","cheville","divers","U",1.25,"numplat1","plâtre de rebouchage","plâtre","plâtrerie","U",12.45,"plâtrerie"]
["NCLCH2","coude simple M/F 20' d.40","PVC 40","plomberie","U",3.18,"SCH13394","mini coffret opale 8 pas ","coffret","électricité","u",9.84,"numcarre2","colle sol pk2 anti-poussière(1sac de 25kg = env 5 à 9m²)","colle","carrelage","U",5.1840000000000002,"numprest2","achat de la hotte","cuisine","prestations","Mo",268.8,"numsani2","mitigeur lavabo \"grohe\" eurosmart","mitigeur","sanitaire","U",93.5,"numplac","tablette mélaminée blanche en 18mm","placard","placard","Mo",17.23,"numquinc2","chevilles placos 5 x 50","cheville","divers","U",1.25,"numplat2","enduit de lissage 5kg","enduit","plâtrerie","U",0,"quincaillerie"]
["NCLCH22","coude simple F/F 20' d.40","PVC 40","plomberie","U",3.18,"SCH13396","mini coffret opale 12 pas ","coffret","électricité","u",20.98,"numcarre3","ragréage \"plano 3\" en sac de 25 kg","joint","carrelage","U","18,58","numprest3","achat de l'évier ","cuisine","prestations","M²",302.54000000000002,"numsani3","vidage de  lavabo chromée","bonde/siphon","sanitaire","U",60.6,"numplac","support central","placard","placard","Mo",18.23,"numquinc3","chevilles crampon 8mm","cheville","divers",null,2.25,"numplat3","enduit de rebouchage 5kg","joint","plâtrerie","U",0,"prestations"]
["NCLCH4","coude simple M/F 45' d.40 ","PVC 40","plomberie","U",1.58,"SCH13398","mini coffret opale 16 pas ","coffret","électricité","u",24.36,"numcarre4","joint gris clair 111 (sac 25kg)","joint","carrelage","U",25.58,"numprest4","achat du mitigeur","cuisine","prestations","Mo",80.59,"numsani4","lot de 2 chevilles fixation murale","lavabo","sanitaire","U",5.69,"numplac","étagère blanche épaisseur 22mm  1530 x 600 à ajustée sur place","placard","placard","Mo",19.23,"numquinc4","chevilles placos 6 x 34","cheville","divers","U",3.25,"numplat4","map en sac de 25kg","joint","plâtrerie","M²",8.58,"sanitaire"]
["NCLCH44","coude simple F/F 45' d.40 ","PVC 40","plomberie","U",1.58,"SCH13401","opale coffret 1 rangée ","coffret","électricité","u",33.729999999999997,"numcarre5","joint sol gris ciment (sac 5kg)","joint","carrelage","U","14,68","numprest5","frais de déplacement","depla","prestations","Mo",62,"numsani5","bonde lavabo","bonde/siphon","sanitaire","U",3.7,"numplac","joues latérales blanche d'épaisseur 22mm","placard","placard","Mo",20.23,"numquinc5","rondelles Ø 10","rondelle","divers","U",4.25,"numplat5","rail R48 de 3ml","rail/mont","plâtrerie","Ml",3.25,"carrelage"]
["NCLCH6","coude simple M/F 67'30 d.40 ","PVC 40","plomberie","U",3.32,"SCH13402","opale coffret 2 rangées ","coffret","électricité","u",53.3,"numcarre6","joint blanc 100 (sac de 5kg)","joint","carrelage","U",{"$f":"#REF!*1.3","v":{"$error":"#REF!"}},"numprest6","pose de la cuisine ","cuisine","prestations","Mo",450,"numsani6","syphon lavabo bi-matière","bonde/siphon","sanitaire","U",15.85,"numplac","étagère blanche épaisseur 22mm  650 x 600 ","placard","placard","Mo",21.23,"numquinc6","rondelles Ø 8x40x2","rondelle","divers","U",5.25,"numplat6","stilmontant M48-35 L 3 m","rail/mont","plâtrerie","Ml",0,"plomberie"]
["NCLCH66","coude simple F/F 67'30 d.40 ","PVC 40","plomberie","U",2.09,"SCH13403","opale coffret 3 rangées ","coffret","électricité","u",77.599999999999994,"numcarre7","joint sol gris perle(sac 5kg)","joint","carrelage","U","10,2465","numprest7","pose du panneau, crédence et de la hotte","sdb","prestations","Mo",42,"numsani7","surface antidérapante sur commande","receveur","sanitaire","U","212,3","numplac","taquets support étagères ","placard","placard","Mo",22.23,"numquinc7","rondelles Ø 7","rondelle","divers","U",6.25,"numplat7","stilmontant M48-35 L 2,80 m","rail/mont","plâtrerie","Ml",0,"electricité"]
["NCLCH8","coude simple M/F 87'30 d.40 ","PVC 40","plomberie","U",1.78,"SCH13404","opale coffret 4 rangées ","coffret","électricité","u",108.26,"numcarre8","joint sol gris 113 (sac 5kg)","joint","carrelage","U",11.258999999999999,"numprest8","pose des placos","sdb","prestations","Mo","45","numsani8","vidage baignoire \"easybain\" a cable 650mm","bain","sanitaire","U",54.35,"numplac","crémaillère bois","placard","placard","Mo",23.23,"numquinc8","rondelles Ø 6","rondelle","divers","U",7.25,"numplat8","stilmontant M48-35 L 2,60 m","rail/mont","plâtrerie","Ml",2.68,"placard"]
["NCLCH88","coude simple F/F 87'30 d.40 ","PVC 40","plomberie","U",1.78,"SCH13421","porte opaque opale 1 r ","coffret","électricité","u",25.36,"numcarre9","croisillon de 2mm x 100","faience","carrelage","U",12.271499999999998,"numprest9","pose des placos platres au map","sdb","prestations","Mo",45,"numsani9","bonde de douche 90 turboflow cpot abs","bonde/siphon","sanitaire","U",33.01,"numplac","tasseaux 27 x 27","placard","placard","Mo",2.57,"numquinc9","vis torx 4 x 40","vis","divers",null,8.25,"numplat9","stilmontant M48-35 L 2,50 m","rail/mont","plâtrerie","Ml",2.4900000000000002]
["NCLFH","tampon de visite avec bouchon M/F d.40 ","PVC 40","plomberie","U",1.27,"SCH13422","porte opaque opale 2 r ","coffret","électricité","u",35.72,"numcarre10","croisillon de 4mm x 100","faience","carrelage","U",13.283999999999999,"numprest10","pose des rails et montants","sdb","prestations","Mo",45,"numsani10","sol de douche \"PANODUR LINEAL 90 x 90 avec bonde","receveur","sanitaire","U",464.01,"numplac","étagères blanches 560 x 440  en remplacement","cuisine","étagère","U",25,"numquinc10","vis torx 4 x 25","vis","divers",null,9.25,"numplat10","fourrure  en 3,00 Ml","rail/mont","plâtrerie","U",4.5]
["NCLFLEXH","manchette souple pour rénovation F/F d.40 ","PVC 40","plomberie","U",12.35,"SCH13423","porte opaque opale 3 r ","coffret","électricité",null,39.28,"numcarre11","joint de dilatation gris","joint","carrelage","U",14.296499999999998,"numprest11","pose des joints et finition à l'enduit","sdb","prestations","Mo","45","numsani11","barrette inox LINEAL  L69 pour LINEAL 90","bonde/siphon","sanitaire","U",54.08,"numplac","étagères blanches 935 x 480 en remplacement","cuisine","étagère","U",35,"numquinc11","vis torx 4 x 35","vis","divers","U",10.25,"numplat11","suspente super longue 220 mm","rail/mont","plâtrerie","U",6.76]
["NCLFLEXHM","manchette souple pour rénovation M/F d.40 ","PVC 40","plomberie","U",12.35,"SCH13424","porte opaque opale 4 r ","coffret","électricité","u",54.08,"numcarre12","beton pour chape","ciment","carrelage","U",18.309000000000001,"numprest12","dépose carrelage sol ","sdb","prestations","Mo",100,"numsani12","colonne de douche \"valentin\" modèle Opium rond avec des tablettes porte objets, pommeau rond Ø 300mm et mitigeur thermostatique anti brûlure","colonne","sanitaire","U",664.2,"numplac","étagères blanches 400x500 en remplacement","cuisine","étagère","U",25,"numquinc12","vis torx 5 x 70","vis","divers","U",11.25,"numplat12","rail clips optima  2,50","rail/mont","plâtrerie","U",5.38]
["NCLBH14","culotte simple M/F 45' d.40 ","PVC 40","plomberie","U",5.73,"SCH13425","porte transp.opale 1r ","coffret","électricité","u",26.11,"numcarre13","trappe de visite aimantée (baignoire)","faience","carrelage","U",16.3215,"numprest13","mise en place du micro-onde","sdb","prestations","Mo",3.33,"numsani13","paroi douche 1200 \"ALTERNA\" modèle night & day, verre transparent de 8mm  a portillon de 350 et barre de maintien, les parties aluminium sont chromées","paroi","sanitaire","U",716,"numplac","étagère d'angle a recoupée sur place","cuisine","étagère","U",35,"numquinc13","vis torx  3 ,5 x 13","vis","divers","U",12.25,"numplat13","placoplâtre hydrofuge BA13   2,6mx 1,20m ","placos","plâtrerie","U",24.95]
["NCLBH144","culotte simple F/F 45' d.40 ","PVC 40","plomberie","U",3.61,"SCH13426","porte transp.opale 2r ","coffret","électricité","u",35.31,"numcarre14","faience murale azt seasons 20 x60 blanche au m²","faience","carrelage","U",22.16,"numprest14","pose du carrelage au M²","sdb","prestations","Mo",45,"numsani14","plaque de douche \"robifix\"pour placo en PER 12","plomb","sanitaire","U",47.73,"numplac","chute de plan de travail 25mm hydro","cuisine","plan","U",25,"numquinc14","vis tête ronde 5 x 30","vis","divers","U",13.25,"numplat14","placos standard 2,50 x 1,20","placos","plâtrerie","U",14.15]
["NCLBH18","culotte simple M/F 87'30 d.40 ","PVC 40","plomberie","U",5.73,"SCH13427","porte transp.opale 3r ","coffret","électricité","u",40.06,"numcarre15","décor (par 2 carreaux)","faience","carrelage","U",18.346499999999999,"numprest15","pose carrelage antidérapant en entrée douche avec colle-joints époxy","sdb","prestations","Mo",65,"numsani15","plaque de douche\"robifix\" pour placo en PER 16","plomb","sanitaire","U",47.73,"numplac","barre de seuil alu saha 47mml83","cuisine","barsel","U",11.35,"numquinc15","silicone  acrylique blanc ","silicone","divers","U",14.25,"numplat15","placoplatre hydrofuge BA13    2,5m x 1,20m au m²","placos","plâtrerie","U",18.95]
["NCLBH188","culotte simple F/F 87'30 d.40 ","PVC 40","plomberie","U",5.73,"SCH13428","porte transp.opale 4r ","coffret","électricité","u",54.33,"numcarre16","carrelage sol azt seasons graphite 41 x 41 au M²","carrelage","carrelage","U",23.37,"numprest16","dépose de la baignoire et son bandeau","sdb","prestations","Mo",120,"numsani16","rallonge de 25mm chromée pour écarter mitigeur douche","plomb","sanitaire","U",8,"numplac","agglo hydrofuge 30 mm d'épaisseur","sdb","aglo","U",75,"numquinc16","silicone  blanc ","silicone","divers","U",15.25,"numplat16","laine de roche \"rockmur\" 1,35 x 0,6 ep 40 mm","isolation","plâtrerie","U",10.56]
["NCLTH188","té pied de biche F/F 87'30 d.40 ","PVC 40","plomberie","U",3.48,"SCH16156","IDCLICXE 63A 30 mA type A(protection générale et électroménager)embrochable","differentiel","électricité","u",194,"numcarre17","plinthe modèle \"Carbonara White\" 30,4 x 7,5 à la pièce","carrelage","carrelage","U",20.371500000000001,"numprest17","pose de la faïence forfait de 2 a 6 m² (colle incluse)","sdb","prestations","Mo",250,"numsani17","pack wc NEXO compact","toilette","sanitaire","U",303,"numplac","plaque de polystyrène noir a l'unité","sdb","aglo","U",22,"numquinc17","silicone  translucide","silicone","divers","U",16.25,"numplat17","boite de vis 25mm","vis","plâtrerie","M²",12.25]
["NCLTH188MF","té pied de biche M/F 87'30 d.40 ","PVC 40","plomberie","U",4.88,"SCH16158","IDCLICXE  30ma 40A type A (pour cuisine)embrochable","differentiel","électricité","u",115.41,"numcarre18","sous couche étanche\"prolicoat\" avant pose faience ","faience","carrelage","U",58.29,"numprest18","mise en place de l'étanchéité","sdb","prestations","Mo",45,"numsani18","robinet flotteur à alimentation latérale","toilette","sanitaire","U",28.35,"numplac","nez de mur en 70 prépeint","sdb","nez","U",15.28,"numquinc18","néoprène tube","silicone","divers","U",17.25,"numplat18","boite de vis 35mm","vis","plâtrerie","U",0]
["NCLKH","coulisse F/F d.40 ","PVC 40","plomberie","U",1.42,"SCH16160","IDCLICXE  30ma 40A type AC( pour habitation)embrochable","differentiel","électricité","u",93.36,"numcarre19","bande d'étanchéité pour les angles \"proliband\"","faience","carrelage","U",35.119999999999997,"numprest19","dépose/repose plan de travail jusque la plaque de cuisson","cuisine","prestations","Mo",45,"numsani19","robinet d'entrée d'eau de chasse 1/4 t 3/8","toilette","sanitaire","U",8.2100000000000009,"numplac","porte neo-style lm10-4 carreaux à peindre avec verre sati NOVO","cuisine","porte","U",268.45,"numquinc19","nettoyant inox 400ml","produit","divers","U",20.83,"numplat19","placojoint \"PR4\"","joint","plâtrerie","U",12.13]
["NCLM2H","manchon à butée F/F d.40 ","PVC 40","plomberie","U",0.74,"SCH16162","IDCLICXE  63A 30mA type AC (coupure générale)embrochable","differentiel","électricité","u",163.22,"numcarre20","bordures \"Steuler nice time tao\" K-NCT 5172","faience","carrelage","U",23.408999999999999,"numprest20","reconstruction entrée douche en béton","sdb",null,null,null,"numsani20","receveur PRIMA d'angle  blanc 1m x 1m","receveur","sanitaire","U",416,"numplac","mortaise pour poser les serrures","cuisine","porte","U",8.8000000000000007,"numquinc20","vis 5 x 90/47","vis","quincaillerie","U",22,"numplat20","semin bande armée","joint","plâtrerie","U",13.87]
["NCLZHH","manchette de réparation M d.40 ","PVC 40","plomberie","U",2.48,"SCH14910","peigne verticale \"opale\"","differentiel","électricité","u",13.82,"numcarre21","baguettePVC de finition d'angle RE 8","baguette","carrelage","U",24.421499999999998,"numprest21","pose du sol moduléo coupe au cutter donc sans poussières au M²","sdb","prestations","Mo",45,"numsani21","paroi douche 1/4 rond DOMINO , Portes pivotantes vers l'extérieure, passage de 71 cm, hauteur de 190cm","paroi","sanitaire","U",652.99,"numplac","ensemble poignée BERGEN sur Rosace","cuisine","porte","U",101.58,"numquinc21","vis 4 x 60","vis","quincaillerie","U",22,"numplat21","bande de joint ","joint","plâtrerie","U",9.75]
["NCLCM40","collier monobloc insert  d.40 gris ","PVC 40","plomberie","U",1.8,"SCH16724","DCLIC XE unipolaire 2 A de protection télérupteur et vmc embrochable","disjoncteur","électricité","U",29.47,"numcarre22","baguette finition d'angle RE 6 ","baguette","carrelage","U",{"$f":"#REF!*1.3","v":{"$error":"#REF!"}},"numprest22","pose plaque de cuisson sur prise et arrivée de gaz existants sans modification","cuisine","prestations","Mo",48,"numsani22","combinée de douche thermostatic PLENITUDE","colonne","sanitaire","U",369.29,"numplac","serrure encastrable ","cuisine","porte","U",17.899999999999999,"numquinc22","vis 4 x 30","vis","quincaillerie","U",22,"numplat22","couche de peinture d'impression","peinture","plâtrerie","U",58]
["NCLE4033F","embout mal ou fem d.40/50 filet 33/42 ","PVC 40","plomberie","U",5.96,"SCH16725","DCLIC XE unipolaire 10 A ( spot et lumière) embrochable","disjoncteur","électricité","U",20.53,"numcarre23","brique marena ondulée clair 19,8 x 19,8","murbriq","carrelage","U",8.8699999999999992,"numprest23","pose et raccordement évier sur arrivées et évacuations existantes sans modification","cuisine","prestations","Mo",44,"numsani23","kit auto siroc3 4rk","vmc","sanitaire","U",106.99,"numplac","paumelle de porte","cuisine","porte","U",12.35,"numquinc23","bombe de mousse","bbmou","quincaillerie","U",18,"numplat23","isolation phonique en rouleau 2 x 10 m x 0,60","isolation","plâtrerie","U",45]
["RPTSH","siphon  m.a.l. sortie horizontale","PVC 40","plomberie","U",9.09,"SCH16726","DCLIC XE unipolaire 16 A  (prise, frigo, hotte…) embrochable","disjoncteur","électricité","U",20.53,"numcarre24","1/2 brique marena ondulée clair 19,8 x 9,4","murbriq","carrelage","U",9.25,"numprest24","pose et raccordement d'un réfrigérateur ou congélateur sur installation aux normes, sans modification","cuisine","prestations","Mo",52,"numsani24","eco participation","eco","sanitaire","U",0.42,"numplac","lambris red cedar 11,5 x84 x 2130","porte","porte","U",57.88,"numquinc24","coulisse de tiroirs en 450 mm de long","couli","quincaillerie","U",15.25,"numplat24","isolation polystyrene noire la plaque de 1m x 1,20","isolation","plâtrerie","U",24.25]
["NCLYH42C","siphon simple m.a.l. sortie horizontale d ","PVC 40","plomberie","U",11.63,"SCH16727","DCLIC XE unipolaire 20 A  ( four ou/et LV ) embrochable","disjoncteur","électricité","U",20.53,"numcarre25","1/2 brique marena ondulée clair 19,8 x 9,5","murbriq","carrelage","U",13.25,"numprest25","pose et raccordement d'un groupe d'aspiration ou hotte décor murale (recyclage où évacuation) sur prise et évacuation en attente à l'emplacement prévue","cuisine","prestations","Mo",56,"numsani25","tuyau isolés en 80 de 3 m","vmc","sanitaire","U",59.35,"numplac","lasure longue durée \"BLANCHON\" incolore","porte","porte","U",32.68,"numquinc25","lyre gaz inox long 0m45 garatie a vie","gaz","quincaillerie","U",82.37,"numplat25","chevilles a frapper 6x50","placos","plâtrerie","U",12.95]
["NCLCO40","collier lyre  d.40 gris ","PVC 40","plomberie","U",1.35,"SCH16729","DCLIC XE unipolaire 32 A  (plaque induction,piano) obligatoire embrochable","disjoncteur","électricité","U",25.18,"numcarre26","crolisillon de montage et calage briques","murbriq","carrelage","U",5.38,"numprest26","pose et raccordement d'un four sur installation aux normes, et sans modification","cuisine","prestations","Mo",50,"numsani26","tuyau isolés en 125 de 3 m","vmc","sanitaire","U",65.89,"numplac","tasseaux 20 x 20","cuisine","plan","U",3.15,"numquinc26","scellement chimique ","sce","divers","U",13.9,"numplat26","placos sigma décor 2,60 x 1,20","placos","plâtrerie","U",24.56]
["NCLN40F","union 3 pieces a coller press. d.40 ","PVC 40","plomberie","U",15.47,"SCH16170","districlicxe 5M avec connecteur pour adapter embrochable sur coffret","disjoncteur","électricité","U",10.62,"numcarre27","primaire d'accrochage","carrelage","carrelage","U",15.28,"numprest27","pose et raccordement de la hotte centrale( ilôt ) sur arrivées existantes sans perçage du mur","cuisine","prestations","Mo",59,"numsani27","receveur TRENDY 100 X 80 blanc","receveur","sanitaire","U",650,"numplac","panneau médium 19mm 1700 x 900 ","cuisine","plan","U",120,"numquinc27","tamis 12 x 50","sce","divers","U",1.25,"numplat27","laine de verre 200mm en rouleau de 6,60 m²","isolation","plâtrerie","U",6.4]
["NCLMFA43","manchette femelle adaptation a visser d.40/32","PVC 40","plomberie","U",2.74,"SCH16171","districlicxe 8M avec connecteur pour adapter embrochable sur coffret","disjoncteur","électricité","U",12.56,"numcarre28","nouveauté sol synthétiques, insonore, resistant a l'eau ,rayure, tache, entretien facile","carrelage","carrelage",null,null,"numprest28","pose et raccordement  lave vaisselle ou lave linge sur installations électrique et plomberie existante aux normes en vigueur","cuisine","prestations","Mo",46,"numsani28","paroi de douche 1 fixe + 1 porte rentrante ,profil argent, verre sécurit clair","paroi","sanitaire","U",1492,"numplac","crédence inox 90 x 70","cuisine","cred","U",90.92,"numquinc28","goujons d'ancrage pour poteau","sce","divers","U",12.35,"numplat28","peinture sous couche placos","placos","plâtrerie","U",25]
["WAV3025627","tuyau PVC 32 au ml","PVC 32","plomberie","U",2.09,"SCH16172","districlicxe 13M avec connecteur pour adapter embrochable sur coffret","disjoncteur","électricité","U",16.14,"numcarre29","moduléo transform click CU 0,55MM , lames de 19,1x 131,6 (divers colori et référence a voir en magasin)","solsyntmodul","carrelage","M²",39.619999999999997,"numprest29","pose des meubles, vasque, mitigeur et miroirs avec tous les branchement et fixation","sdb","prestations","Mo",350,"numsani29","colonne de douche \"TOUAREG 2\" ELLE & LUI avec 2 étagères","colonne","sanitaire","U",745.63,null,null,null,null,null,null,null,null,null,null,null,null,"numplat29","peinture finitions blanc satiné","peinture","plâtrerie","U",38.99]
["NCLM2F","manchon a butee F/F d.32 ","PVC 32","plomberie","U",0.62,"SCH16173","districlicxe 18M avec connecteur pour adapter embrochable sur coffret","disjoncteur","électricité","U",22.52,"numcarre30","jackon/wedi de compensation d'épaisseur 6mm","faience","carrelage","U",16.579999999999998,"numprest30","pose du nouveau receveur avec ses branchements et étanchéité faite","sdb","prestations","Mo",45,"numsani30","evier inox structuré 1 cuve 1 égouttoir 1000 x 500 mm","evier","sanitaire","U",302.54000000000002]
["NCLCF4","coude 32 mm M/F 45'  ","PVC 32","plomberie","U",1.1299999999999999,"SCH16180","districlicxe 5M pour adapter embrochable sur coffret","disjoncteur","électricité","U",8.9600000000000009,"numcarre31","baguettes sous faience en rebord douche/baignoire \"PRO AS 20 BW\"","baguette","carrelage","U",25.58,"numprest31","pose du mitigeur et colonne","sdb","prestations","Mo",120,"numsani31","mitigeur thermostatic","evier","sanitaire","U",80.59]
["NCLCF44","coude 32mm F/F 45'  ","PVC 32","plomberie","U",1.1200000000000001,"SCH16181","districlicxe 8M pour adapter embrochable sur coffret","disjoncteur","électricité","U",11.51,"numcarre32","faïence rc destiny blanco 25 X 40 ","faïence","carrelage","U",19.559999999999999,"numprest32","pose du lave-vaisselle ","cuisine","prestations","Mo",35,"numsani32","kit de 50 briques pour paroi en pavé de verre ondulée neutre","mur","sanitaire","U",716]
["NCLCF6","coude pvc 32mm 67° M/F","PVC 32","plomberie","U",2.3199999999999998,"SCH16182","districlicxe 13M pour adapter embrochable sur coffret","disjoncteur","électricité","U",15.49,"numcarre33","faîence \"BALTICA\" 25 X 40 blanco au m²","faïence","carrelage","U",19.190000000000001,"numprest33","remplacement des prises et interrupteurs avec rainurage et remplacement ","cuisine","prestations","Mo",31,"numsani33","receveur SMO en marbre de synthèse recoupable 3cm possibilités 4 coloris","RECEVEUR","sanitaire","U",519.75]
["NCLCF66","coude pvc 32mm 67° F/F","PVC 32","plomberie","U",2.3199999999999998,"SCH16406","tlclic 16a 1ph n ","disjoncteur","électricité","U",37.01,"numcarre34","faîence \"BALTICA\" 25 X 40 mocca au m²","faïence","carrelage","U",19.190000000000001,"numprest34","pose du sèche serviette","sdb","prestations","Mo",80,"numsani34","porte \"swing-line\" pivotant avec fermeture sur paroi fixe L1400   H1950 extensible de 138,5 à 142,5","PAROI","sanitaire","U",558.9]
["NCLCF8","coude simple M/F 87'30 d.32 ","PVC 32","plomberie","U",1.33,"SCHS520204","interrupteur va et vient série\" ODACE\"","interrupteur","électricité","U",5.53,"numcarre35","listel \"baltico\" cenefa estonia beige a l'unité","faïence","carrelage","U",6.22,"numprest35","pose des tasseaux, du lambris et des angles au plafond du toilette","couloir","prestations","Mo",150,"numsani35","receveur 90 x 70 blanc antigliss",null,"sanitaire","U"]
["NCLCF88","coude simple F/F 87'30 d.32 ","PVC 32","plomberie","U",1.31,"SCHS520206","interrupteur poussoir série \"ODACE\"","interrupteur","électricité","U",10.64,"numcarre36","carrelage sol baltico 15 x 60 marron","carrelage","carrelage","U",19.190000000000001,"numprest36","pose des plinthes a la colle P22","couloir","prestations","Mo",3,"numsani36","receveur plato gama pizzarra natural 90 x 140 , possibilité de l'avoir en 4 coloris","RECEVEUR","sanitaire","U",522.45000000000005]
["NCLBF14","culotte simple M/F 45' d.32 ","PVC 32","plomberie","U",3.57,"SCHS520207","interrupteur volet roulant 2 poussoir blanc série \"ODACE\"","interrupteur","électricité","U",28.5,"numcarre37","carrelage antidérapant blanc 10 x 10","carrelage","carrelage","M²",31.18,"numprest37","pose des plans de travail, évier et plaques de cuisson","cuisine","prestations","Mo",254,"numsani37","sol de douche \"rovaro plus\" avec support base, en matère composite pour le montage  sur sol 1000 x 1200","RECEVEUR","sanitaire","U",1269.4000000000001]
["NCLBF144","culotte simple F/F 45' d.32 ","PVC 32","plomberie","U",2.25,"SCHS520214","interrupteur double va et vient  blanc série \"ODACE\"","interrupteur","électricité","U",15.93,"numcarre38","colle/joint époxy gris clair","joint","carrelage","U",55,"numprest38","pose des crédences stratifiées avec percage pour prises et interrupteurs au m²","cuisine","prestations","Mo",47.37,"numsani38","surface antidérapante","RECEVEUR","sanitaire","U",212.3]
["NCLBF188","culotte simple F/F 87'30 d.32 ","PVC 32","plomberie","U",3.57,"SCHS520216","interrupteur double poussoir blanc \"ODACE\"","interrupteur","électricité","U",25.7,"numcarre39","brique de béton cellulaire de 10 ep 60 x 50","ciment","carrelage","U",6.95,"numprest39","pose de la porte lave/linge et /où vaisselle","cuisine","prestations","Mo",47,"numsani39","paroi fixe 1000 x 2000 avec porte pivotante sur élément fixe a gauche1200 x 2000 transparent/profil argent poli ","PAROI","sanitaire","U",1497]
["NCLTF188","té pied de biche F/F 87'30 d.32 ","PVC 32","plomberie","U",2.94,"SCHS520227","interrupteur volet roulant 2 poussoir + stop blanc série \"ODACE\"","interrupteur","électricité","U",27.58,"numcarre40","les exclusifs \"blanco lustré 25 x 40 \"CADIX\"","faïence","carrelage","U",21.79,"numprest40","pose de la paroi avec ses étanchéités","sdb","prestations","Mo",150,"numsani40","sèche serviettes a eau chaude atoll spa966 watt H 1708 L 600","RADI","sanitaire","U",161.37]
["NCLTF188MF","té pied de biche M/F 87'30 d.32 ","PVC 32","plomberie","U",3.27,"SCHS520233","interrupteur VMC  \"ODACE\"","interrupteur","électricité","U",12.36,"numcarre41","listel \"iris iper A\" 2,8 x 20","faïence","carrelage","U",4.24,"numprest41","pose de la cuisine ","cuisine","prestations","Mo",850,"numsani41","robinet manuel ove équerre 15 x 21","RADI","sanitaire","U",13.4]
["NCLFF","tampon de visite avec bouchon M/F D.32","PVC 32","plomberie","U",1.22,"SCHS520243","interrupteur VMC + stop \"ODACE\"","interrupteur","électricité","U",26.1,"numcarre42","plinthe \"castille noir rectifiée 7,5 x 60 DL359 R ","plinte","carrelage","U",7.58,"numprest42","pose des lames de vinyles avec colle fournie","cuisine","prestations","Mo",45,"numsani42","coude de réglage ove 15 x 21 DN COMBI 2 NICKELE","RADI","sanitaire","U",10.55]
["NCLFLEXF","manchette souple pour rénovation F/F d.32 ","PVC 32","plomberie","U",10.33,"SCHS520285","interrupteur va et vient + poussoir \"ODACE\"","prises","électricité","U",22.08,"numcarre43","remboursement pose crédence","cred","cuisine","Mo",27.58,"numprest43","petites fournitures diverses de pose (vis,chevilles,équerres,silicone etc…)","divpose","prestations","Mo",61,"numsani43","éco-participation ","RADI","sanitaire","U",1.17]
["NCLCM32","collier monobloc insert p.7/150 d.32 gris ","PVC 32","plomberie","U",1.65,"SCHS520059","prise  2P+1T 16A \" ODACE\" ","prises","électricité","U",4.8499999999999996,"numcarre44","faïence RUGGINE TITANIO 33,3 X 44,6","faience","carrelage","M²",26.51,"numprest44","percage des portes pour mettre les charnières","cuisine","prestations","Mo",35,"numsani44","meuble sous vasque à 4 tiroirs 1400 blanc mat","meuble","sanitaire","U",752.51]
["NCLCO32","collier lyre insert p.7/150 d.32 gris ","PVC 32","plomberie","U",1.2,"SCHS520445","prise TV série \"ODACE\"","prises","électricité","U",11.88,"numcarre45","faïence RUGGINE (51C/P) 33,3 X 44,6","faience","carrelage","M²",26.51,"numprest45","panneau mélanminée blanc épaisseur 22 ajusté pour le meuble","cuisine","prestations","Mo",45,"numsani45","plan de synthèse 1410 mm à 2 vasques intégrées a 35 mm de chaque bord, prof 490mm H 25 mm","meuble","sanitaire","U",668.9]
["NCLKF","coulisse F/F d.32 ","PVC 32","plomberie","U",1.24,"SCHS520471","prise RJ45  modèle \"ODACE\"","prises","électricité","U",13.82,"numcarre46","faïence blanche 15 x 15 au m²","faïence","carrelage","M²",11.61,"numprest46","nombres d'entailles pour encastrement évier où plaque avec protection(colle où Rubson)","cuisine","prestations","Mo",39,"numsani46","mitigeur lavabos FG eurostyle new","meuble","sanitaire","U",136.29]
["NCLE32F","embout fileté F D.32","PVC 32","plomberie","U",5.4,"SCHS520496","conjoncteur téléphone  \"ODACE\"","prises","électricité","U",16.03,"numcarre47","panneau de compensation d'épaisseur en 6mm","faïence","carrelage","U",25.96,"numprest47","nombre d'heures de pose de travaux spéciaux suivant descriptif","cuisine","prestations","Mo",62.16,"numsani47","panneau miroir éclairant a leds en 1400 x 640 x 30 mm  style","meuble","sanitaire","U",330.27]
["NCLN32F","union 3 pièces a coller press. d.32 ","PVC 32","plomberie",null,11.76,"SCHS520712","odace styl pratic tel ","differentiel","électricité","U",9.26,"numcarre48","colle pour beton cellulaire","colle","carrelage","U",15.26,"numprest48","nombre de pose étagères et/où fileurs","cuisine","prestations","Mo",41,"numsani48","éco-participation ","meuble","sanitaire","U",0.1]
["NCLIJF","réduction incorporée M/F d.50/32 ","REDUCT PVC","plomberie",null,2.21,"SCH13413","repartiteur telephonique ","prises","électricité","U",20.36,"numcarre49","panneau wedi a recouper pour compenser le sol et le receveur et poser de la faïence","faïence","carrelage","U",25,"numprest49","nombre de pose et raccord de néons et spots sur arrivées électrique et interrupteurs existants sans modification","cuisine","prestations","Mo",54,"numsani49","style colonne L350 x 1440 x 318 mm blanc mat 1 porte, 4 étagères dont 3 en verre profilé ","meuble","sanitaire","U",584.45000000000005]
["NCLIH","réduction incorporée M/F d.40/32 ","REDUCT PVC","plomberie","U",1.08,"SCHS520690","odace 10 griffes ","prises","électricité","U",6.36,"numcarre50","carrelage FERROKER 44,3 X 44,3 ","carrelage","carrelage","M²",45.6,"numprest50","montage des caissons","cuisine","prestations","Mo",35,"numsani50","évier noir  granité \"opus schock\" de chez AQUATOP 1 bac, 1 égouttoir dim (mm)860 x 500 x 195","EVIER","sanitaire","U",416]
["NCLIJ","réduction incorporée M/F d.50/40 ","REDUCT PVC","plomberie","U",1.34,"SCHS520691","odace rallonges griffes ","prises","électricité","U",8.1,null,null,null,null,null,null,"numprest51","modification plan de travail pour la nouvelle plaque","cuisine","prestations","Mo",25,"numsani51","sèche serviettes électrique 750w ","RADI","sanitaire","U",258.86]
["NCLIT2","réduction extérieure excentrée MF D.100/80","REDUCT PVC","plomberie","U",10.53,"SCHS520702","odace styl plaque blc 1p ","prises","électricité","U",1.71,null,null,null,null,null,null,"numprest52","modification du meuble d'angle","cuisine","prestations","Mo",0,"numsani52","paroi fixe CORAIL 0 90° 900 mm poli-brillant vitre claire H 1900","PAROI","sanitaire","U",183.11]
["NCLT5","tampon de réduction simple M/F d.100/50 ","REDUCT PVC","plomberie","U",10.79,"SCHS520704","odace styl plaq blc 2p71 ","prises","électricité","U",4,null,null,null,null,null,null,"numprest53","modification de la plomberie par rainurage pour brancher le mitigeur  et raccorder l'évacuation","sdb","prestations","Mo",85,"numsani53","paroi mobile CORAIL 1000 mm poli-brillant vitre claire H 1900, ouverture intérieure extérieure","PAROI","sanitaire","U",342.81]
["NCLTT5","tampon de réduction pour tube M/F d.93/50 ","REDUCT PVC","plomberie","U",10.79,"SCHS520706","odace styl plaq blc 3p71 ","prises","électricité","U",7.89,null,null,null,null,null,null,"numprest54","ml de pose des éléments du bas, haut, armoires …","cuisine","prestations","Mo",36,"numsani54","receveur KINESURF 100 x 90 cm H 3cm anti dérapant","RECEVEUR","sanitaire",null,475.2]
["NCLR4","tampon de réduction simple M/F d.80/40 ","REDUCT PVC","plomberie","U",10.85,"SCHS520708","odace styl plaq blc 4p71 ","prises","électricité","U",10.55,null,null,null,null,null,null,"numprest55","mise en déchetterie des gravas","dechet","prestations","Mo",33,"numsani55","éco-participation ","eco","sanitaire","U",0.17]
["NCLT54","tampon de réduction double M/F d.100/50/40 ","REDUCT PVC","plomberie","U",11.4,"SCHS520666","odace obturateur blc vis ","prises","électricité","U",7.2,null,null,null,null,null,null,"numprest56","frais de déplacement ","depla","prestations","Mo",50,"numsani56","hotte casquette ROBLIN 5102026","Hotte","cuisine","U",233]
["NCLT6","tampon de réduction simple M/F d.100/63 ","REDUCT PVC","plomberie","U",11.39,"SCHALB71819","couvercle rond boite d67 ","prises","électricité","U",1.59,null,null,null,null,null,null,"numprest57","pose du caniveau avec ses raccords et étanchéités","sdb","prestations","Mo",45,"numsani57","éco-participation ","Hotte","cuisine","U",1.9]
["NCLT8","tampon de réduction simple M/F d.100/80 ","REDUCT PVC","plomberie","U",11.39,"SCHALB71820","couvercle carre boite d85 ","prises","électricité","U",2.83,null,null,null,null,null,null,"numprest58","dépose de l'ancienne paroi","sdb","prestations","Mo",45,"numsani58","receveur flight blanc 100 x 70 x 4 cm","RECEVEUR","sdb","U",468]
["NCLTT4","tampon de réduction pour tube M/F d.93/40 ","REDUCT PVC","plomberie","U",10.69,"LEG31490","sort.de cables 20/32a 95x95mm ","prises","électricité","U",6.44,null,null,null,null,null,null,"numprest59","dépose de l'ancienne baignoire","sdb","prestations","Mo",75,"numsani59","receveur dalle latitude en grès 100 x 90","RECEVEUR","sdb","U",536.75]
["NCLTT44","tampon de réduction pour tube M/F d.93,6/4 ","REDUCT PVC","plomberie","U",10.79,"LEG55849","cadre pour prises 20a et 32a ","prises","électricité","U",8.52,null,null,null,null,null,null,"numprest60","dépose muret d'entrée","sdb","prestations","Mo",75,"numsani60","bonde slim de douche extra plate 60mm","RECEVEUR","sdb","U",47]
["NCLT3","tampon de réduction simple M/F d.100/32 ","REDUCT PVC","plomberie","U",11.39,"LEG664798","cadre saillie 1p blanc ","prises","électricité","U",5.81,null,null,null,null,null,null,"numprest61","dépose de la faîence","sdb","prestations","Mo",150,"numsani61","jeu de 11 pieds reglables pour receveur flight","RECEVEUR","sdb","U",12.54]
["NCLR5","tampon de réduction simple M/F d.80/50 ","REDUCT PVC","plomberie","U",10.85,"LEG664799","cadre saillie 2p blanc ","prises","électricité","U",8.66,null,null,null,null,null,null,"numprest62","découpe plan de travail pour encastrer le nouvel évier et plaque","cuisine","prestations","Mo",65,"numsani62","colonne combi croma100 vario/ecostat comfort avec mitigeur","MITIGEUR","sdb","U",250]
["NCLR6","tampon de réduction simple M/F D.80/63","REDUCT PVC","plomberie","U",10.86,"LEG664795","cable blanc ","boitiers","électricité","U",4.1900000000000004,null,null,null,null,null,null,"numprest63","carrotage pour passer tuyau évacuation","aera","prestations","Mo",45,"numsani63","barre de douche croma 100","MITIGEUR","sdb","U",113.71]
["NCLL4","tampon deréduction simple M/F d.63/40 ","REDUCT PVC","plomberie","U",8.5500000000000007,"SCHS520762","ODACE STYL BOITE BLANC 1P ","boitiers","électricité","U",6.67,null,null,null,null,null,null,"numprest64","carrotage du mur avec fourniture tuyau pvc ","aera","prestations","Mo",130,"numsani64","porte pivotante ouverture int/ext poli brillant verre granité","PAROI","sdb","U",900.9]
["NCLL5","tampon de réduction simple M/F d.63/50 ","REDUCT PVC","plomberie","U",8.5500000000000007,"SCHS520764","ODACE STYL BOITE BLANC 2P ","boitiers","électricité","U",9.11,null,null,null,null,null,null,"numprest65","pose du primaire d'accrochage fourni","sdb","prestations","Mo",45,"numsani65","siège rembourré avec dossier et accoudoirs","siège","sdb","U",304.66000000000003]
["NCLT4","tampon de réduction simple M/F D.100/40","REDUCT PVC","plomberie","U",11.05,"SCHS520662","odace sort cable blc vis ","boitiers","électricité","U",7.69,null,null,null,null,null,null,"numprest66","frais de déplacement","dépla","prestations","Mo",50,"numsani66","barre d'appui coudée angle 135° symétrique 265 x 265 mm","barre","sdb","U",50.69]
["NCLT44","tampon de réduction simple M/F d.100/40/40 ","REDUCT PVC","plomberie","U",10.79,"SCHALB71320","boitier à placos Ø67 p40","boitiers","électricité","U",0.98,null,null,null,null,null,null,"numprest67","supplément pour ajustage de la porte d'angle et de la tôle sous évier en accord avec TONY","sdb","prestations","Mo",50,"numsani67","réducteur de pression en entrée chauffe eau","réduc","buand","U",42.55]
["NCLV10","tampon de réduction simple M/F D.110/100","REDUCT PVC","plomberie","U",14.02,"SCHALB71322","boitier à placos Ø67 p50","boitiers","électricité","U",1.76,null,null,null,null,null,null,"numprest68","dépose du radiateur","sdb","prestations","Mo",80,"numsani68","four micro-ondes WHIRPOOL GT281WH","MO","cuisine",null,124.17]
["NCLX10","tampon de réduction simple M/F d.125/100 ","REDUCT PVC","plomberie","U",14.05,"SCHALB71332","boite double 71 Ø67 p 40","boitiers","électricité","U",5.42,null,null,null,null,null,null,"numprest69","frais de déplacement ","dépla","prestations","U",50,"numsani69","eco participation",null,null,null,1.67]
["GUR19193","flexible gpl nf inox 1m blister ","FLEXIBLE","plomberie","U",56.93,"SCHALB71335","boite triple entraxe 71 Ø67 P40","boitiers","électricité","U",6.61,null,null,null,null,null,null,"numprest70","dépose de l'ancien évier ","cuisine","prestations","U",45]
["GUR19195","flexible gpl nf inox 1,50m blister ","FLEXIBLE","plomberie","U",62.56,"SCHALB71339","boite double H/V entraxe 71 Ø67 P50","boitiers","électricité","U",10.19,null,null,null,null,null,null,"numprest71","pose du nouvel évier avec tous ses raccords faits","cuisine","prestations","U",65]
["GUR19196","flexible gpl nf inox 2m blister ","FLEXIBLE","plomberie","U",71.25,"SCHALB71334","boite triple H/V entraxe 71 Ø67 P50","boitiers","électricité","U",8.1,null,null,null,null,null,null,"numprest72","déplacement de la prise four et réfrigérateur","cuisine","prestations","U",20]
["GUR18513","flexible gn nf inox 1m blister ","FLEXIBLE","plomberie","U",56.93,"SCHIMT35000","boite double étanche 71 Ø 67 P40","boitiers","électricité","U",7.34,null,null,null,null,null,null,"numprest73","mise en place de la peinture d'impression","placos","prestations","U",45]
["GUR18514","flexible gn nf inox 1,25m blister ","FLEXIBLE","plomberie","U",67.5,"SCHIMT35001","boitier à placos étanche Ø67 p40","boitiers","électricité","U",1.9,null,null,null,null,null,null,"numprest74","dépose du lavabo et miroir","sdb","prestations","Mo",45]
["GUR18515","flexible gn nf inox 1,50m blister ","FLEXIBLE","plomberie","U",62.56,"SCHIMT35002","boitier à placos étanche Ø67 p50","boitiers","électricité","U",2.37,null,null,null,null,null,null,"numprest75","dépose du receveur ","sdb","prestations","Mo",45]
["GUR18516","flexible gn nf inox 2m blister ","FLEXIBLE","plomberie","U",71.25,"SCHIMT35031","boite triple étanche 71 Ø67 ",null,null,null,11.65,null,null,null,null,null,null,"numprest76","dépose de la colonne de douche","sdb","prestations","Mo",45]
["SHE298501","flexible sani dn8 inox l300 F/F 15/21 ","FLEXIBLE","plomberie","U",3.75,"SCHIMT35032","multifix air b d67 1p p47 ","boitiers","électricité","U",1.91,null,null,null,null,null,null,"numprest77","démolition du pied d'entrée de douche","sdb","prestations","Mo",35]
["SHE298502","flexible sani dn8 inox l300 F/F 15/21 ","FLEXIBLE","plomberie","U",2.87,"SCHIMT35034","multifix air b d85 1p p47 ","boitiers","électricité","U",8,null,null,null,null,null,null,"numprest78","pose du receveur avec réfection étanchéité","sdb","prestations","Mo",45]
["SHE298516","flexible sani dn8 inox l300 M/F12/17 ","FLEXIBLE","plomberie","U",3.08,"SCHALB71361","boîte ronde 1p 40","boitiers","électricité","U",1.74,null,null,null,null,null,null,"numprest79","pieds pour  réhausse du receveur ","sdb","prestations","kit",58]
["SHE298517","flexible sani dn8 inox l300 F/F12/17","FLEXIBLE","plomberie","U",2.68,"SCHALB71385","boitiers a placos Ø 85 profondeur 40","boitiers","électricité","U",8.34,null,null,null,null,null,null,"numprest80","reconstruction du pied d'entrée au beton","sdb","prestations","Mo",55]
["SHE298522","flexible sani dn8 inox l500 F/F 15/21 ","FLEXIBLE","plomberie","U",3.54,"SCHALB71386","boitiers a placos Ø 85 profondeur 50","boitiers","électricité","U",9.3800000000000008,null,null,null,null,null,null,"numprest81","pose des galets fournis","sdb","prestations","Mo",45]
["SHE298530","flexible sani dn10 inox l500 F/F 20/27","FLEXIBLE","plomberie","U",8.07,"SCHALB71614","couvercle rond boite d40 ","boitiers","électricité","U",1.35,null,null,null,null,null,null,"numprest82","mise en place de l'étanchéité","sdb","prestations","Mo",45]
["SHE298531","flexible sani dn10 inox l1000 F/F 20/27 ","FLEXIBLE","plomberie","U",12.76,"CAP736419","miniclips ø 40 ","fils","électricité","Ml",2.59,null,null,null,null,null,null,"numprest83","frais de déplacement ","dépla","prestations","U",62]
["SHE298534","flexible sani dn8 inox l500 M/F 12/17 ","FLEXIBLE","plomberie","U",3.75,"IBOBDD150X110G","boite de derivation 50x110","fils","électricité","Ml",19.850000000000001,null,null,null,null,null,null,"numprest84","mise en déchetterie des gravas","dechet","prestations","U",33]
["SHE298537","flexible sani dn8 inox l300 M3/8-F15/21 ","FLEXIBLE","plomberie","U",6.64,"FIL000105","Fil h07vu 1,5mm²  (V/J,R , B) ","fils","électricité","Ml",0.93,null,null,null,null,null,null,"numprest85","dépose de la paroi","sdb","prestations","Mo",45]
["SHE298557","flexible sani dn10 inox l300 mf1/2 ","FLEXIBLE","plomberie","U",8.16,"FIL001005","Fil h07vu 2,5mm²  (V/J,R , B) ","fils","électricité","Ml",1.5,null,null,null,null,null,null,"numprest86","pose des compensateurs d'épaisseur","sdb","prestations","Mo",25]
["SHE298569","flexible sanitaire inox l500 F/F 12/17 ","FLEXIBLE","plomberie","U",3.3,"FIL002705","Fil h07vr 6 mm²  (V/J,R , B) ","fils","électricité","Ml",4.17,null,null,null,null,null,null,"numprest87","modification de la plomberie pour raccorder la baignoire","sdb","prestations",null,55]
["CMPE211084001","réduction M/M 15/21-12/17","METAL-reduit","plomberie","U",2.0299999999999998,"FIL003405","Fil h07vr 10 mm²  (V/J,R , B) ","fils","électricité","Ml",8.4600000000000009,null,null,null,null,null,null,"numprest88","montage de la paroi de briques de verre","sdb","prestations","Mo",42]
["CMPE211087001","réduction brut M/F 12/17 -15/21 ","METAL-reduit","plomberie","U",2.93,"FIL004005","Fil h07vr 16mm²  (V/J,R , B) ","gaines","électricité","Ml",13.49,null,null,null,null,null,null,"numprest89","pose da la nouvelle paroi, du tabouret et la barre  avec l'étanchéité faite","sdb","prestations","Mo",150]
["CMPE122004001","manchon réduit M/M 3/4-15/21","METAL-reduit","plomberie","U",2.92,"FIL026504","Fil gainés R2V CU 3G1,5  ","gaines","électricité","Ml",1.28,null,null,null,null,null,null,"numprest90","dépose du lavabo, toilette, portes","sdb","prestations","Mo",55]
["CMPE122006001","manchon dbl F réduit  15/21-12/17","METAL-reduit","plomberie","U",4.13,"FIL026704","Fil gainés R2V CU 3G2,5 ","gaines","électricité","Ml",1.99,null,null,null,null,null,null,"numprest91","démolition de la cloison et rebouchage de la semelle vide au béton","sdb","prestations","Mo",250]
["CMPE211131001","manchon  F 15/21-15/21","METAL-reduit","plomberie","U",4.13,"FIL 027104","Fil gainés R2V CU 3G6 ","gaines","électricité","Ml",6,null,null,null,null,null,null,"numprest92","creusage du sol pour encastrer le receveur et son syphon","sdb","prestations","Mo",150]
["CMPE211108001","reduit M/F 15/21- 20/27","METAL-reduit","plomberie","U",3.35,"ARD05116","gaine passe-fils Ø16 avec tire fils au ml","fils","électricité","Ml",0.81,null,null,null,null,null,null,"numprest93","pose des barres de maintien","sdb","prestations","Mo",45]
["CMPE211105001","reduit M/F 12/17-15/21","METAL-reduit","plomberie","U",2.06,"ARD05120","gaine passe-fils Ø20 avec tire fils au ml ","gaines","électricité","U",0.85,null,null,null,null,null,null,"numprest94","pose du lavabo et ses branchement","sdb","prestations","Mo",80]
["CMPE122017001","reduit M/F 15/21-12/17 ","METAL-reduit","plomberie","U",1.61,"ARD05125","gaine passe-fils Ø25 avec tire fils au ml","gaines","électricité","U",1.5,null,null,null,null,null,null,"numprest95","pose de l'armoire et l'éclairage","sdb","prestations","Mo",45]
["CMPE122026001","manchon égal F/F 15/21 ","METAL-reduit","plomberie","U",2.2400000000000002,"ARD05132","gaine passe-fils Ø32 avec tire fils au ml","gaines","électricité","U",2.75,null,null,null,null,null,null,"numprest96","pose du receveur et son étanchéité","sdb","prestations","Mo",80]
["CMPE211074001","réduction à butée M/F 15/21","METAL-reduit","plomberie","U",2.15,"ARD09016","gaine Ø 16 préfilé 3 x 1,5 B-R-J/V","gaines","électricité","U",4.09,null,null,null,null,null,null,"numprest97","pose du chassis et du toilette","sdb","prestations","Mo",80]
["CMP1616","coude M 12/17 ","METAL-coude","plomberie","U",3.41,"ARD09031","pref 3x2,5 b.n. v/j 20 ","gaines","électricité","U",5.17,null,null,null,null,null,null,"numprest98","pose du ragréage au m²","terrasse","prestations","Mo",45]
["CMP1617","coude M 15/21'","METAL-coude","plomberie","U",3.94,"IBO IRL3321D16TG","tube  IRL 16","gaines","électricité","U",0.69,null,null,null,null,null,null,"numprest99","pose du support Natte didra","terrasse","prestations","Mo",45]
["CMP1625","coude F  12/17 ","METAL-coude","plomberie","U",3.35,"IBO IRL3321D20TG","tube  IRL 20","gaines","électricité","U",0.9,null,null,null,null,null,null,"numprest100","pose du carrelage sur marche en sortie de porte fenêtre","terrasse","prestations","Mo",45]
["CMP1633","coude M/F 12/17 ","METAL-coude","plomberie","U",4.13,"IBO IRL3321D25TG","tube  IRL 25 ","gaines","électricité","U",1.32,null,null,null,null,null,null,"numprest101","pose des barrières  avec modification des nouvelles","terrasse","prestations","Mo",45]
["CMPE212020001","coude M/F 15/21 ","METAL-coude","plomberie","U",4.75,"IBO IRL3321D32TG","tube  IRL 32","gaines","électricité","U",1.96,null,null,null,null,null,null,"numprest102","remplacement du placos dans la cuisine sous cheminée par un neuf","cuisine","prestations","Mo",45]
["DU713020","té F 12/17 ","METAL-té","plomberie","U",2.23,"IBOCUG16H","coude IRL de 16 ","gaines","électricité","U",3.65,null,null,null,null,null,null,"numprest103","reprise des joints","cuisine","prestations","Mo",45]
["DU713025","té F 15/21 ","METAL-té","plomberie","U",2.78,"IBOCUG20H","coude IRL de 20 ","gaines","électricité","U",3.84,null,null,null,null,null,null,"numprest104","pose du toilette fourni","toilettes","prestations","Mo",45]
["CMPE212040001","té M 15/21","METAL-té","plomberie","U",4.03,"IBOCUG25H","coude IRL de 25 ","gaines","électricité","U",5.36,null,null,null,null,null,null,"numprest105","dépose des plaques et évier","cuisine","prestations","Mo",45]
["CMPE212033001","té F 15/21","METAL-té","plomberie","U",5.16,"IBOCUG32H","coude IRL de 32 ","gaines","électricité","U",7.74,null,null,null,null,null,null,"numprest106","dépose des plans de travail ","cuisine","prestations","Mo",45]
["CMP8514010","té égal 10","METAL-té","plomberie","U",9.7799999999999994,"IBO MAG16H","manchon  IRL de 16 ","fixation","électricité","U",0.76,null,null,null,null,null,null,"numprest107","pose de la plaque fournie","cuisine","prestations","Mo",45]
["CMP8514012","té égal 12","METAL-té","plomberie","U",7.89,"IBO MAG20H","manchon  IRL de 20 ","fixation","électricité","U",0.73,null,null,null,null,null,null,"numprest108","branchement de l'évier","cuisine","prestations","Mo",38]
["CMP8514014","té égal 14 ","METAL-té","plomberie","U",12.67,"IBO MAG25H","manchon  IRL de 25 ","fixation","électricité","U",1.01,null,null,null,null,null,null,"numprest109","déplacement et remplacement d'un mitigeur à LOCQUIREC","cuisine","prestations","Mo",60]
["CMP8514016","té égal 16 ","METAL-té","plomberie","U",13.52,"IBO MAG32H","manchon  IRL de 32 ","fixation","électricité","U",1.5,null,null,null,null,null,null,"numprest110","pose de la faience fournie dans la douche de l'appartement du haut à droite(colle et joint) inclus","sdb","prestations","Mo",150]
["CMP8514018","té égal 18","METAL-té","plomberie","U",27.68,"LEG30027","moulure 40x20 blanc ss cloison ","fixation","électricité","U",9.2200000000000006,null,null,null,null,null,null,"numprest111","pose des étagères fournies dans le placard de la chambre de l'étage et dans le meuble de la cuisine","chambre","prestations","Mo",100]
["CMP8500042","union droit  M 10-15/21","METAL-union","plomberie","U",4.87,"BIZ710225","colliers biz clips simple16","fixation","électricité","U",38.78,null,null,null,null,null,null,"numprest112","pose du parquet fourni a landévénnec","sdb","prestations","Mo",50]
["CMP8501042","union droit F 10-15/21","METAL-union","plomberie","U",4.87,"BIZ710226","colliers biz clips simple 20 ","fixation","électricité","U",40.67,null,null,null,null,null,null,"numprest113","pose de la porte coulissante","sdb","prestations","Mo",180]
["CMP8501043","union droit F 12-15/21","METAL-union","plomberie","U",4.5199999999999996,"BIZ710227","colliers biz clips simple 25 ","fixation","électricité","U",42.53,null,null,null,null,null,null,"numprest114","pose du tabouret de douche","sdb","prestations","Mo",50]
["CMP8501034","union droit F 14-12/17","METAL-union","plomberie","U",5.82,"BIZ710228","colliers biz clips  double 20 ","fixation","électricité","U",51.23,null,null,null,null,null,null,"numprest115","modification de l'électricité en vue de la pose des spots","sdb","prestations","Mo",45]
["CMP8501047","union droit F 18-15/21","METAL-union","plomberie","U",12.4,"BIZ710229","colliers biz clips  double 25 ","fixation","électricité","U",34.03,null,null,null,null,null,null,"numprest116","recherche où se trouve le point bas du  tuyau pour l'évacuation de la douche ","sdb","prestations","Mo",45]
["CMP8500033","union droit M 12-12/17","METAL-union","plomberie","U",3.2,"BIZ710330","colliers biz clips  double 16MM ","fixation","électricité","U",66.89,null,null,null,null,null,null,"numprest117","pose de la baignoire sur tasseaux","sdb","prestations","Mo",65]
["CMP8500034","union droit M 14-12/17 ","METAL-union","plomberie","U",6.03,"BIZ710332","colliers biz clips simple 32MM ","fixation","électricité","U",49.4,null,null,null,null,null,null,"numprest118","dépose de la baignoire","sdb","prestations","Mo",45]
["CMP8500047","union droit M 18-15/21","METAL-union","plomberie","U",12.4,"BIZ320001","barrettes dominos 2,5mm² noires ","connectique","électricité","U",1.66,null,null,null,null,null,null,"numprest119","modification de la plomberie pour le nouveau mitigeur","sdb","prestations","Mo",45]
["DU712035","raccord bic M 10 12/17 ","METAL-raccord","plomberie","U",3.81,"BIZ320002","barrettes dominos 6mm² noires ","connectique","électricité","U",1.95,null,null,null,null,null,null,"numprest120","pose du mitigeur et colonne avec ses branchements","sdb","prestations","Mo",65]
["DU712050","raccord bic M 12 12/17 ","METAL-raccord","plomberie","U",3.91,"BIZ320003","barrettes dominos 10mm² noires ","connectique","électricité","U",2.59,null,null,null,null,null,null,"numprest121","pose du receveur de douche avec ses branchements et son étanchéité","sdb","prestations","Mo",55]
["DU712270","raccord bic F 12 12/17 ","METAL-raccord","plomberie","U",4.18,"BIZ320004","barrettes dominos 16mm² noires ","connectique","électricité","U",4.3499999999999996,null,null,null,null,null,null,"numprest122","pose de la colonne de douche","sdb","prestations","Mo",45]
["DU712055","raccord bic M 12 15/21 ","METAL-raccord","plomberie","U",4.8,"BIZ320005","barrettes dominos 25mm² noires ","connectique","électricité","U",10.01,null,null,null,null,null,null,"numprest123","pose de la paroi avec ses étanchéités","sdb","prestations","Mo",65]
["DU712065","raccord bic M 14 12/17 ","METAL-raccord","plomberie","U",5.86,"BIZ300306","borne opaque 2 entrées ","connectique","électricité","U",12.88,null,null,null,null,null,null,"numprest124","création du support douche en béton","sdb","prestations","Mo",55]
["DU712070","raccord bic M  14 15/21 ","METAL-raccord","plomberie","U",4.87,"BIZ300307","borne opaque 3 entrées ","connectique","électricité","U",16.2,null,null,null,null,null,null,"numprest125","création des murets de bord de baignoire","sdb","prestations","Mo",55]
["DU712290","raccord bic F 14 15/21 ","METAL-raccord","plomberie","U",5.22,"BIZ300308","borne opaque 4 entrées ","connectique","électricité","U",19.7,null,null,null,null,null,null,"numprest126","modification de la plomberie par rainurage pour brancher le mitigeur  et raccorder l'évacuation","sdb","prestations","Mo",450]
["DU712080","raccord bic M 16 15/21 ","METAL-raccord","plomberie",null,5.08,"BIZ300309","borne opaque 5 entrées ","connectique","électricité","U",9.85,null,null,null,null,null,null,"numprest127","échange de la bonde","cuisine","prestations","Mo",25]
["DU712090","raccord bic M 18 20/27 ","METAL-raccord","plomberie",null,9.26,"BIZ300310","borne opaque 8 entrées ","connectique","électricité","U",21.23,null,null,null,null,null,null,"numprest128","pose des nez de cloisons","sdb","prestations","Mo",45]
["DU712310","raccord bic F 18 20/27 ","METAL-raccord","plomberie","U",10.09,"BIZ300422","bornes christal 2 entrées ","connectique","électricité","U",17.149999999999999,null,null,null,null,null,null,"numprest129","pose du meuble","sdb","prestations","Mo",25]
["DU713250","coude F 12/17 ","METAL-coude","plomberie","U",1.93,"BIZ300433","bornes christal 3 entrées ","connectique","électricité","U",19.84,null,null,null,null,null,null,"numprest130","mise en œuvre du béton","sdb","prestations","Mo",45]
["DU713251","coude F 15/21 ","METAL-coude","plomberie","U",2.3199999999999998,"BIZ300444","bornes christal 4 entrées ","connectique","électricité","U",22.53,null,null,null,null,null,null,"numprest131","création d'un muret pour poser les produits de douche","sdb","prestations","Mo",45]
["CMPE122003001","manchon double F réduit,  15/21 - 20/27 ","METAL-reduit","plomberie","U",4.4800000000000004,"BIZ300455","borne christal 5 entrées ","connectique","électricité","U",13.96,null,null,null,null,null,null,"numprest132","mise en place des compensateurs","sdb","prestations","Mo",45]
["CMPE211139001","mamelon M/M 12/17","METAL-mamelon","plomberie","U",1.2,"BIZ300488","borne christal 8 entrées ","connectique","électricité","U",19.34,null,null,null,null,null,null,"numprest133","création d'un plafond en placos hydro","sdb","prestations","Mo",45]
["CMPE211140001","mamelon M/M 15/2 1","METAL-mamelon","plomberie","U",1.56,"BIZ300490","borne luminaire 1 souple 1 rigide ","connectique","électricité","U",37.36,null,null,null,null,null,null,"numprest134","tuyau semi rigide de 125 pour la hotte","cuisine","prestations","Mo",28.52]
["CMPE211141001","mamelon M/M 20/27 ","METAL-mamelon","plomberie","U",2.36,"BIZ300491","borne luminaire 1 souple 2 rigides","connectique","électricité","U",38.49]
["CMPE211167001","bouchon F 12/17 ","METAL-bouchon","plomberie","U",1.07,"ivvalu","interrupteur va et vient série\" ODACE\" alu","interrupteur","électricité","U",5.96]
["CMPE211168001","bouchon F 15/21","METAL-bouchon","plomberie","U",1.48,"2p1t16","prise  2P+1T 16A \" ODACE\" alu","prises","électricité","U",5.09]
["CMPE211170001","bouchon F 20/27 ","METAL-bouchon","plomberie","U",2.57,"ods1palu","odace styl plaque alu 1p ","prises","électricité","U",2.61]
["CMPE122040001","bouchon M 12/17","METAL-bouchon","plomberie","U",1.02,"ods2palu","odace styl plaq alu 2p71 ","prises","électricité","U",6.58]
["CMPE211158001","bouchon M 15/21","METAL-bouchon","plomberie","U",1.65,"E13971","kit spot 230 v led GU10 à LED 6 W","spot","électricité","U",38]
["CMPE211160001","bouchon M 20/27","METAL-bouchon","plomberie","U",2.69,"E08525","kit spot 230 v led GU5 spécial SDB à LED 6 W","spot","électricité","U",49.2]
["PMC039020","rallonge 7x150 acier 20 ","METAL-collier","plomberie","U",0.3,"E13320","aérateur silent 200CZ,  silencieux, clapet anti retour","sdb","électricité","U","143,72"]
["PMC039030","rallonge 7x150 acier 30 ","METAL-collier","plomberie","U",0.38]
["PMC039040","rallonge 7x150 acier 40 ","METAL-collier","plomberie","U",0.45]
["PMC005012","collier double 7x150 10x12 ","METAL-collier","plomberie","U",0.39]
["PMC005014","collier double 7x150 12x14 ","METAL-collier","plomberie","U",0.42]
["PMC005016","collier double 7x150 14x16 ","METAL-collier","plomberie","U",0.43]
["PMC007116","collier double 7x150 iso 10x12 ","METAL-collier","plomberie","U",0.51]
["PMC007118","collier double 7x150 iso 12x14 ","METAL-collier","plomberie","U",0.55000000000000004]
["PMC007120","collier double 7x150 iso 14x16 ","METAL-collier","plomberie","U",0.56999999999999995]
["PMC007122","collier double 7x150 iso 16x18 ","METAL-collier","plomberie","U",0.63]
["PMC007016","collier simple iso 7x150 t 12 ","METAL-collier","plomberie","U",0.3]
["PMC007018","collier simple iso 7x150 t 14 ","METAL-collier","plomberie","U",0.31]
["PMC007020","collier simple iso 7x150 t 16 ","METAL-collier","plomberie","U",0.33]
["PMC007022","collier simple iso 7x150 t 18 ","METAL-collier","plomberie","U",0.34]
["PMC007026","collier simple iso 7x150 t 22 ","METAL-collier","plomberie","U",0.37]
["PMC007032","collier simple iso 7x150 t 28 ","METAL-collier","plomberie","U",0.46]
["PMC007036","collier simple iso 7x150 t 32 ","METAL-collier","plomberie","U",0.49]
["PMC011130","patte vis bois 7x150 30 ","METAL-collier","plomberie","U",0.06]
["PMC011140","patte vis bois 7x150 40 ","METAL-collier","plomberie","U",7.0000000000000007E-2]
["PMC011150","patte vis bois 7x150 50 ","METAL-collier","plomberie","U",0.1]
["PMC011160","patte vis bois 7x150 60 ","METAL-collier","plomberie","U",0.11]
["PMC011180","patte vis bois 7x150 80 ","METAL-collier","plomberie","U",0.2]
["PMC013145","patte vis métaux 7x150 5x45 ","METAL-collier","plomberie","U",0.15]
["PMC013150","patte vis métaux 7x150 5x50 ","METAL-collier","plomberie","U",0.15]
["PMC013740","patte vis métaux 7x150 6x40 ","METAL-collier","plomberie","U",0.14000000000000001]
["PMC013750","patte vis métaux 7x150 6x50 ","METAL-collier","plomberie","U",0.18]
["PMC013770","patte vis métaux 7x150 6x70 ","METAL-collier","plomberie","U",0.2]
["PMC008809","rosace écartement super 9 ","METAL-collier","plomberie","U",7.0000000000000007E-2]
["PMC008814","rosace écartement super 14 ","METAL-collier","plomberie","U",0.08]
["PMC008819","rosace écartement super 19 ","METAL-collier","plomberie","U",0.18]
["PMC008824","rosace écartement super 24 ","METAL-collier","plomberie","U",0.21]
["PMC008125","rosace plate super 25 ","METAL-collier","plomberie","U",0.05]
["SFR122002","jts cnk bleu 12/17 ","JOINT","plomberie","U",0.26]
["SFR122003","jts cnk bleu 15/21 ","JOINT","plomberie","U",0.3]
["SFR122005","jts cnk bleu 20/27 ","JOINT","plomberie","U",0.53]
["WAV3025631","tuyau PVC 125 au ml","PVC 125","plomberie","U",10.48]
["NCLKX","coulisse F/F d.125 ","PVC 125","plomberie","U",9.0500000000000007]
["NCLM2X","manchon à butée F/F d.125 ","PVC 125","plomberie","U",5.22]
["NCLFX","tampon de visite avec bouchon M/F d.125 ","PVC 125","plomberie","U",19.16]
["NCLBX14","culotte simple M/F 45' d.125 ","PVC 125","plomberie","U",17.350000000000001]
["NCLBX144","culotte simple F/F 45' d.125 ","PVC 125","plomberie","U",20.89]
["NCLBX188","culotte simple F/F 87'30 d.125 ","PVC 125","plomberie","U",20.89]
["NCLCX4","coude simple M/F 45' d.125 ","PVC 125","plomberie","U",11.96]
["NCLCX44","coude simple F/F 45' d.125 ","PVC 125","plomberie","U",13.01]
["NCLCX88","coude simple F/F 87'30 d.125 ","PVC 125","plomberie","U",14]
["NCLCOX","collier à bride à d.125 gris ","PVC 125","plomberie","U",6.15]
["WAV3025634","tuyau PVC 100 au ml","PVC 100","plomberie","U",4.8600000000000003]
["NCLST1","secteur de coude F/F 15' d.100 ","PVC 100","plomberie","U",7.39]
["NCLCT2","coude simple M/F 20' d.100 ","PVC 100","plomberie","U",8.6999999999999993]
["NCLCT22","coude simple F/F 20' d.100 ","PVC 100","plomberie","U",10.74]
["NCLCT3","coude simple M/F 30' d.100 ","PVC 100","plomberie","U",18.34]
["NCLCT33","coude simple F/F 30' d.100 ","PVC 100","plomberie","U",20.75]
["NCLST3","secteur de coude M/F 30' d.100 ","PVC 100","plomberie","U",7.79]
["NCLCT4","coude simple M/F 45' d.100 ","PVC 100","plomberie","U",7.07]
["NCLCT44","coude simple F/F 45' d.100 ","PVC 100","plomberie","U",8.52]
["NCLBT14","culotte simple M/F 45' d.100 ","PVC 100","plomberie","U",10.28]
["NCLBT144","culotte simple F/F 45' D.100 ","PVC 100","plomberie","U",12.4]
["NCLBT64","embranchement simple M/F 45' D.100/50","PVC 100","plomberie","U",21.38]
["NCLBT644","embranchement simple F/F 45' D.100/50","PVC 100","plomberie","U",24.32]
["NCLCT6","coude simple M/F 67'30 d.100 ","PVC 100","plomberie","U",7.7]
["NCLCT66","coude simple F/F 67'30 d.100 ","PVC 100","plomberie","U",9.5299999999999994]
["NCLCT8","coude simple M/F 87'30 d.100 ","PVC 100","plomberie","U",8.16]
["NCLCT88","coude simple F/F 87'30 d.100 ","PVC 100","plomberie","U",8.9600000000000009]
["NCLBT18","culotte simple M/F 87'30 d.100 ","PVC 100","plomberie","U",10.28]
["NCLBT188","culotte simple F/F 87'30 d.100 ","PVC 100","plomberie","U",12.27]
["NCLAT188","culotte équerre F/F 87'30 d.100 ","PVC 100","plomberie","U",64.2]
["NCLSL104","selle de branchement M/F 90' d.100/40 ","PVC 100","plomberie","U",8.09]
["NCLSL105","selle de branchement M/F 90' d.100/50 ","PVC 100","plomberie","U",8.19]
["NCLM2T","manchon à butée F/F d.100 ","PVC 100","plomberie","U",3.43]
["NCLCOT","collier à bride  d.100 gris ","PVC 100","plomberie","U",4.8899999999999997]
["NCLKT","coulisse F/F d.100 ","PVC 100","plomberie","U",6.53]
["NCLRT14","culotte double M/F 45' d.100 ","PVC 100","plomberie","U",41.11]
["NCLBT16","culotte simple M/F 67'30 D.100","PVC 100","plomberie","U",11.37]
["NCLBT166","culotte simple F/F 67'30 D.100","PVC 100","plomberie","U",15.47]
["WAV3025624","tuyau PVC 80 au ml","PVC 80","plomberie","U",6.15]
["NCLM2R","manchon à butée F/F d.80 ","PVC 80","plomberie","U",2.76]
["NCLKR","coulisse F/F d.80 ","PVC 80","plomberie","U",5.33]
["NCLCR4","coude simple M/F 45' d.80 ","PVC 80","plomberie","U",4.21]
["NCLCR44","coude simple F/F 45' d.80 ","PVC 80","plomberie","U",6.27]
["NCLCR8","coude simple M/F 87'30 d.80 ","PVC 80","plomberie","U",5.3]
["NCLCR88","coude simple F/F 87'30 d.80 ","PVC 80","plomberie","U",6.32]
["NCLBR14","culotte simple M/F 45' d.80 ","PVC 80","plomberie","U",8.64]
["NCLBR144","culotte simple F/F 45' d.80 ","PVC 80","plomberie","U",10.38]
["NCLBR18","culotte simple M/F 87'30 d.80 ","PVC 80","plomberie","U",9.4499999999999993]
["NCLBR188","culotte simple F/F 87'30 d.80 ","PVC 80","plomberie","U",10.38]
["NCLFR","tampon de visite avec bouchon M/F D.80","PVC 80","plomberie","U",14.59]
["NCLCOR","collier à bride  d.80 gris ","PVC 80","plomberie","U",3.77]
["WAV3025620","tuyau PVC 75 au ml","PVC 75","plomberie","U",5.95]
["NCLM2P","manchon a butée F/F d.75 ","PVC 75","plomberie","U",4.29]
["NCLCP4","coude simple M/F 45' d.75 ","PVC 75","plomberie","U",7.63]
["NCLCP44","coude simple F/F 45' D.75","PVC 75","plomberie","U",3.64]
["NCLBP18","culotte simple M/F 87'30 d.75 ","PVC 75","plomberie","U",16.350000000000001]
["NCLBP188","culotte simple F/F 87'30 d.75 ","PVC 75","plomberie","U",16.89]
["NCLCOP","collier a bride d.75 gris ","PVC 75","plomberie","U",3.64]
["WAV3025621","tuyau PVC 63 au ml","PVC 63","plomberie","U",5.26]
["NCLCL2","coude M/F 20°  Ø63","PVC 63","plomberie","U",6.62]
["NCLCL22","coude F/F 20°  Ø63","PVC 63","plomberie","U",8.16]
["NCLCL4","coude simple M/F 45' d.63 ","PVC 63","plomberie","U",7.29]
["NCLCL44","coude simple F/F 45' d.63 ","PVC 63","plomberie","U",7.63]
["NCLCL8","coude simple M/F 87'30 d.63 ","PVC 63","plomberie","U",6.81]
["NCLCL88","coude simple F/F 87'30 d.63 ","PVC 63","plomberie","U",7.69]
["NCLBL18","culotte simple M/F 87'30 d.63 ","PVC 63","plomberie","U",15.87]
["NCLBL188","culotte simple F/F 87'30 d.63 ","PVC 63","plomberie","U",16.170000000000002]
["NCLM2L","manchon a butée F/F d.63 ","PVC 63","plomberie","U",4.53]
["NCLFL","tampon de visite avec bouchon M/F d.63 ","PVC 63","plomberie","U",12.95]
["NCLCOL","collier à bride  d.63 gris ","PVC 63","plomberie","U",3.42]
["WAV3025625","tuyau PVC 50 au ml","PVC 50","plomberie","U",4.3600000000000003]
["NCLCJ4","coude simple M/F 45' d.50 ","PVC 50","plomberie","U",2.93]
["NCLCJ44","coude simple F/F 45' d.50 ","PVC 50","plomberie","U",2.93]
["NCLCJ6","coude simple M/F 67'30 D.50","PVC 50","plomberie","U",5.7]
["NCLCJ66","coude simple F/F 67'30 D.50","PVC 50","plomberie","U",5.7]
["NCLCJ8","coude simple M/F 87'30 d.50 ","PVC 50","plomberie","U",3.49]
["NCLCJ88","coude simple F/F 87'30 d.50 ","PVC 50","plomberie","U",3.49]
["NCLTJ18","té pied de biche M/F 87'30 d.50 ","PVC 50","plomberie","U",11.64]
["NCLTJ188","té pied de biche F/F 87'30 d.50 ","PVC 50","plomberie","U",7.33]
["NCLBJ14","culotte simple M/F 45' d.50 ","PVC 50","plomberie","U",8.07]
["NCLBJ144","culotte simple F/F 45' d.50 ","PVC 50","plomberie","U",5.65]
["NCLM2J","manchon a butée F/F d.50 ","PVC 50","plomberie","U",1.34]
["NCLFLEXJ","manchette souple pour renovation F/F d.50 ","PVC 50","plomberie","U",15.76]
["NCLFJ","tampon de visite avec bouchon M/F d.50","PVC 50","plomberie","U",1.89]
["NCLCO50","collier monobloc insert p.7/150 d.50 gris ","PVC 50","plomberie","U",1.65]
["NCLE50F","embout filete fem d.50 ","PVC 50","plomberie","U",9.8800000000000008]
["NCLN50F","union 3 pieces a coller press. d.50 ","PVC 50","plomberie","U",21.89]
["NCLGOTS","grille pour hotte de cuisine sable ","HOTTE","plomberie","U",26.35]
["NCLGOTB","grille pour hotte de cuisine blanche ","HOTTE","plomberie","U",37.450000000000003]
["GF26302439","T-88 COLLE PVC LIQUIDE","COLLE","plomberie","U",12.5]
["VRX262600","FILETFIX III 2626","COLLE","plomberie","U",41.33]
["CMP4337","coude F 16-15/21 ","PER 16","plomberie","U",5.63]
["CMP4294","coude fixeF 16-15/21 ","PER 16","plomberie","U",14.26]
["CMPB621001001","gaine bleue PER16 ","PER 16","plomberie","U",1.66]
["CMPB622001002","gaine rouge PER16","PER 16","plomberie","U",1.66]
["CMP4288","applique F16-15/21 ","PER 16","plomberie","U",7.99]
["CMP4291","applique longue F 16-15/21 ","PER 16","plomberie","U",9.23]
["CMP4262","raccord F 16-12/17 ","PER 16","plomberie","U",3.71]
["CMP4263","raccord F 16-15/21","PER 16","plomberie","U",2.89]
["CMP4271","mamelon M à visser 12/17-16X1,5 ","PER 16","plomberie","U",3.29]
["CMP4282","raccord F fixe 16-15/21","PER 16","plomberie","U",4.43]
["CMP4297","té égal 16 ","PER 16","plomberie","U",8.7799999999999994]
["CMP4331","coude égal à 90° 16","PER 16","plomberie","U",6.51]
["CMP4322","manchon egal 16x1.5 ","PER 16","plomberie","U",4.41]
["CMP4342","coude M 16-15/21 ","PER 16","plomberie","U",7.99]
["CMP4272","mamelon droit a visser M 15/21-16 ","PER 16","plomberie","U",3.78]
["CMP4346","té M vis 15/21-16","PER 16","plomberie","U",10.37]
["CMP4301","té réduit 12-12-16 ","REDUC PER","plomberie","U",11.24]
["CMP4302","té réduit 12-16-16","REDUC PER","plomberie","U",12.38]
["CMP4303","té réduit 16-12-16 ","REDUC PER","plomberie","U",9.4]
["CMP4325","manchon réduit 12-16 ","REDUC PER","plomberie","U",5.38]
["CMP4287","applique F pour PER12 ","PER 12","plomberie","U",8.42]
["CMP4290","applique longue F pour PER12  ","PER 12","plomberie","U",9.3800000000000008]
["CMP2457","robinet machine à laver à clapet ","PER 12","plomberie","U",9.3800000000000008]
["CMP3013","robinet machine à laver 1/4 de tour","PER 12","plomberie","U",14.67]
["CMP4269","sortie PER12 vers vis M 12/17","PER 12","plomberie","U",3]
["CMP4270","sortie PER12 vers vis M 15/21","PER 12","plomberie","U",2.94]
["CMP4280","sortie PER12 vers vis F 15/21","PER 12","plomberie","U",4.07]
["CMP4260","sortie PER12 vers écrou  12/17","PER 12","plomberie","U",2.87]
["CMP4261","sortie PER12 vers écrou  15/21","PER 12","plomberie","U",2.87]
["CMP4296","té égal 12","PER 12","plomberie","U",9.5399999999999991]
["CMP4349","té F 12-15/21","PER 12","plomberie","U",7.87]
["CMP4293","coude F 12-15/21","PER 12","plomberie","U",13.88]
["CMP4321","manchon droit 12","PER 12","plomberie","U",4.59]
["CMP4330","coude égal à 90°12 x 12 ","PER 12","plomberie","U",7.63]
["CMP4335","coude F 1/2-12","PER 12","plomberie","U",6.75]
["CMP4340","coude M 12/17-12 ","PER 12","plomberie","U",6.72]
["CMP4341","coude M 15/21-12","PER 12","plomberie","U",6.97]
["CMPB621004001","gaine bleue PER12","PER 12","plomberie","U",1.25]
["CMPB622004001","gaine rouge PER12 ","PER 12","plomberie","U",1.25]
["CMP4330","coude égal PER 12","PER 12","plomberie","U",7.63]
["CMP4334","coude PER12 vers 12/17 F","PER 12","plomberie","U",6.8]
["CMP4335","coude PER12 vers 15/21 F","PER 12","plomberie","U",6.75]
["CMP4340","coude PER12 vers 12/17M","PER 12","plomberie","U",6.72]
["CMP4341","coude PER12 vers 15/21M","PER 12","plomberie","U",6.97]
["CMPB621004001","PER rouge Ø 12 eau chaude au ml ","PER 12","plomberie","U",1.25]
["CMPB622004001","PER bleu Ø 12 eau froide au ml ","PER 12","plomberie","U",1.25]