{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Feuil1","Feuil2","Feuil4"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":14,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Feuil1","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[[10,4,11,5],[10,1,11,3],[21,4,22,5],[21,6,22,7],[10,6,11,7],[21,1,22,3],[0,1,0,5],[0,6,0,7]]}
[null,"Parois Exterieurs",null,null,null,null,"+",null,"<== bouton ajout paroi\npar Double clic"]
[null,"Choix du mur","Type de mur","Resistance Thermique","Epaisseur","Type isolant","Conductivite L","Resistance R","Epaisseur isolant"]
[]
[null,"véranda",2,21,32,43,54,64,73]
[null,"Choix du mur",5,23,34,43,55,66,74]
[null,"Ext",3,22,34,43,54,64,75]
[null,"véranda",5,25,36,44,54,65,71]
[null,"garage",4,22,33,44,53,63,74]
[]
[]
[null,"MURS INTERIEURS",null,null,"+",null,"<== bouton ajout paroi\npar Double clic"]
[]
[null,"Choix de la paroi","type de paroi","Marque","Epaisseur"]
[]
[null,"cloison","…","…",12]
[null,"cloison","brique","marque","Epaisseur"]
[null,"cloison","brique","…",12]
[null,"cloison","Type","marque",16]
[null,"Choix","brique","…",16]
[null,"cloison","brique","…",12]
[]
[null,"PLANCHERS BAS",null,null,"+",null,"<== bouton ajout paroi\npar Double clic"]
[]
[null,"Choix plancher","type de plancher","Marque","Epaisseur","Résistance thermique","Epaisseur","Type d'isolant","Conductivité L"]

{"sheet":"Feuil2","index":1,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["Choix du mur","Type de mur","Resistance Thermique","Epaisseur","Type isolant","Conductivite L","Resistance R","Epaisseur isolant"]
["Ext",1,20,30,40,50,60,70]
["garage",2,21,31,41,51,61,71]
["véranda",3,22,32,42,52,62,72]
[null,4,23,33,43,53,63,73]
[null,5,24,34,44,54,64,74]
[null,6,25,35,45,55,65,75]
[null,7,26,36,46,56,66,76]
[null,8,27,37,47,57,67,77]
[null,9,28,38,48,58,68,78]
[null,10,29,39,49,59,69,79]
[]
["Choix","Type","marque","Epaisseur"]
["cloison","brique","…",12]
["…","…","…",16]

{"sheet":"Feuil4","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}