{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Feuil1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Feuil1","index":0,"n_rows":651,"n_cols":16,"rows_kept":651,"cut":false,"hidden":false,"merged":[[57,23,57,24],[55,23,55,24],[56,23,56,24],[0,0,0,14]]}
["Choix du critère de filtrage"]
["ISO","DIN","Graisse","Huile","Densité \nKG/m3","T\nmini","T°\nd'écoulement","T°\nd'éclair","T\nmaxi","NLGI","Base","Viscosité\n40°Cmm²/s","Viscosité\n100°Cmm²/s","Nom","Fournisseur"]
[]
[]
[]
["ISO","DIN","Graisse","Huile","Densité \nKG/m3","T\nmini","T°\nd'écoulement","T°\nd'éclair","T\nmaxi","NLGI","Base","Viscosité\n40°Cmm²/s","Viscosité\n100°Cmm²/s","Nom","Fournisseur","Documentation"]
["ISOVG???","K0K-20",null,null,null,-20,null,null,120,"0","Lithium/Lithium complex",null,null,"FlieRfett AN0","ARAL","http://www.lubebase.com/"]
["ISOVG???","K0K-20",null,null,null,-20,170,null,120,0,"Lithium/Lithium complex",null,null,"G.A.No.850EP","BRUGAROLAS","DOCGRAISSE\\brugarolas\\brugarolas.pdf"]
["ISOVG???","K2K-20",null,null,0.9,-25,300,200,140,2,"Lithium",null,null,"G.A.No.80","BRUGAROLAS","DOCGRAISSE\\brugarolas\\brugarolas.pdf"]
["ISOVG???","K2R-40",null,null,0.9,-40,null,218,180,2,null,null,null,"Renolit ST-V2","FUCHSEUROPE","http://www.lubebase.com/"]
["ISOVG???","K3K-20",null,null,null,-20,null,null,120,3,"Lithium",null,null,"G.A.No.95","BRUGAROLAS","cataloguebrugarolas.pdf"]
["ISOVG???","KP1K-20",null,null,null,-20,null,null,null,1,null,null,null,"LTX 1","BP"]
["ISOVG???","KP2K-30",null,null,null,-30,null,null,null,2,null,null,null,"Olex PR9142","BP "]
["ISOVG???","KP2K-30",null,null,null,-30,null,null,null,2,null,null,null,"Aralub FK 2","ARAL "]
["ISOVG???","KP2N-20",null,null,null,-20,245,null,150,2,"Lithium complex",null,null,"G.A.Plex 2","BRUGAROLAS","DOCGRAISSE\\brugarolas\\GRASAS.pdf"]
["ISOVG???","KP3K-20",null,null,"920à15°C",-20,null,200,120,3,"Minérale",null,null,"Rolexa 3","ELF","DOCGRAISSE\\ELF\\ELFROLEXA3.(12.02.2008).pdf"]
["ISOVG???",null,null,null,"0,94g/cm3 à 20°C",-10,null,null,150,null,"Minérale",null,null,"Polylub HVT 50 A","KLÜBER","DOCGRAISSE\\Klüber\\Polylub_HVT_50_A_Spray.pdf"]
["ISOVG???",null,null,null,"0,910 g/cm3 à 25°C",-30,null,100,150,"3","LITHIUM COMPLEX","57,9","81","MOLYKOTE G-1001","DOW CORNING"]
["ISOVG???",null,null,null,"1 à 25°C",-50,null,200,130,null,"LITHIUM CALCIUM",null,null,"MOLYKOTE G-2001","DOW CORNING","DOC GRAISSE\\DOW CORNING\\G-2001 MSDS.pdf"]
["ISOVG???",null,null,null,"0,83 à 25°C",-51,null,260,163,"1","ALUMINIUM COMPLEX / PTFE",null,null,"MOLYKOTE G-4501","DOW CORNING","DOC GRAISSE\\DOW CORNING\\TDS_MOLYKOTEG_4501_ger.pdf"]
["ISOVG???",null,null,null,"0,87 à 25°C",-40,null,230,177,"2","LITHIUM COMPLEX-BISULFURE DE MOLYBDENE",null,null,"MOLYKOTE G-4700","DOW CORNING"]
["ISOVG???",null,null,null,"1,01 g/cm3 à 25°C",-45,null,null,182,null,"LITHIUM COMPLEX","55",null,"MOLYKOTE BG-20","DOW CORNING","DOC GRAISSE\\DOW CORNING\\BG20.pdf"]
["ISOVG???",null,null,null,"1,01 g/cm3 à 25°C",-40,null,195,150,null,"LITHIUM","26",null,"MOLYKOTE BG-555","DOW CORNING","DOC GRAISSE\\DOW CORNING\\BG-555 TDS.pdf"]
["ISOVG???",null,null,null,"1,28 à 25°C",-40,null,101.1,204,"1","POLYUREA",null,null,"MOLYKOTE 1292","DOW CORNING"]
["ISOVG???",null,null,null,"1,1 à 25°C",-65,null,101,177,"1","LITHIUM",null,null,"MOLYKOTE 55","DOW CORNING","DOC GRAISSE\\DOW CORNING\\MSDS_MOLYKOTE_55_O_Ring_eng.pdf"]
["ISOVG100","DIN 51 524",null,null,"880 à 15°C",null,-30,245,null,0,"Minérale",68,8.6999999999999993,"Hyspin DSP ","CASTROL","DOC HUILE\\CASTROL\\Hyspin SP.pdf"]
["ISOVG100","DIN 51517-3",null,null,"1050  à 15°C",null,-42,280,null,0,"Synthétique",100,20,"Tribol 800","CASTROL","DOC HUILE\\CASTROL\\Tribol 800 .pdf"]
["ISOVG100","DIN 51517-3",null,null,null,-30,-45,250,150,0,"Synthétique",100,null,"Gearmaster SYN","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG100","GE00K-30",null,null,"1000 à 20°C ",-35,null,200,120,"00-000","LITHIUM CALCIUM","90",null,"ARALUB BAB EP 00/000","ARAL","DOC GRAISSE\\ARAL\\aralub\\217100Aral Aralub BAB EP 00_000.pdf"]
["ISOVG100","GL3-30",null,null,"900à15°C",-30,190,null,120,3,"Lithium",100,10.199999999999999,"Alvania RL3","SHELL","DOCGRAISSE\\schell\\AlvaniaRL.pdf"]
["ISOVG100","GLP00K-30",null,null,null,-30,null,null,120,"00","LITHIUM COMPLEX","95",null,"ARALUB HLP 00","ARAL"]
["ISOVG100","GP00K-30",null,null,null,-20,null,null,120,"00","Lithium/Lithiumcomplex",105,null,"Aralub MFL00","ARAL","DOCGRAISSE\\ARAL\\AralubMFL00.pdf"]
["ISOVG100","K0D-20",null,null,null,-20,null,null,70,0,"Végétale",68,null,"Beslux Hidro-Bio ","BRUGAROLAS","DOC HUILE\\BRUGAROLAS\\lubricantes-brugarolas_aceites_industriales.pdf"]
["ISOVG100","K0G-15",null,null,null,-15,null,null,100,0,"Minérale",100,null,"Eco Gear M","BECHEM"]
["ISOVG100","K0G-40",null,null,null,-40,null,null,100,0,"Synthétique",100,null,"Eco Gear S","BECHEM"]
["ISOVG100","K0H-0",null,null,"0,89g/cm3 à 15°C",0,-10,235,110,0,"Minérale",150,null,"Beslux Camin","BRUGAROLAS","DOC HUILE\\BRUGAROLAS\\lubricantes-brugarolas_aceites_industriales.pdf"]
["ISOVG100","K0H-15",null,null,"0,88 à 15°C",-15,-21,250,110,0,"Minérale",100,10.8,"Staroil No. 100","BECHEM","DOC HUILE\\BECHEM\\Staroil No. 100.pdf"]
["ISOVG100","K0K-10",null,null,"0,89 g/cm3 à 20°C",-10,null,250,120,0,"Minérale",150,null,"Structovis FHD","KLÜBER","DOC HUILE\\KLUBER\\STRUCTOVIS_FHD-sp.pdf"]
["ISOVG100","K0K-15",null,null,null,-15,-24,231,120,0,"Minérale",100,null,"Gearmaster CLP","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG100","K0K-20",null,null,"0,89g/cm3 à 15°C",-20,-21,210,120,0,"Minérale",100,null,"Fluid Drive HM","BRUGAROLAS","DOC HUILE\\BRUGAROLAS\\lubricantes-brugarolas_aceites_industriales.pdf"]
["ISOVG100","K0N-15",null,null,null,-15,-19,290,150,0,"Minérale",215,null,"Stabylan 2001","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG100","K0N-30",null,null,"925 à 15°C",-30,-35,230,140,0,"Végétale",100,16.2,"Tribol Bio Top 1428","CASTROL","DOC HUILE\\CASTROL\\Tribol Bio Top 1428.pdf"]
["ISOVG100","K0N-30",null,null,null,-30,-39,220,150,0,"Synthétique",100,null,"Gearmaster PGP ","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG100","K0N-35",null,null,"0,84 g/cm3 à 20°C",-35,-40,240,135,0,"Minérale",95,12.7,"Klüber Summit HySyn FG-100","KLÜBER","DOC HUILE\\KLUBER\\Klüber Summit HySyn FG-100.pdf"]
["ISOVG100","K0P-20",null,null,null,-20,null,null,160,0,"Minérale",100,null,"Berulit IKP","BECHEM"]
["ISOVG100","K0P-40",null,null,null,-40,null,null,160,0,"Synthétique",81,null,"Stabylan ECO 20","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG100","K0U-0",null,null,"0,96 g/cm3 à 20°c",0,-30,270,250,0,"Synthétique",90,12,"Klübersynth CH2 - 100","KLÜBER","DOC HUILE\\KLUBER\\Klubersynth_CH_2_100.pdf"]
["ISOVG100","K0U-10",null,null,null,-10,-30,260,240,0,"Synthétique",100,null,"Stabylan 5000","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG100","K0U-20",null,null,"0,969g/cm3 à 15°C",-20,-22,245,240,0,"Synthétique",100,null,"Beslux Ramca ","BRUGAROLAS","DOC HUILE\\BRUGAROLAS\\lubricantes-brugarolas_aceites_industriales.pdf"]
["ISOVG100","K2K-20",null,null,null,-20,null,-21,120,2,"Lithium",110,null,"Renolit FWA","FUCHSEUROPE","DOCGRAISSE\\FUCHSEUROPE\\RenolitFWA.pdf"]
["ISOVG100","K2K-20",null,null,"0,9à20°C",-20,null,200,120,2,"Lithium",110,10,"Centoplex","KLÜBER","DOCGRAISSE\\Klüber\\CENTOPLEX_2_3-en.pdf"]
["ISOVG100","K2K-20",null,null,"0,9g/cm3à15°C",-20,null,200,130,2,"Lithium",100,11,"Alvania G","SHELL","DOCGRAISSE\\schell\\AlvaniaG2+3.pdf"]
["ISOVG100","K2K-30",null,null,"900à15°C",-30,180,200,120,2,"Minérale",100,10.199999999999999,"Alvania RL2","SHELL","DOCGRAISSE\\schell\\SHELL_AlvaniaRL2.pdf"]
["ISOVG100","K2K-30",null,null,"0,95à20°C",-30,185,180,120,2,"Lithium",110,null,"GR MU","AGIP","DOCGRAISSE\\AGIP\\agipgrmu.pdf"]
["ISOVG100","K2K-30",null,null,"0,89g/cm3à20°C",-30,null,41,120,2,"Lithium",100,9,"High-LubL","BECHEM","DOCGRAISSE\\bechem\\bechem_high-lub_l_2_ep_2.PDF"]
["ISOVG100","K2N-20",null,null,"0,93à15°C",-30,230,null,190,2,"Savon de lithium",115,12.2,"Unirex N2","ESSO","DOCGRAISSE\\Esso\\unirexn2.pdf"]
["ISOVG100","K2N-20",null,null,"0,99g/cm3à20°C",-20,220,200,140,2,"Minérale",95,12,"Staburags NBU 8EP","KLÜBER","DOCGRAISSE\\Klüber\\StaburagsNBU8EP.pdf"]
["ISOVG100","K2P-20",null,null,null,-20,260,null,170,2,"huile",115,12.2,"Polyrex EM","ESSO","DOCGRAISSE\\Esso\\mobil_polyrex_em.pdf"]
["ISOVG100","K2P-20",null,null,"0,884 à 15°C",-20,null,204,160,"2","POLYUREA","113",null,"MOBIL POLYREX EM","MOBIL","DOC GRAISSE\\Mobil\\MSDS Mobil polyrex EM.pdf"]
["ISOVG100","K2P-40",null,null,null,-40,null,null,260,"2/1","calcium",100,12.3,"RENOLIT CX-TOM15","FUCHS","DOCGRAISSE\\fuchs\\NB-RenolitCX-TOM–Produ-Sve–P1819–j4.pdf"]
["ISOVG100","K3K-20",null,null,"920à20°C",-20,null,200,140,"3","Lithium",105,null,"Aralub HL","ARAL","DOCGRAISSE\\ARAL\\ArialaralubHL3.docx"]
["ISOVG100","K3K-20",null,null,null,-20,null,null,120,3,"Lithium",100,9,"High-LubL","BECHEM","DOCGRAISSE\\bechem\\bechem_high-lub_l_2_ep_2.PDF"]
["ISOVG100","K3K-20",null,null,"0,9 g/cm3 à 15°C",-20,null,210,120,3,"Lithium",100,11,"Alvania G","SHELL","DOCGRAISSE\\schell\\AlvaniaG2+3.pdf"]
["ISOVG100","K3K-20",null,null,null,-20,null,null,120,3,"Lithium",100,11,"Multifak RSP","TEXACO","DOCGRAISSE\\texaco\\MultifakRSP3.pdf"]
["ISOVG100","K3N-20",null,null,"0,92g/cm3à20°C",null,230,200,null,3,"Savon de lithium",113,null,"Unirex N3","ESSO","DOCGRAISSE\\Esso\\unirexn2.pdf"]
["ISOVG100","KP0K-20",null,null,"900 à 15°C",-20,180,180,120,0,"Lithium","111",null,"GR MU EP","AGIP","DOC GRAISSE\\AGIP\\agip gr mu.pdf"]
["ISOVG100","KP0N-30",null,null,null,-30,200,null,140,"0","LITHIUM COMPLEX","100",null,"MOBILGREASE XHP 100 MINE","MOBIL","DOC GRAISSE\\Mobil\\mobilgrease-xhp-mine-series.pdf"]
["ISOVG100","KP1K-20",null,null,"900  à 15 °C",-30,null,140,130,1,"Lithium",100,10.199999999999999,"ALVANIA GREASE R1","SHELL","DOCGRAISSE\\schell\\ALVANA.pdf"]
["ISOVG100","KP1K-20",null,null,"0,93 g/cm³ à  20°C",-20,185,200,120,1,"Lithium",111,null,"GRMU/EPI","AGIP","DOCGRAISSE\\AGIP\\agipgrmuep.pdf"]
["ISOVG100","KP2K-20",null,null,"0,95 g/cm3 à 20°C",-20,185,200,120,2,"Lithium",111,null,"GR MU EP","AGIP","DOCGRAISSE\\AGIP\\agipgrmuep.pdf"]
["ISOVG100","KP2K-20",null,null,null,-20,180,230,120,2,"Lithium",100,10,"Tribal3030/100","CASTROL","DOCGRAISSE\\castrol\\Tribol3030fr.pdf"]
["ISOVG100","KP2K-30",null,null,null,-20,300,200,140,2,"calcium",113,null,"GP Grease","ESSO ","DOCGRAISSE\\Esso\\GPGREASE.pdf"]
["ISOVG100","KP2K-30",null,null,null,-30,185,null,130,2,"Lithium",96,null,"Beacon2","ESSO","DOCGRAISSE\\Esso\\Beacon2.pdf"]
["ISOVG100","KP2K-30",null,null,"1000 à 20°C ",-30,null,200,120,2,"Lithium",100,9,"AralubHLP","ARAL","DOCGRAISSE\\ARAL\\Aralub_HLP_2.pdf"]
["ISOVG100","KP2N-30",null,null,"0,9à15°C",-30,240,null,150,2,"Calcium",100,9.8000000000000007,"TexandoFO20","TEXACO","DOCGRAISSE\\texaco\\TexandoF020.pdf"]
["ISOVG100","KP3K-20",null,null,"900 à 15 °C",-40,190,195,100,3,"Minérale",75,11,"AlvaniaR3","SHELL","DOCGRAISSE\\schell\\AlvaniaRL.pdf"]
["ISOVG100","KP3K-20",null,null,null,-20,null,null,140,3,"lithium",105,null,"AralubHL3","ARAL","DOCGRAISSE\\ARAL\\ArialaralubHL3.docx"]
["ISOVG100","KP3K-20",null,null,"0,9 à 15°C",-30,280,250,145,3,"Minérale",110,9.8000000000000007,"TexandoFO20","TEXACO ","DOCGRAISSE\\texaco\\TexandoF020.pdf"]
["ISOVG100","KP3K-20",null,null,"1000 kg/m³ à 15°C",-25,null,null,130,3,"Lithium",110,null,"Energrease","BP","DOCGRAISSE\\BP\\engrease.pdf"]
["ISOVG100","KP3K-20",null,null,null,-20,null,100,120,3,"Lithium",110,null,"RenolitFWA","FUCHSEUROPE","DOCGRAISSE\\FUCHSEUROPE\\RenolitFWA.pdf"]
["ISOVG100","KP3P-10",null,null,"0,88 à 15°C",-10,null,204,160,"3","POLYUREA","113",null,"MOBIL POLYREX EM 103","MOBIL","DOC GRAISSE\\Mobil\\mobil_polyrex_em_103.pdf"]
["ISOVG100","KPE1K-40",null,null,"0,97 à 15°C",-40,180,232,120,"1","LITHIUM","100",null,"MOBIL SHC GREASE 101 EAL","MOBIL","DOC GRAISSE\\Mobil\\Mobil-SHC-Grease-100-EAL-Series.pdf"]
["ISOVG100","KPE2K-30",null,null,null,-35,null,null,120,"2","LITHIUM CALCIUM","100",null,"ARALUB BAB EP 2","ARAL"]
["ISOVG100","KPE2K-40",null,null,"0,97 à 15°C",-40,180,232,120,"2","LITHIUM","100",null,"MOBIL SHC GREASE 102 EAL","MOBIL","DOC GRAISSE\\Mobil\\Mobil-SHC-Grease-100-EAL-Series.pdf"]
["ISOVG100","KPF1K-20",null,null,"0,9 à 15°C",-20,null,216,120,"1","ALUMINIUM COMPLEX","100","13","MOBILGREASE FM 101","MOBIL","http://www.mobil.com/Australia-English/Lubes/PDS/GLXXENGRSMOMobilgrease_FM_101_FM_222.aspx"]
["ISOVG100","KPHC2N-40",null,null,"1 à 15°C",-40,265,204,150,"2","LITHIUM COMPLEX","100","14,5","MOBILITH SHC 100","MOBIL","DOC GRAISSE\\Mobil\\MOBILITH SHC serie.pdf"]
["ISOVG100",null,null,null,"0,850 à 15°C",null,-33,230,null,0,"Synthétique",100,11.8,"Blasia SX 100","AGIP","DOC HUILE\\AGIP\\BLASIA-SX-100-220-320.pdf"]
["ISOVG100",null,null,null,null,null,-27,280,null,0,"Minérale",60,14,"Deganit BA","ARAL","http://www.lubebase.com/"]
["ISOVG100",null,null,null,"0,85 à 15°C",null,-22,220,null,0,"Minérale",100,14.4,"Basic Tronic SAE10W-40","ARAL","DOC HUILE\\ARAL\\Basic Tronic SAE10W-40.pdf"]
["ISOVG100",null,null,null,"886 à 15 °C",null,-27,212,null,0,"Minérale",100,11,"Deganit B","ARAL","http://www.lubebase.com/"]
["ISOVG100",null,null,null,"883 à 15°C",null,-18,246,null,0,"Minérale",100,12,"Degol BG","ARAL","DOC HUILE\\ARAL\\DEGOL.pdf"]
["ISOVG100",null,null,null,"888 à 15°C",null,-24,225,null,0,"Minérale",100,18.8,"Degol BG Plus","ARAL","DOC HUILE\\ARAL\\Degol BG 220 Plus.pdf"]
["ISOVG100",null,null,null,"887 à15°C",null,-18,272,null,0,"Minérale",100,8.6,"Vitam GF ","ARAL","DOC HUILE\\ARAL\\Vitam_GF_46.pdf"]
["ISOVG100",null,null,null,"0,89 à 15°C",null,-21,220,null,0,"Minérale",100,11.1,"Energol GR-XP","BP","DOC HUILE\\BP\\ENERGOL GR-XP.pdf"]
["ISOVG100",null,null,null,"0,89 à 15°C",null,-21,226,null,0,"Minérale",105,12.1,"Energol HLP-HM ","BP","DOC HUILE\\BP\\Energol HLP-HM.pdf"]
["ISOVG100",null,null,null,"0,89 g/cm3 à 15°C",null,21,215,null,0,"Minérale",100,11.1,"Alpha SP","CASTROL","DOC HUILE\\CASTROL\\Alpha SP.pdf"]
["ISOVG100",null,null,null,"904 à 15°C",null,-24,170,null,0,"Minérale",100,12.1,"Tribol 1730/100","CASTROL","DOC HUILE\\CASTROL\\Tribol 1730_100.pdf"]
["ISOVG100",null,null,null,"892 à 15°C",null,-30,240,null,0,"Minérale",100,11.2,"Tribol 1100","CASTROL","DOC HUILE\\CASTROL\\Tribol 1100.pdf"]
["ISOVG100",null,null,null,"880 à 15°C",null,-27,230,null,0,"Minérale",100,11.5,"Spartan EP series","ESSO","DOC HUILE\\ESSO\\Spartan EP series.pdf"]
["ISOVG100",null,null,null,"924 à 15°C",null,-36,300,null,0,"Synthétique",100,null,"Plantotac HV 100 N","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\238_Planto Brochure.pdf"]
["ISOVG100",null,null,null,"845 à 15°C",null,-54,250,null,0,"Synthétique",100,14.4,"Renolin Unisyn CLP series","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\RENOLIN_UNISYN_CLP.pdf"]
["ISOVG100",null,null,null,"881 à 15°C",null,-21,230,null,0,"Minérale",100,11.3,"Renotac 343","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\Renotac 343.pdf"]
["ISOVG100",null,null,null,"878 à 15°C",null,-18,232,null,0,"Minérale",100,11.1,"Renolin B ","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\RENOLIN_B.pdf"]
["ISOVG100",null,null,null,"890 à 15°C",null,-24,240,null,0,"Minérale",100,11.2,"Renolin CLP ","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\Renolin CLP.pdf"]
["ISOVG100",null,null,null,"883 à 15°C",null,-18,248,null,0,"Minérale",100,11.4,"Renolin MR 30","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\RENOLIN_MR.pdf"]
["ISOVG100",null,null,null,"1043 à 15°C",null,-48,260,null,0,"Synthétique",100,19.600000000000001,"Renolin PG","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\RENOLIN_PG.pdf"]
["ISOVG100",null,null,null,"1,04 g/cm3 à 20°C",null,-40,200,null,0,"Synthétique",100,19.5,"Syntheso D EP","KLÜBER","DOC HUILE\\KLUBER\\Syntheso D EP.pdf"]
["ISOVG100",null,null,null,null,null,-21,236,null,0,"Minérale",71.2,8.5299999999999994,"Mobil DTE 20 series","MOBIL","DOC HUILE\\MOBIL\\Mobil DTE 20 series.pdf"]
["ISOVG100",null,null,null,"0,86 g/cm3 à 15°C",null,-42,248,null,0,"Minérale",99.1,13.9,"Mobil SHC 600 series","MOBIL","DOC HUILE\\MOBIL\\Mobil_SHC_600.pdf"]
["ISOVG100",null,null,null,"0,89 g/cm3 à 15,6°C",null,-30,250,null,0,"Minérale",100,11.1,"Mobilgear XMP series","MOBIL","DOC HUILE\\MOBIL\\mobilgear_xmp_series.pdf"]
["ISOVG100",null,null,null,"0,884 à 15°C",null,-15,242,null,0,"Minérale",100,11.1,"Nuto H series","MOBIL","DOC HUILE\\MOBIL\\Nuto.pdf"]
["ISOVG100",null,null,null,"882,6 à 20°C",null,-24,195,null,0,"Minérale",100,11.4,"Shell Omala","SHELL","DOC HUILE\\SHELL\\Shell Omala.pdf"]
["ISOVG100",null,null,null,"0,891 à 15°C",null,-24,234,null,0,"Minérale",100,11.1,"Tellus","SHELL","DOC HUILE\\SHELL\\Tellus.pdf"]
["ISOVG100",null,null,null,"883 à 15°C",null,-21,228,null,0,"Minérale",68,8.9,"Tellus DO","SHELL","DOC HUILE\\SHELL\\Tellus DO(TDS).pdf"]
["ISOVG100",null,null,null,"0,9 à 20 °C",null,null,200,null,0,"Synthétique",null,null,"Talcor CBR Fluid","TEXACO","DOC HUILE\\TEXACO\\Talcor_CBR_Fluid-MSDS (1).pdf"]
["ISOVG100",null,null,null,"0,886 à 15°c",null,-27,220,null,0,"Minérale",46,6.5,"Alcor DD ","TEXACO","http://www.lubebase.com/"]
["ISOVG100",null,null,null,"0,91 à 15°C",null,-30,225,null,0,"Minérale",100,11.4,"Meropa","TEXACO","DOC HUILE\\TEXACO\\Meropa 100.pdf"]
["ISOVG100",null,null,null,"0,887 à 15°C",null,-27,240,null,0,"Minérale",100,11.2,"Meropa WM ","TEXACO","DOC HUILE\\TEXACO\\Meropa WM  220.pdf"]
["ISOVG100",null,null,null,null,null,-15,250,null,0,"Minérale",95,11,"Rando HD","TEXACO","DOC HUILE\\TEXACO\\Rando HD.pdf"]
["ISOVG100",null,null,null,null,null,null,200,null,0,"Synthétique",100,null,"Talcor Chain Lube NF","TEXACO","DOC HUILE\\TEXACO\\Talcor Chain Lube NF.pdf"]
["ISOVG100",null,null,null,"888 à 15°C",null,-18,254,null,0,"Minérale",97.5,11.2,"Azolla ZS","TOTAL ","DOC HUILE\\TOTAL\\AZOLLA_ZS.pdf"]
["ISOVG100",null,null,null,"0,88 à 15°C",null,-21,233,null,0,"Minérale",107,11.8,"Carter EP","TOTAL ","DOC HUILE\\TOTAL\\CARTER EP.pdf"]
["ISOVG100",null,null,null,"0,882à15°C",null,-27,219,null,null,"Lithium",68,9.3000000000000007,"TonnaT68","SHELL","DOCHUILE\\SHELL\\TonnaT.pdf"]
["ISOVG100",null,null,null,"0,9 à 15°c",-50,260,204,180,"2","CLAY","100","14","MOBILTEMP SHC 100","MOBIL","DOC GRAISSE\\Mobil\\MOBILTEMP SHC 100.pdf"]
["ISOVG100",null,null,null,"0,89 à 20°C",-29,null,null,129,"2","LITHIUM-BISULFURE DE MOLYBDENE","114",null,"MOLYKOTE BR-2 PLUS","DOW CORNING","DOC GRAISSE\\DOW CORNING\\MolykoteBR2plus.pdf"]
["ISOVG100",null,null,null,"0,89 g/cm3 à 20°C",-30,null,232,150,"1","ALUMINIUM COMPLEX","100",null,"MOLYKOTE G-0051FG","DOW CORNING","DOC GRAISSE\\DOW CORNING\\molykote g-0050 fg3.pdf"]
["ISOVG100",null,null,null,"0,93 à 25°C",-30,null,null,170,"2","POLYUREA","125",null,"MOLYKOTE G-0010","DOW CORNING"]
["ISOVG100",null,null,null,"0,83 à 25°C",-51,null,270,163,"2","ALUMINIUM COMPLEX / PTFE","110","13,5","MOLYKOTE G-4500","DOW CORNING","DOC GRAISSE\\DOW CORNING\\Molykote_G4500.pdf"]
["ISOVG100",null,null,null,"1,1 à 25°C",-73,null,101,204,"1","LITHIUM","100 à 25°C",null,"MOLYKOTE 33","DOW CORNING","DOC GRAISSE\\DOW CORNING\\TDS_MOLYKOTE_41_eng.pdf"]
["ISOVG100",null,null,null,"0,85 à 25°C",-40,null,200,200,"2","POLYUREA","103",null,"MOLYKOTE G-6000","DOW CORNING","DOC GRAISSE\\DOW CORNING\\G-6000 TDS.pdf"]
["ISOVG1000","DIN 51517-3",null,null,"0,87g/cm3à15°C",null,-33,222,null,0,"Minérale",1000,98.8,"Mobil SHC 639","MOBIL","DOCGRAISSE\\Mobil\\MobilSCH639.pdf"]
["ISOVG1000","K0G-0",null,null,"0,91g/cm3 à 15°C",0,null,null,100,0,"Minérale",680,42.7,"Beslux Gear XP ","BRUGAROLAS","DOC HUILE\\BRUGAROLAS\\lubricantes-brugarolas_aceites_industriales.pdf"]
["ISOVG1000","K0P-20",null,null,null,-20,-33,290,150,0,"Synthétique",1000,null,"Gearmaster PGP ","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG1000","KF1S+10",null,null,"1,018 à 15°C",10,-30,null,200,1,"Argile",1040,42,"MalleusGreaseJB","SHELL","DOCGRAISSE\\schell\\MalleusGreaseJB1+2.pdf"]
["ISOVG1000","KF2C-10",null,null,"0,94à15°C",-10,null,200,60,2,"Calcium",875,36.5,"Texclad2","TEXACO","DOCGRAISSE\\texaco\\Texclad2.pdf"]
["ISOVG1000","KF2S+10",null,null,null,10,-30,null,200,2,"Argile",1040,42,"MalleusGreaseJB","SHELL","DOCGRAISSE\\schell\\MalleusGreaseJB1+2.pdf"]
["ISOVG1000","KP1G-10",null,null,"0,946 à 15°C",-10,null,204,120,"1","LITHIUM","1000","43,61","MOBILUX EP 111","MOBIL","DOC GRAISSE\\Mobil\\MLEP111-mobilux-ep-111-msds.pdf"]
["ISOVG1000","KPFHC2N-30",null,null,"1 à 15°C",-30,265,204,150,"1","LITHIUM COMPLEX","1000","83","MOBILITH SHC 1000 SPECIAL","MOBIL","DOC GRAISSE\\Mobil\\MOBILITH SHC serie.pdf"]
["ISOVG1000","OGPFOR-25",null,null,null,-10,null,null,180,"0-00","ALUMINIUM COMPLEX","1050",null,"ARALUB MKA Z 1","ARAL"]
["ISOVG1000",null,null,null,"1080 à 15°C",null,-36,285,null,0,"Synthétique",150,null,"Degol GS","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG1000",null,null,null,"1,06 g/cm3 à 15°C",null,-30,300,null,0,null,1020,170,"Berusynth EP ","BECHEM","DOC HUILE\\BECHEM\\BECHEM Berusynth EP_68_1000_9590019(GB).pdf"]
["ISOVG1000",null,null,null,"0,93 g/cm3 à 15°C",null,-3,230,null,0,"Minérale",1000,43.6,"Alpha SP","CASTROL","DOC HUILE\\CASTROL\\Alpha SP 1000.pdf"]
["ISOVG1000",null,null,null,"931 à 15°C",null,-18,253,null,0,"Minérale",956,42.7,"Tribol 1100","CASTROL","DOC HUILE\\CASTROL\\Tribol 1100.pdf"]
["ISOVG1000",null,null,null,"1074 à 15°C",null,-24,300,null,0,"Synthétique",1000,152,"Tribol 800","CASTROL","DOC HUILE\\CASTROL\\Tribol 800 .pdf"]
["ISOVG1000",null,null,null,"918 à 15°C",null,-10,270,null,0,"Minérale",680,36.799999999999997,"Renolin CLP ","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\Renolin CLP.pdf"]
["ISOVG1000",null,null,null,null,null,null,null,null,0,"Minérale",1000,null,"Renolin CLP Plus","FUCHS EUROPE "]
["ISOVG1000",null,null,null,"1075 à 15°C",null,-36,280,null,0,"Synthétique",1000,162,"Renolin PG","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\RENOLIN_PG.pdf"]
["ISOVG1000",null,null,null,"1,05 g/cm3 à 20°C",null,-20,250,null,0,"Synthétique",1000,170,"Syntheso D EP","KLÜBER","DOC HUILE\\KLUBER\\Syntheso D EP.pdf"]
["ISOVG1000",null,null,null,"1,05 g/cm3 à 15°C",null,-37,280,null,0,"Synthétique",680,114,"Glycoyle HE series","MOBIL","DOC HUILE\\MOBIL\\Glygoyle HE Series pds.pdf"]
["ISOVG1000",null,null,null,"0,937 g/cm3 à 15°C",null,-9,244,null,0,"Minérale",1000,43.5,"Carter EP","TOTAL ","DOC HUILE\\TOTAL\\CARTER EP.pdf"]
["ISOVG120","000H-20",null,null,"940 à 20°C",-25,null,200,100,"00-000","SODIUM","130","10","ARALUB FDP 00","ARAL","DOC GRAISSE\\ARAL\\aralub\\Aral Aralub FDP 00 (1).pdf"]
["ISOVG120","K2K-20",null,null,"800à20°C",-30,null,null,120,2,"Lithium",120,null,"SpheerolAP","CASTROL","DOCGRAISSE\\castrol\\SpheerolAP2,AP3.pdf"]
["ISOVG120","K2K-25",null,null,null,-25,185,200,120,"2","LITHIUM-CALCIUM","120",null,"MULTIS 2","ELF","DOC GRAISSE\\ELF\\MULTIS 2.pdf"]
["ISOVG120","K3K-20",null,null,null,-20,null,null,120,3,"Lithium",120,null,"GRMU","AGIP","DOCGRAISSE\\AGIP\\agipgrmu.pdf"]
["ISOVG120","K3K-20",null,null,null,-20,180,null,120,"3","LITHIUM-CALCIUM","120",null,"MULTIS 3","ELF","DOC GRAISSE\\ELF\\MULTIS 3.pdf"]
["ISOVG120","K3K-30",null,null,"1000 à 25°C",-30,null,150,120,3,"Lithium",120,null,"SpheerolAP","CASTROL","DOCGRAISSE\\castrol\\SpheerolAP2,AP3.pdf"]
["ISOVG120","KP2P-30",null,null,"0,95g/cm3à25°C",-30,230,100,160,2,"Lithium complex",112,10.8,"Renolit Duraplex EP2","FUCHSEUROPE","DOCGRAISSE\\FUCHSEUROPE\\RENOLIT_DURAPLEX_EP_2.pdf"]
["ISOVG120",null,null,null,"0,910 g/cm3 à 25°C",-20,260,null,150,"2","LITHIUM COMPLEX","101","11,5","MOLYKOTE G-0101","DOW CORNING","DOC GRAISSE\\DOW CORNING\\MOLYKOTE G-0101.pdf"]
["ISOVG150","DIN 51517",null,null,"904à15°C",-30,-24,238,120,0,"Minérale",150,14.5,"ENERGOLGR-XP150","BP","DOCHUILE\\BP\\ENERGOLGR-XP.pdf"]
["ISOVG150","DIN 51517-3",null,null,"0,847g/cm3à15°C",null,-51,205,null,0,"Minérale",150,21,"SUPERTAUROSINTETICO150","REPSOL","DOCHUILE\\REPSOL\\Lubrifiant_SUPER_TAURO_SINTETICO.pdf"]
["ISOVG150","DIN 51517-3",null,null,"884à15°C",null,-27,240,null,0,"Minérale",150,14.7,"SPARTANEP.150","ESSO","DOCHUILE\\ESSO\\SpartanEPseries.pdf"]
["ISOVG150","DIN 51517-3",null,null,"0,892à15°C",-30,-21,227,400,0,"Minérale",153.4,14.8,"CARTEREP.150","TOTAL","DOCHUILE\\TOTAL\\CARTEREP.pdf"]
["ISOVG150","DIN 51517-3",null,null,null,-40,-40,244,140,0,"Minérale",150,null,"CORVUS150EP","VERKOL","DOCHUILE\\verkol\\CORVUS-150EP.pdf"]
["ISOVG150","DIN 51517-4",null,null,"886à20°C",null,-24,195,100,0,"Minérale",150,15,"OMALA150","SHELL","DOCHUILE\\SHELL\\ShellOmala.pdf"]
["ISOVG150","DIN 51517-5",null,null,"0,899g/cm3à15°C",null,-18,215,null,0,"Minérale",151.1,14.9,"ENGRANAJESHP.150","CEPSA","DOCHUILE\\CEPSA\\CEPSA-ENGRANAJE-HP.pdf"]
["ISOVG150","DIN 51517-6",null,null,"849à15°C",null,-54,235,null,0,"Minérale",150,19.7,"OMALAOILHD.150","SHELL","DOCHUILE\\SHELL\\ShellOmalaHD.pdf"]
["ISOVG150","DIN 51524-2",null,null,"0,895à15°C",null,-24,238,null,0,"Huile hydrolique",150,14.7,"OSO150","AGIP","DOCHUILE\\AGIP\\oso.pdf"]
["ISOVG150","GP00G-20",null,null,null,-20,null,null,100,"00","LITHIUM","150",null,"MOBILUX EP 004","MOBIL","http://www.mobil.com/Australia-English/Lubes/PDS/GLXXENGRSMOMobilux_EP.aspx"]
["ISOVG150","GP0G20",null,null,"0,918 à 15°C",-20,null,204,120,"0","Lithium/Lithium complex",160,16,"Mobilux EP","MOBIL","DOCGRAISSE\\Mobil\\mobilux_ep234.pdf"]
["ISOVG150","GP0G-20",null,null,"0,918 à 15°C",-20,null,204,100,"0","LITHIUM","150",null,"MOBILUX EP 0","MOBIL","http://www.mobil.com/Australia-English/Lubes/PDS/GLXXENGRSMOMobilux_EP.aspx"]
["ISOVG150","K0G-20",null,null,null,-20,-27,265,100,0,"Minérale",150,15,"Staroil G ","BECHEM","DOC HUILE\\BECHEM\\Staroil No. 100.pdf"]
["ISOVG150","K0K-15",null,null,null,-15,-24,254,120,0,"Minérale",150,null,"Gearmaster CLP","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG150","K0K-20",null,null,"900 à 20°C",-20,170,200,120,0,"Lithium/Lithium complex",150,15,"MultisEP","TOTAL","DOCGRAISSE\\Total\\MULTISEP0FR.pdf"]
["ISOVG150","K0N-30",null,null,null,-30,-39,250,147,0,"Synthétique",150,null,"Gearmaster SYN","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG150","K0N-30",null,null,null,-30,-39,230,150,0,"Synthétique",150,null,"Gearmaster PGP ","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG150","K2K-40",null,null,"1 g/cm 3 à 25 °C",-20,250,150,110,2,"Aluminium complex",130,7.3,"LGHP2","SKF","DOCGRAISSE\\SKF\\12048EN_LGFP2.pdf"]
["ISOVG150","K2N-20",null,null,"1000à15°C",-20,null,200,140,2,"Lithium complex",150,null,"SpheerolEPL","CASTROL","DOCGRAISSE\\castrol\\Castrol-Spheerol-EPL.pdf"]
["ISOVG150","K2N-20",null,null,"900à15ºC.",-20,260,150,140,2,"Lithium complex",160,15.5,"RetinaxLX","SHELL","DOCGRAISSE\\schell\\RetinaxLX.pdf"]
["ISOVG150","K2N-30",null,null,"950 à 20°C",-30,55,204,140,2,"Lithium complex",150,null,"EnergreaseLC","BP","DOCGRAISSE\\BP\\EnergreaseLC2.pdf"]
["ISOVG150","KP1K-20",null,null,null,-20,190,204,120,1,"Lithium",155,16,"BEACONEP1","ESSO","DOCGRAISSE\\Esso\\PI_ESSO_Beacon_EP.pdf"]
["ISOVG150","KP1K-30",null,null,"1000 à 15°C",-30,-23,230,120,"1","Lithium/Lithium complex",150,54,"Tribol3020/1000","CASTROL","DOCGRAISSE\\castrol\\tribol_3020_1000_1_2_eu_tds.pdf"]
["ISOVG150","KP1K-30",null,null,"0,92 à 15°C",-30,null,204,120,"1","LITHIUM","150",null,"MOBILUX EP 1","MOBIL","http://www.mobil.com/Australia-English/Lubes/PDS/GLXXENGRSMOMobilux_EP.aspx"]
["ISOVG150","KP2K-20",null,null,"0,922 à 15°C",-20,190,204,130,2,"lithium",160,16,"BeaconEP2","ESSO","DOCGRAISSE\\Esso\\PI_ESSO_Beacon_EP.pdf"]
["ISOVG150","KP2K-20",null,null,"900à15°C",null,180,140,null,2,"lithium",190,16,"AlvaniaEP2","SHELL","DOCGRAISSE\\schell\\alvaniaep2.pdf"]
["ISOVG150","KP2K-30",null,null,"1001 à 15°C",-30,-23,230,120,"2","Lithium/Lithium complex",150,54,"Tribol3020/1000","CASTROL","DOCGRAISSE\\castrol\\tribol_3020_1000_1_2_eu_tds.pdf"]
["ISOVG150","KP2K-30",null,null,"920à15°C",-20,null,210,120,2,"Lithium",150," ","EPEXA2","ELf","DOCGRAISSE\\ELF\\epexa.pdf"]
["ISOVG150","KP2K-30",null,null,"0,92 à 15°C",-30,null,204,120,"2","LITHIUM","150",null,"MOBILUX EP 2","MOBIL","http://www.mobil.com/Australia-English/Lubes/PDS/GLXXENGRSMOMobilux_EP.aspx"]
["ISOVG150","KP2K-30L",null,null,"0,901à15°C",-20,260,200,140,"2","Lithium complex",115,null,"RonexMP","MOBIL","DOCGRAISSE\\Mobil\\RonexMP.pdf"]
["ISOVG150","KP2P-20",null,null,null,-25,null,null,150,"2",null,"150",null,"ARALUB HTR 2","ARAL"]
["ISOVG150","KP2P-30",null,null,"890 à 15°C",-30,null,230,150,2,"Lithium",180,null,"LMXGREASE","CASTROL","DOCGRAISSE\\castrol\\LMXGREASE.pdf"]
["ISOVG150","KP2P-30",null,null,null,-30,260,null,150,2,"Lithium complex",160,14,"AralubMKL","ARAL","DOCGRAISSE\\ARAL\\AralAralubMKL2.pdf"]
["ISOVG150","KP3K-20",null,null,"0,9g/cm3à20°C",-20,null,null,130,3,"Minérale",180,14,"Klüber Centoplex2EP","KLÜBER","DOCGRAISSE\\Klüber\\CENTOPLEX_0_EP_2_EP-en.pdf"]
["ISOVG150","KP3K-20",null,null,"0,92 à 15°C",-20,null,204,130,3,"Lithium",160,16,"Mobilux EP3","MOBIL","DOCGRAISSE\\Mobil\\mobilux_ep234.pdf"]
["ISOVG150","KP3K-20",null,null,"1 à 15°C",-20,null,204,120,"3","LITHIUM","150",null,"MOBILUX EP 3","MOBIL","http://www.mobil.com/Australia-English/Lubes/PDS/GLXXENGRSMOMobilux_EP.aspx"]
["ISOVG150",null,null,null,"846 à 15°C",null,-54,260,null,0,"Synthétique",150,19,"Cassida Chain Oil 150","SHELL","DOC HUILE\\SHELL\\Cassida Chain Oil 150.pdf"]
["ISOVG150",null,null,null,"0,885 g/cm3 à 15°C",null,-12,282,null,0,"Minérale",150,null,"Degol BG","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG150",null,null,null,"0,892 g/cm3 à 15°C",null,-21,245,null,0,"Minérale",150,null,"Degol BG Plus","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG150",null,null,null,"0,872 g/cm3 à 15°C",null,-51,222,null,0,"Synthétique",150,null,"Degol PAS ","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG150",null,null,null,"1 g/cm3 à 15°C",null,-45,236,null,0,"Synthétique",150,null,"Degol GS","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG150",null,null,null,null,null,null,null,null,0,"Minérale",150,null,"Eco Gear M","BECHEM","DOC HUILE\\BECHEM\\Bechem lubricants for high load and high temperature.pdf"]
["ISOVG150",null,null,null,null,null,null,null,null,0,"Synthétique",150,null,"Eco Gear S","BECHEM","DOC HUILE\\BECHEM\\Bechem lubricants for high load and high temperature.pdf"]
["ISOVG150",null,null,null,"889 à 15°C",null,-15,238,null,0,"Minérale",150,14,"Energol GR-XF ","BP","DOC HUILE\\BP\\ENERGOL GR-XF.pdf"]
["ISOVG150",null,null,null,"904 à 15°C",null,-24,238,null,0,"Minérale",150,14.5,"Energol GR-XP","BP","DOC HUILE\\BP\\ENERGOL GR-XP.pdf"]
["ISOVG150",null,null,null,"0,86 à 15°C",null,-48,220,null,0,"Synthétique",150,18,"Alphasyn EP ","CASTROL","DOC HUILE\\CASTROL\\Alphasyn EP.pdf"]
["ISOVG150",null,null,null,"0,92 à 15°C",null,-18,220,null,0,"Minérale",150,14.3,"Alpha SP","CASTROL","DOC HUILE\\CASTROL\\Alpha SP.pdf"]
["ISOVG150",null,null,null,"897 à 15°C",null,-27,245,null,0,"Minérale",151,14.7,"Tribol 1100","CASTROL","DOC HUILE\\CASTROL\\Tribol 1100.pdf"]
["ISOVG150",null,null,null,"1,05 g/cm3 à 15°C",null,-39,210,null,0,"Synthétique",150,28,"Alphasyn PG","CASTROL","DOC HUILE\\CASTROL\\Alphasyn PG.pdf"]
["ISOVG150",null,null,null,"1056 à 15°C",null,-36,280,null,0,"Synthétique",150,26,"Tribol 800","CASTROL","DOC HUILE\\CASTROL\\Tribol 800 .pdf"]
["ISOVG150",null,null,null,"884 à 15°C",null,-27,240,null,0,"Minérale",150,14.7,"Spartan EP series","ESSO","DOC HUILE\\ESSO\\Spartan EP series.pdf"]
["ISOVG150",null,null,null,"849 à 15°C",null,-45,250,null,0,"Synthétique",150,19.399999999999999,"Renolin Unisyn CLP series","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\RENOLIN_UNISYN_CLP.pdf"]
["ISOVG150",null,null,null,"894 à 15°C",null,-24,250,null,0,"Minérale",150,14.5,"Renolin CLP","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\Renolin CLP.pdf"]
["ISOVG150",null,null,null,null,null,null,null,null,0,"Minérale",150,null,"Renolin CLP Plus","FUCHS EUROPE"]
["ISOVG150",null,null,null,"1051 à 15°C",null,-51,260,null,0,"Synthétique",145,27,"Renolin PG","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\RENOLIN_PG.pdf"]
["ISOVG150",null,null,null,"1,05g/cm3 à 20°C",null,-40,200,null,0,"Synthétique",150,29,"Syntheso D EP","KLÜBER","DOC HUILE\\KLUBER\\Syntheso D EP.pdf"]
["ISOVG150",null,null,null,"0,855 g/cm3 à 15°C",null,-48,240,null,0,"Synthétique",150,21.6,"Mobilgear SHC XMP","MOBIL","DOC HUILE\\MOBIL\\Mobilgear SHC XMP Series pds.pdf"]
["ISOVG150",null,null,null,"0,86 g/cm3 à 15°C",null,-45,228,null,0,"Minérale",143,18.3,"Mobil SHC 600 series","MOBIL","DOC HUILE\\MOBIL\\Mobil_SHC_600.pdf"]
["ISOVG150",null,null,null,"0,896 g/cm3 à15°C",null,-27,258,null,0,"Minérale",150,14.6,"Mobilgear XMP series","MOBIL","DOC HUILE\\MOBIL\\mobilgear_xmp_series.pdf"]
["ISOVG150",null,null,null,"849 à 15°C",null,-54,235,null,0,"Synthétique",150,19.7,"Shell Omala HD ","SHELL","DOC HUILE\\SHELL\\Shell Omala HD.pdf"]
["ISOVG150",null,null,null,"886 à 20°C",null,-24,195,null,0,"Minérale",150,15,"Shell Omala","SHELL","DOC HUILE\\SHELL\\Shell Omala.pdf"]
["ISOVG150",null,null,null,"0,897 à 15°C",null,-21,196,null,0,"Minérale",150,15,"Shell Omala F","SHELL","DOC HUILE\\SHELL\\Shell Omala F.pdf"]
["ISOVG150",null,null,null,"0,89 à 15°C",null,-30,240,null,0,"Minérale",142,14.4,"Meropa","TEXACO","DOC HUILE\\TEXACO\\Meropa150.pdf"]
["ISOVG150",null,null,null,"0,89 à 15°C",null,-24,248,null,0,"Minérale",150,14.5,"Meropa WM ","TEXACO","DOC HUILE\\TEXACO\\meropa_wm_pds.pdf"]
["ISOVG150",null,null,null,"856,5 à 15°C",null,-45,230,null,0,"Synthétique",147.9,19.399999999999999,"Carter SH","TOTAL ","DOC HUILE\\TOTAL\\Carter-SH.pdf"]
["ISOVG150",null,null,null,"892 à 15°C",null,-27,227,null,0,"Minérale",153.4,14.8,"Carter EP","TOTAL ","DOC HUILE\\TOTAL\\CARTER EP.pdf"]
["ISOVG150",null,null,null,null,null,-12,250,null,0,null,150,null,"ODIEL150","ERTOIL"]
["ISOVG150",null,null,null,"0,910 g/cm3 à 25°C",-25,null,300,140,"2","CALCIUM COMPLEX","150","11,2","MOLYKOTE G-0102","DOW CORNING","DOC GRAISSE\\DOW CORNING\\TDS_MOLYKOTE_G_0102_eng.pdf"]
["ISOVG1500","KP0-20",null,null,null,-20,200,null,120,"00-0","LITHIUM","1500",null,"MOBILGEAR OGL 009","MOBIL"]
["ISOVG1500","KPHC1N-30",null,null,"1 à 15°C",-30,265,204,150,"1","LITHIUM COMPLEX","1370","100","MOBILITH SHC 1500","MOBIL","DOC GRAISSE\\Mobil\\MOBILITH SHC serie.pdf"]
["ISOVG1500","KPHC2N-30",null,null,"1 à 15°C",-30,265,204,150,"2","LITHIUM COMPLEX","1370","100","MOBILITH SHC 1500","MOBIL","DOC GRAISSE\\Mobil\\MOBILITH SHC serie.pdf"]
["ISOVG1500",null,null,null,"1 à 25°C",0,null,200,160,"2","BISULFURE DE MOLYBDENE","1500",null,"MOLYKOTE 1122","DOW CORNING","DOC GRAISSE\\DOW CORNING\\TDS_MOLYKOTE_1122_eng.pdf"]
["ISOVG180","1K-20",null,null,"1000 à 20°C ",-20,null,null,120,"0-1","LITHIUM","170",null,"ARALUB LFZ 1","ARAL","DOC GRAISSE\\ARAL\\aralub\\216331Aral Aralub LFZ 1.pdf"]
["ISOVG180","G00R-20",null,null,null,-20,280,null,120,"00","Lithium/Lithium complex",180,null,"Notropeen LXG00","FUCHSEUROPE","DOCGRAISSE\\FUCHSEUROPE\\NotropeenLXG00.pdf"]
["ISOVG180","GP000E-30",null,null,null,-30,null,null,90,"0","Lithium/Lithium complex",null,null,"Rhus LIC","BECHEM"]
["ISOVG180","K00P-40",null,null,"0,9g/cm3à20°C",-40,220,190,160,"00","Synthetic",180,null,"Gearmaster","FUCHS","DOCGRAISSE\\fuchs\\GearmasterLXG00.pdf"]
["ISOVG180","K0K-20",null,null,null,-30,null,null,140,"00","Lithium/Lithium complex",180,null,"Gearmaster LI400","FUCHSEUROPE","DOCGRAISSE\\FUCHSEUROPE\\GEARMASTER_LI_400_ru.pdf"]
["ISOVG180","K3K-30",null,null,"1000à25°C",-30,195,150,120,"3","Lithium/Lithium complex",180,null,"Energrease LS-EP","BP","DOCGRAISSE\\BP\\Energrease_LS-EP_series.pdf"]
["ISOVG180","KP1N-30",null,null,"1à15°C",-30,null,230,150,1,"Lithium complex",185,16.5,"Energrease LC","BP","DOCGRAISSE\\BP\\EnergreaseLC2.pdf"]
["ISOVG180","KP2K-20",null,null,"900à15°C",-20,180,250,120,2,"Lithium",190,16,"Alvania EP(LF)","SHELL","DOCGRAISSE\\schell\\AlvaniaEP1et2.pdf"]
["ISOVG180","KP2M-20",null,null,"0,9 g/cm3 à 20°C",-20,null,null,130,2,"Lithium",180,14,"Centoplex 2EP","KLÜBER","DOCGRAISSE\\Klüber\\CENTOPLEX_2_3-en.pdf"]
["ISOVG180","KP2M-30",null,null,"900 à 15°C",-30,null,140,130,2,"Lithium",188,15.16,"Retinax EP","SHELL","DOCGRAISSE\\schell\\RetinaxEP2.pdf"]
["ISOVG180","KP2N-30",null,null," 0.91 g/cm3 à 15°C",-30,250,150,150,2,"Lithium complex",180,16,"BeruplexLI-EP2","BECHEM","DOCGRAISSE\\bechem\\LI_EP_2_5307201(RUS).pdf"]
["ISOVG2000","KP00U-10",null,null,"1 à 15°C",-20,193,243,268,"00-0","LITHIUM","2000","120","MOBIL DYNAGEAR 2000","MOBIL","DOC GRAISSE\\Mobil\\mobil_dynagear_2000.pdf"]
["ISOVG22","K0M-20",null,null,"0,88  à 15°C",-20,-33,180,110,0,"Minérale",22,null,"Fluid Drive HM","BRUGAROLAS","DOC HUILE\\BRUGAROLAS\\lubricantes-brugarolas_aceites_industriales.pdf"]
["ISOVG22","KP2M-40",null,null,"0,99g/cm3à20°C",-40,220,230,130,2,"Barium complex",21,4.7,"IsoflexNBU15","KLÜBER","DOCGRAISSE\\Klüber\\ISOFLEX-NBU-Donnees-Techniques.pdf"]
["ISOVG22",null,null,null,"857 à 15°C",null,-33,215,null,0,"Minérale",22,4.4000000000000004,"Oso - D ","AGIP","DOC HUILE\\AGIP\\Oso - D.pdf"]
["ISOVG22",null,null,null,"0,857 à 15°C",null,-39,192,null,0,"Minérale",22,5.2,"Arnica","AGIP","DOC HUILE\\AGIP\\Arnica.pdf"]
["ISOVG22",null,null,null,"0,856 à 15°C",null,-30,195,null,0,"Minérale",21.5,4.2,"Oso","AGIP","DOC HUILE\\AGIP\\oso.pdf"]
["ISOVG22",null,null,null,"905 à 15°C",null,-21,260,null,0,"Synthétique",22,null,"Vitam EHF ","ARAL","http://www.lubebase.com/"]
["ISOVG22",null,null,null,"864 à 15°C",null,-21,214,null,0,"Minérale",22,null,"Vitam DE ","ARAL","http://www.lubebase.com/"]
["ISOVG22",null,null,null,"862 à 15°C",null,-21,210,null,0,"Minérale",22,null,"Vitam GF ","ARAL","http://www.lubebase.com/"]
["ISOVG22",null,null,null,null,null,null,null,null,0,"Minérale",22,null,"Staroil No. 22","BECHEM"]
["ISOVG22",null,null,null,"0,87 à 15°C",null,-30,205,null,0,"Minérale",22,4.21,"Energol HLP-HM ","BP","DOC HUILE\\BP\\Energol HLP-HM.pdf"]
["ISOVG22",null,null,null,"870 à 15°C",null,-33,205,null,0,"Minérale",22,4.3,"Hyspin SP ","CASTROL","DOC HUILE\\CASTROL\\Hyspin SP.pdf"]
["ISOVG22",null,null,null,"861 à 15°C",null,-30,180,null,0,"Minérale",22,4.3,"Tribol 943 AW ","CASTROL","DOC HUILE\\CASTROL\\Tribol 943 AW.pdf"]
["ISOVG22",null,null,null,"865 à 15°C",null,-30,180,null,0,"Minérale",22,4.2,"HLPD-Oel ","ESSO","DOC HUILE\\ESSO\\HLPD-Oel.PDF"]
["ISOVG22",null,null,null,"926  à 15°C",null,-36,240,null,0,"Synthétique",22,5.4,"Plantohyd S","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\238_Planto Brochure.pdf"]
["ISOVG22",null,null,null,"861 à 15°C",null,-27,180,null,0,"Minérale",22,4.3,"Renolin B ","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\RENOLIN_B.pdf"]
["ISOVG22",null,null,null,"868 à 15°C",null,-30,165,null,0,"Minérale",22,4.3,"RENOLIN MR 310","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\RENOLIN_MR.pdf"]
["ISOVG22",null,null,null,"0,86 à 15°C",null,-30,200,null,0,"Minérale",21,4.5,"Mobil DTE 20 series","MOBIL","DOC HUILE\\MOBIL\\Mobil DTE 20 series.pdf"]
["ISOVG22",null,null,null,"865 à 15°C",null,-36,202,null,0,"Minérale",22,4.3,"Nuto H series","MOBIL","DOC HUILE\\MOBIL\\Nuto.pdf"]
["ISOVG22",null,null,null,"1 à 15°C",null,-57,236,null,0,"Synthétique",23.2,4.5999999999999996,"MOBIL EAL ARCTIC  series","MOBIL","DOC HUILE\\MOBIL\\ss_eal_arctic.pdf"]
["ISOVG22",null,null,null,"0,866 à 15°C",null,-30,204,null,0,"Minérale",22,4.3,"Tellus","SHELL","DOC HUILE\\SHELL\\Tellus.pdf"]
["ISOVG22",null,null,null,"868 à 15°C",null,-27,189,null,0,"Minérale",22,4.3,"Tellus DO","SHELL","DOC HUILE\\SHELL\\Tellus DO(TDS).pdf"]
["ISOVG22",null,null,null,null,null,null,null,null,0,"Minérale",22,null,"Alcor DD ","TEXACO"]
["ISOVG22",null,null,null,null,null,-36,177,null,0,"Minérale",23.1,4.4000000000000004,"Rando HD","TEXACO","DOC HUILE\\TEXACO\\Rando HD.pdf"]
["ISOVG22",null,null,null,"866 à 15°C",null,-36,202,null,0,"Minérale",22.5,4.4000000000000004,"Azolla DZF","TOTAL ","DOC HUILE\\TOTAL\\Azolla DZF.pdf"]
["ISOVG22",null,null,null,"867 à 15°C",null,-30,221,null,0,"Minérale",22.5,4.4000000000000004,"Azolla ZS","TOTAL ","DOC HUILE\\TOTAL\\AZOLLA_ZS.pdf"]
["ISOVG22",null,null,null,"0,866à15°C",null,-30,218,null,null,"Hydraulique",22,4.3,"TellusC22","SHELL","DOCHUILE\\SHELL\\Tellus.pdf"]
["ISOVG220"," KPHC1N-40",null,null,"0,863 g/cm3 à 15°C",-40,-36,220,150,"1","LITHIUM COMPLEX","220","34,7","MOBILITH SHC PM 220","MOBIL","DOC GRAISSE\\Mobil\\ss_mobilith_shc_pm.pdf"]
["ISOVG220","DIN 51502",null,null,"1000à15°C",null,-36,230,null,0,"Polyglycol",228,36,"CLPPGVG220","EUROLUB","DOCHUILE\\EUROLUB\\CLP_PG_220_PI_D.pdf"]
["ISOVG220","DIN 51517",null,null,"0846à15°C",null,-20,245,null,0,"Minérale",210.3,25,"ENGRANAJESHPX.220","CEPSA","DOCHUILE\\CEPSA\\ht_cepsa_engranajes_hpx_eng.pdf"]
["ISOVG220","DIN 51517-3",null,null,"899à15°C",null,-18,200,null,0,"Minérale",220,19.399999999999999,"Omala220","SHELL","DOCHUILE\\SHELL\\Omala220.pdf"]
["ISOVG220","DIN 51517-3",null,null,"0,89à15,6°C(Kg/L)",-24,-9,200,240,0,"Minérale",220,19,"Mobilgear 600-XP220","MOBIL","S:\\2015\\CULRICH\\stage\\DOCHUILE\\MOBIL\\mobilgear600_xp_220.pdf"]
["ISOVG220","DIN 51517-3",null,null,"1060à15°C",-35,-35,250,160,0,"Polyglycol",220,40,"KlübersynthGH6-220","KLÜBER","DOCHUILE\\KLUBER\\KlubersynthGH6.pdf"]
["ISOVG220","DIN 51517-3",null,null,"860à15°C",null,-42,220,null,0,"Minérale",200,25,"ALPHASYN-EP220","CASTROL","DOCHUILE\\CASTROL\\AlphasynEP.pdf"]
["ISOVG220","DIN 51517-3",null,null,"1g/cm3 à 15°C",null,-45,280,null,0,"Synthetic",220,36,"AralDegol/PAS220","ARAL","DOCHUILE\\ARAL\\DEGOL.pdf"]
["ISOVG220","GP00k-30",null,null,null,-30,170,null,110,"00","Lithium/Lithium complex",190,15,"AlvaniaGL","SHELL","DOCGRAISSE\\schell\\ShellAlvaniaGL00_f.pdf"]
["ISOVG220","GPFHC00K-30",null,null,"0,871 à 15°C",-30,270,188,170,"00","POLYUREA","220","30","MOBIL SHC POLYREX 005","MOBIL","DOC GRAISSE\\Mobil\\mobil_shc_polyrex_series.pdf"]
["ISOVG220","K00K+30",null,null,"0,93g/cm3 à 20°C",{"$f":"--30","v":30},null,200,120,"00","Lithium/Lithium complex",195,null,"AutolTop2000Typ00","AGIP","DOCGRAISSE\\AGIP\\agipautoltop2000type00.pdf"]
["ISOVG220","K0K-15",null,null,null,-15,-21,220,120,0,"Minérale",220,null,"Gearmaster CLP","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG220","K0K-20",null,null,null,-20,180,null,120,0,"Lithium/Lithium complex",220,18,"RenolitFEP","FUCHSEUROPE","DOCGRAISSE\\fuchs\\RENOLIT_FEP_0.pdf"]
["ISOVG220","K0N-20",null,null,null,-20,-39,250,150,0,"Synthétique",220,null,"Gearmaster SYN","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG220","K0N-30",null,null,null,null,null,null,null,0,"Minérale",220,null,"Renolin CLP Plus","FUCHS EUROPE "]
["ISOVG220","K0U-40",null,null,"0,956 à 15°C",-40,-45,260,250,0,"Synthétique",250,25,"Berusynth CU ","BECHEM","DOC HUILE\\BECHEM\\BECHEM Berusynth CU_100_9306309(GB).pdf"]
["ISOVG220","K2N-20",null,null,"900 à 15 °C",-20,232,250,140,2,"Lithium",220,19,"GadusS3V220C","SHELL","DOCGRAISSE\\schell\\Gadus_S3_V220C_2_(en)_TDS.pdf"]
["ISOVG220","K2N-20",null,null,"0,916g/cm3à20°C",-20,-23,225,140,2,"Lithium complex",220,19,"Tribol4020/220-2","CASTROL","DOCGRAISSE\\castrol\\Tribol4020.pdf"]
["ISOVG220","K2N-20",null,null,"900à15°C",-20,null,200,140,2,"Lithium complex",210,17.8,"MultiscomplexS2A","TOTAL","DOCGRAISSE\\Total\\MULTIS-COMPLEX-S2Agb.pdf"]
["ISOVG220","K2P-40",null,null,"0,93à15°C",-40,-12,274,170,2,"Lithium complex",226,20.7,"Starplex","TEXACO","DOCGRAISSE\\texaco\\Starplex2.pdf"]
["ISOVG220","KP1N-20",null,null,null,-20,280,204,140,"1","LITHIUM COMPLEX","220",null,"MOBILGREASE XHP 221","MOBIL","DOC GRAISSE\\Mobil\\FT_Mobilgrease_XHP_fr221 222.pdf"]
["ISOVG220","KP2G-30",null,null,"0,95 à 20°C",-30,null,200,110,"2","Lithium/Lithium complex",850,null,"AutolTop2000","AGIP","DOCGRAISSE\\AGIP\\AGIP_Top_2000.pdf"]
["ISOVG220","KP2K-30",null,null,"0,92 à 15°C",-20,175,204,130,2,"Lithium",150,45,"Mobilux EP2","MOBIL ","DOCGRAISSE\\Mobil\\mobilux_ep234.pdf"]
["ISOVG220","KP2K-30",null,null,null,-40,null,null,175,"2","POLYUREA","235","18,4","MOBIL POLYREX EP 2","MOBIL","http://www.mobil.com/USA-English/Lubes/PDS/GLXXENGRSMOMobil_Polyrex_EP_2.aspx"]
["ISOVG220","KP2M-20",null,null,"0,9 g/cm3à 25 °C",-20,-36,236,130,2,"Lithium",200,null,"LagermeisterEP2","FUCHSEUROPE","DOCGRAISSE\\FUCHSEUROPE\\LagermeisterEP2.pdf"]
["ISOVG220","KP2N-15",null,null,"0,99g/cm3 à 20°C",-15,null,250,140,2,"Minérale+barium complex",220,19,"StaburagsNBU12","KLÜBER","DOCGRAISSE\\Klüber\\STABURAGS_NBU_12.pdf"]
["ISOVG220","KP2N-20",null,null,"0,95 g/cm3 à 20 °C",-20,180,206,140,2,"Lithium",200,null,"RenolitF-EP","FUCHSEUROPE","DOCGRAISSE\\fuchs\\RENOLIT_FEP_0.pdf"]
["ISOVG220","KP2N-20",null,null,"0,91 à 15°C",-20,280,204,140,"2","LITHIUM COMPLEX","220","16","MOBILGREASE XHP 222","MOBIL","DOC GRAISSE\\Mobil\\FT_Mobilgrease_XHP_fr221 222.pdf"]
["ISOVG220","KPF2K-20",null,null,"0,88 à 15°C",-20,null,249,120,"2","ALUMINIUM COMPLEX","220",null,"MOBILGREASE FM 222","MOBIL","http://www.mobil.com/Australia-English/Lubes/PDS/GLXXENGRSMOMobilgrease_FM_101_FM_222.aspx"]
["ISOVG220","KPFHC1P-30",null,null,null,-30,260,188,170,"1","POLYUREA","220","30","MOBIL SHC POLYREX 221","MOBIL","DOC GRAISSE\\Mobil\\mobil_shc_polyrex_series.pdf"]
["ISOVG220","KPFHC2P-30",null,null,"0,881 à 15°C",-30,270,188,170,"2","POLYUREA","220","30","MOBIL SHC POLYREX 222","MOBIL","DOC GRAISSE\\Mobil\\mobil_shc_polyrex_series.pdf"]
["ISOVG220","KPHC2N-30",null,null,"0,9 à 15°c",-40,265,204,150,"2","LITHIUM COMPLEX","220","23,8","MOBILITH SHC 220","MOBIL","DOC GRAISSE\\Mobil\\MOBILITH SHC serie.pdf"]
["ISOVG220",null,null,null,"1012 à 15°C",null,-24,260,null,0,"Minérale",220,18.899999999999999,"Renolin CLP Plus","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\catalogue fuchs.pdf"]
["ISOVG220",null,null,null,"1000 à 15°C",null,-15,235,null,0,"Minérale",220,18.8,"Degol BG Plus","ARAL","DOC HUILE\\ARAL\\Degol BG 220 Plus.pdf"]
["ISOVG220",null,null,null,"0,898 à 15°C",null,-15,274,null,0,"Minérale",220,null,"DEGOL BG","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG220",null,null,null,"0,872 à 15°C",null,-51,190,null,0,"Synthétique",220,null,"Degol PAS ","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG220",null,null,null,"1 à 15°C",null,-45,280,null,0,"Synthétique",220,null,"Degol GS","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG220",null,null,null,null,null,null,null,null,0,"Minérale",220,null,"Eco Gear M","BECHEM"]
["ISOVG220",null,null,null,null,null,null,null,null,0,"Minérale",220,null,"Staroil G ","BECHEM","DOC HUILE\\BECHEM\\STAROIL G.docx"]
["ISOVG220",null,null,null,null,null,null,null,null,0,"Synthétique",220,null,"Eco Gear S","BECHEM"]
["ISOVG220",null,null,null,"1,02 g/cm3 à 15°C",null,-33,270,null,0,"Synthétique",228,35,"Berusynth EP ","BECHEM","DOC HUILE\\BECHEM\\BECHEM Berusynth EP_68_1000_9590019(GB).pdf"]
["ISOVG220",null,null,null,"907 à 15°C",null,-18,241,null,0,"Minérale",210,18,"Energol GR-XF ","BP","DOC HUILE\\BP\\ENERGOL GR-XF.pdf"]
["ISOVG220",null,null,null,"908 à 15°C",null,-21,241,null,0,"Minérale",220,18.8,"Energol GR-XP","BP","DOC HUILE\\BP\\ENERGOL GR-XP.pdf"]
["ISOVG220",null,null,null,"0,86 à 15°C",null,-42,220,null,0,"Synthétique",220,25,"Enersyn EP-XF ","BP","DOC HUILE\\BP\\Enersyn EP-XF.pdf"]
["ISOVG220",null,null,null,"1,02 à 15°C",null,-36,280,null,0,"Synthétique",220,null,"Enersyn SG-XP ","BP","DOC HUILE\\BP\\Enersyn SG-XP.pdf"]
["ISOVG220",null,null,null,"0,907 g/cm3 à 15°C",null,null,null,null,0,"Minérale",220,18.899999999999999,"Beslux Gear XP ","BRUGAROLAS","DOC HUILE\\BRUGAROLAS\\lubricantes-brugarolas_aceites_industriales.pdf"]
["ISOVG220",null,null,null,"0,86  à 15°C",null,-42,220,null,0,"Synthétique",220,25,"Alphasyn EP ","CASTROL","DOC HUILE\\CASTROL\\Alphasyn EP.pdf"]
["ISOVG220",null,null,null,"0,89  à 15°C",null,-18,225,null,0,"Minérale",220,18.7,"Alpha SP","CASTROL","DOC HUILE\\CASTROL\\Alpha SP.pdf"]
["ISOVG220",null,null,null,"865 à 15°C",null,-30,240,null,0,"Synthétique",220,23.9,"Tribol 1710","CASTROL","DOC HUILE\\CASTROL\\Tribol 1710 .pdf"]
["ISOVG220",null,null,null,"904 à 15°C",null,-24,245,null,0,"Minérale",220,18.899999999999999,"Tribol 1100","CASTROL","DOC HUILE\\CASTROL\\Tribol 1100.pdf"]
["ISOVG220",null,null,null,"1,06 à 15°C",null,-39,210,null,0,"Synthétique",220,40,"Alphasyn PG","CASTROL","DOC HUILE\\CASTROL\\Alphasyn PG.pdf"]
["ISOVG220",null,null,null,"1070 à 15°C",null,-30,290,null,0,"Synthétique",220,34,"Tribol 800","CASTROL","DOC HUILE\\CASTROL\\Tribol 800 .pdf"]
["ISOVG220",null,null,null,"0,895 à 15°C",null,-18,220,null,0,"Synthétique",220,null,"Reductel SP","ELF ","DOC HUILE\\ELF\\Reductel SP.pdf"]
["ISOVG220",null,null,null,"891 à 15°C",null,-15,240,null,0,"Minérale",220,18.600000000000001,"Spartan EP series","ESSO","DOC HUILE\\ESSO\\Spartan EP series.pdf"]
["ISOVG220",null,null,null,null,null,-30,290,null,0,"Synthétique",210,28.8,"Glycolube","ESSO","DOC HUILE\\ESSO\\Esso Glycolube 220, 460.doc"]
["ISOVG220",null,null,null,"852 à 15°C",null,-45,260,null,0,"Synthétique",220,25.7,"Renolin Unisyn CLP series","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\RENOLIN_UNISYN_CLP.pdf"]
["ISOVG220",null,null,null,"896 à 15°C",null,-24,260,null,0,"Minérale",220,18.899999999999999,"Renolin CLP","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\Renolin CLP.pdf"]
["ISOVG220",null,null,null,null,-30,-39,220,150,0,"Synthétique",220,null,"Gearmaster PGP ","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG220",null,null,null,"1075 à 15°C",null,-36,240,null,0,"Synthétique",220,36.799999999999997,"Renolin PG","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\RENOLIN_PG.pdf"]
["ISOVG220",null,null,null,"890 à 15°C",null,-10,200,null,0,"Minérale",220,19,"Kluberoil GEM 1-series","KLÜBER","DOC HUILE\\KLUBER\\Kluberoil GEM 1-series.pdf"]
["ISOVG220",null,null,null,"1,04 g/cm3 à 20°C",null,-30,250,null,0,"Synthétique",220,38,"Syntheso D EP","KLÜBER","DOC HUILE\\KLUBER\\Syntheso D EP.pdf"]
["ISOVG220",null,null,null,"0,850 à 15°C",null,-45,240,null,0,"Synthétique",220,28.3,"Mobilgear SHC XMP","MOBIL","DOC HUILE\\MOBIL\\Mobilgear SHC XMP Series pds.pdf"]
["ISOVG220",null,null,null,null,null,-18,216,null,0,"Minérale",220,18.100000000000001,"Mobil gear 600 series  ","MOBIL","DOC HUILE\\MOBIL\\Mobilgear 600 Series pds.pdf"]
["ISOVG220",null,null,null,"0,9 à 15,6°C",null,-24,272,null,0,"Minérale",220,18.8,"Mobilgear XMP series","MOBIL","DOC HUILE\\MOBIL\\mobilgear_xmp_series.pdf"]
["ISOVG220",null,null,null,"1.077 à 15°C",null,-33,265,null,0,"Synthétique",220,38.1,"Glycoyle HE series","MOBIL","DOC HUILE\\MOBIL\\Glygoyle HE Series pds.pdf"]
["ISOVG220",null,null,null,"1,048 à 15°C",null,-35,275,null,0,"Synthétique",220,39,"Mobil glygoyle series","MOBIL","DOC HUILE\\MOBIL\\mobil_glygoyle_he_series.pdf"]
["ISOVG220",null,null,null,"0,87 à 15°C",null,-42,235,null,0,"Synthétique",216,25.2,"Mobil SHC 600 series","MOBIL","DOC HUILE\\MOBIL\\Mobil_SHC_600.pdf"]
["ISOVG220",null,null,null,"853 à 15°C",null,-48,240,null,0,"Synthétique",220,25.8,"Shell Omala HD","SHELL","DOC HUILE\\SHELL\\Shell Omala HD.pdf"]
["ISOVG220",null,null,null,"8895 à20°C",null,-18,200,null,0,"Minérale",220,19.399999999999999,"Shell Omala","SHELL","DOC HUILE\\SHELL\\Shell Omala.pdf"]
["ISOVG220",null,null,null,"0,899 à 15°C",null,-18,199,null,0,"Minérale",220,19.399999999999999,"Shell Omala F","SHELL","DOC HUILE\\SHELL\\Shell Omala F.pdf"]
["ISOVG220",null,null,null,null,null,-21,245,null,0,"Minérale",209,18.8,"Meropa","TEXACO","DOC HUILE\\TEXACO\\Meropa220.pdf"]
["ISOVG220",null,null,null,"0,893 à 15°C",null,-24,250,null,0,"Minérale",220,19.32,"Meropa WM ","TEXACO","DOC HUILE\\TEXACO\\Meropa WM  220.pdf"]
["ISOVG220",null,null,null,"859,7 à 15°C",null,-45,237,null,0,"Synthétique",220,26.2,"Carter SH","TOTAL ","DOC HUILE\\TOTAL\\Carter-SH.pdf"]
["ISOVG220",null,null,null,"0,893 à 15°C",null,-21,270,null,0,"Minérale",220,18.5,"Carter EP","TOTAL ","DOC HUILE\\TOTAL\\CARTER EP.pdf"]
["ISOVG220",null,null,null,"899 à 15°C",null,-21,226,null,0,"Minérale",220,19.02,"Kassilla GMP","TOTAL ","DOC HUILE\\TOTAL\\Kassilla GMP.pdf"]
["ISOVG220",null,null,null,"0,901 à 15°C",null,-18,215,null,0,"Minérale",198,17.3,"TITAN GEAR MP90","VOGELSANG  ","http://www.fuchs.com.au/ProductMsds.aspx?product_id=37078&ssid=0ysyhb1cef0ggun30fpmvep2"]
["ISOVG220",null,null,null,"1,006à15°C",null,-30,160,null,0,"Synthetic",219,30.2,"Glygoyle30","MOBIL","DOCHUILE\\MOBIL\\GlygoyleSeriespds.pdf"]
["ISOVG220",null,null,null,"0,86à15°C",null,-42,232,null,0,"Semi-synthetic",83,14,"ULTRON5W-40","ESSO","DOCHUILE\\ESSO\\esso__ultron_5w40.pdf"]
["ISOVG220",null,null,null,"0,909 à 15°C",-40,265,204,150,"1","LITHIUM COMPLEX","220",null,"MOBILITH SHC 221","MOBIL","DOC GRAISSE\\Mobil\\MOBILITH SHC serie.pdf"]
["ISOVG220",null,null,null,"0,896 à 15°C",-20,null,200,140,"00","LITHIUM COMPLEX","220",null,"MOBILGREASE XHP 005","MOBIL","DOC GRAISSE\\Mobil\\Mobilgrease XHP 005.pdf"]
["ISOVG220",null,null,null,"0,914 à 15°C",-20,null,200,140,"0","LITHIUM COMPLEX","220",null,"MOBILGREASE XHP 220","MOBIL","DOC GRAISSE\\Mobil\\mobilgrease_xhp_220_series.pdf"]
["ISOVG220",null,null,null,null,-10,null,null,140,"3","LITHIUM COMPLEX","220",null,"MOBILGREASE XHP 223","MOBIL"]
["ISOVG260","KP2R-20",null,null,null,-25,null,null,210,"2","ALUMINIUM COMPLEX","240",null,"ARALUB MKA 2","ARAL"]
["ISOVG280","KP2N-20",null,null,"0,88à15°C",-20,270,204,140,2,"Lithium complex",280,null,"Mobilgrease XHP 222","MOBIL","DOCGRAISSE\\Mobil\\Mobilgrease-XHP-222.pdf"]
["ISOVG280","KP2S-20",null,null,"0,89g/cm3à20°C",-20,220,200,140,2,"Lithium complex",280,20,"Microlube GL262","KLÜBER","DOCGRAISSE\\Klüber\\MicrolubeGL262_EN.pdf"]
["ISOVG280",null,null,null,"1,1 à 25°C",-40,null,101,204,"1","LITHIUM","280 à 25°C",null,"MOLYKOTE 44","DOW CORNING","DOC GRAISSE\\DOW CORNING\\TDS_MOLYKOTE_41_eng.pdf"]
["ISOVG3,2",null,null,null,"1,4 à 25°C",-40,null,101,232,"1","FLUOCARBONE","2,295",null,"MOLYKOTE 3451","DOW CORNING","DOC GRAISSE\\DOW CORNING\\dow_3451_tds.pdf"]
["ISOVG300",null,null,null,"0,93 g/cm3 à 20°C",-40,null,200,110,"00","LITHIUM-BISULFURE DE MOLYBDENE","300",null,"MOLYKOTE LONGTERM 00","DOW CORNING","DOC GRAISSE\\DOW CORNING\\MSDS_MOLYKOTE_Longterm_00_eng.pdf"]
["ISOVG32","DIN 51506_VD-L",null,null,"0,86 à 15°C",null,-24,224,null,0,"Synthétique",30,5.4,"Exxcolub","ESSO","http://mirsmazok.ru/catalog/auto-smazki/category38217/3410.html"]
["ISOVG32","DIN 51524-2",null,null,"0,88 g/cm3 à 20°C",-12,-18,200,120,0,"Minérale",32,5.4,"Lamora HLP","KLÜBER","DOC HUILE\\KLUBER\\LAMORA_HLP-en.pdf"]
["ISOVG32","DIN 51524-2",null,null,"0,872à15°",null,-30,207,null,0,"Minérale",32,5.4,"TellusS32","SHELL","DOCGRAISSE\\schell\\shell-tellus-oils-s-telluss.pdf"]
["ISOVG32","K0D-35",null,null,null,-35,null,290,90,0,"Minérale",33,null,"Eco-Hyd S","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\ECO_HYD_S_PLUS.pdf"]
["ISOVG32","KPHC1K-50",null,null,"0,952 à 15°C",-50,260,204,180,"1","CLAY","30","5,2","MOBILTEMP SHC 32","MOBIL","DOC GRAISSE\\Mobil\\MOBILTEMP SHC 32.pdf"]
["ISOVG32","KPHC2K-50",null,null,"0,952 à 15°C",-50,260,204,180,"2","CLAY","30","5,2","MOBILTEMP SHC 32","MOBIL","DOC GRAISSE\\Mobil\\MOBILTEMP SHC 32.pdf"]
["ISOVG32",null,null,null,"860 à 15°C",null,-33,220,null,0,"Minérale",32.799999999999997,5.7,"Oso - D ","AGIP","DOC HUILE\\AGIP\\Oso - D.pdf"]
["ISOVG32",null,null,null,"0,865 à 15°C",null,-36,202,null,0,"Minérale",32,6.4,"Arnica","AGIP","DOC HUILE\\AGIP\\Arnica.pdf"]
["ISOVG32",null,null,null,"0,875 à 15°C",null,-30,195,null,0,"Minérale",30,5.3,"Oso","AGIP","DOC HUILE\\AGIP\\oso.pdf"]
["ISOVG32",null,null,null,"872 à 15°C",null,-24,226,null,0,"Minérale",32,null,"Vitam DE ","ARAL","http://www.lubebase.com/cgi-bin/ctl/lube?id=5693"]
["ISOVG32",null,null,null,"871 à 15°C",null,-24,224,null,0,"Minérale",32,null,"Vitam GF ","ARAL","http://www.lubebase.com/cgi-bin/ctl/lube?id=5682"]
["ISOVG32",null,null,null,"32 à 40°C",null,-27,270,null,0,"Synthétique",null,null,"Hydrostar HEP","BECHEM","DOC HUILE\\BECHEM\\HYDROSTAR HEP.docx"]
["ISOVG32",null,null,null,"0,87 g/cm3 à 15°C",null,-36,220,null,0,"Minérale",32,5.5,"Staroil No. 32","BECHEM","DOC HUILE\\BECHEM\\Staroil No. 100.pdf"]
["ISOVG32",null,null,null,"877 à 15°C",null,-30,222,null,0,"Minérale",32,5.5,"Energol HLP-D ","BP","DOC HUILE\\BP\\Energol HLP-D.pdf"]
["ISOVG32",null,null,null,"0,88 à 15°C",null,-30,210,null,0,"Minérale",32,5.44,"Energol HLP-HM ","BP","DOC HUILE\\BP\\Energol HLP-HM.pdf"]
["ISOVG32",null,null,null,"0,88 à 15°C",null,-45,200,null,0,"Minérale",32,6.41,"Energol SHF-HV","BP","DOC HUILE\\BP\\Energol SHF-HV.pdf"]
["ISOVG32",null,null,null,"0,882 g/cm3 à 15°c",null,-24,185,null,0,"Minérale",32,null,"Fluid Drive HM","BRUGAROLAS","DOC HUILE\\BRUGAROLAS\\lubricantes-brugarolas_aceites_industriales.pdf"]
["ISOVG32",null,null,null,"0,909 g/cm3",null,-33,212,null,0,"Synthétique",35,7.5,"Tribol Bio Top 1448","CASTROL","DOC HUILE\\CASTROL\\tribol_biotop_1448.pdf"]
["ISOVG32",null,null,null,"870 à 15°C",null,-30,215,null,0,"Minérale",32,5.4,"Hyspin SP ","CASTROL","DOC HUILE\\CASTROL\\Hyspin SP.pdf"]
["ISOVG32",null,null,null,"854 à 15°C",null,-27,200,null,0,"Minérale",33,5.8,"Tribol 943 AW ","CASTROL","DOC HUILE\\CASTROL\\Tribol 943 AW.pdf"]
["ISOVG32",null,null,null,"870 à 15°C",null,-24,220,null,0,"Minérale",32,5.3,"HLPD-Oel ","ESSO","DOC HUILE\\ESSO\\HLPD-Oel.PDF"]
["ISOVG32",null,null,null,"921 à 15°C",null,-51,246,null,0,"Synthétique",32.4,7.1,"Plantohyd S","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\238_Planto Brochure.pdf"]
["ISOVG32",null,null,null,"868 à 15°C",null,-24,205,null,0,"Minérale",32,5.5,"Renolin B ","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\RENOLIN_B.pdf"]
["ISOVG32",null,null,null,"875 à 15°C",null,-30,210,null,0,"Minérale",32,5.4,"Renolin MR 10","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\RENOLIN_MR.pdf"]
["ISOVG32",null,null,null,"0,866 g/cm3 à 15°C",null,-12,236,null,0,"Minérale",32,5.4,"Mobil whiterex 400 series ","MOBIL","http://www.mobil.com/USA-English/Lubes/PDS/GLXXENINDMOMobil_Rarus_400.aspx"]
["ISOVG32",null,null,null,"0,874 à 15°C",null,-45,210,null,0,"Minérale",32,6.1,"Mobil DTE 10M series","MOBIL","DOC HUILE\\MOBIL\\Mobil_DTE_11M_OIl.pdf"]
["ISOVG32",null,null,null,"0,871 à 15,6°C",null,-27,220,null,0,"Minérale",31.5,5.29,"Mobil DTE 20 series","MOBIL","DOC HUILE\\MOBIL\\Mobil DTE 20 series.pdf"]
["ISOVG32",null,null,null,"0,872 à 15°C",null,-24,212,null,0,"Minérale",32,5.4,"Nuto H series","MOBIL","DOC HUILE\\MOBIL\\Nuto.pdf"]
["ISOVG32",null,null,null,"0,876 à 15°C",null,-48,208,null,0,"Minérale",32,6.39,"Univis N series ","MOBIL","DOC HUILE\\MOBIL\\Univis N Series.pdf"]
["ISOVG32",null,null,null,"0,85 à 15°C",null,-54,240,null,0,"Minérale",32.4,6.3,"Mobil SHC 600 series","MOBIL","DOC HUILE\\MOBIL\\Mobil_SHC_600.pdf"]
["ISOVG32",null,null,null,"865 à 15°C",null,-21,205,null,0,"Minérale",30.7,5.0999999999999996,"ONDINA 900 series","SHELL","DOC HUILE\\SHELL\\Univar_produktkatalog_SE_screen.pdf"]
["ISOVG32",null,null,null,"877 à 15°C",null,-24,223,null,0,"Synthétique",32,6,"Naturelle HF-E ","SHELL","DOC HUILE\\SHELL\\Univar_produktkatalog_SE_screen.pdf"]
["ISOVG32",null,null,null,"0,876 à 15°C",null,-48,208,null,0,"Minérale",32,6.39,"Tellus","SHELL","DOC HUILE\\SHELL\\Tellus.pdf"]
["ISOVG32",null,null,null,"886 à 15°C",null,-60,100,null,0,"Synthétique",33.6,9.89,"Tellus artic","SHELL","DOC HUILE\\SHELL\\Tellus artic.pdf"]
["ISOVG32",null,null,null,"868 à 15°C",null,-60,147,null,0,"Minérale",32,5.6,"Tellus DO","SHELL","DOC HUILE\\SHELL\\Tellus DO(TDS).pdf"]
["ISOVG32",null,null,null,"872 à 15°C",null,-39,210,null,0,"Minérale",32,6.1,"Tellus T","SHELL","DOC HUILE\\SHELL\\Tellus T.pdf"]
["ISOVG32",null,null,null,"0,915 à 15°C",null,-50,215,null,0,"Synthétique",32,7.4,"Hydra","TEXACO","DOC HUILE\\TEXACO\\hydra_pds.pdf"]
["ISOVG32",null,null,null,"0,874 à 15°C",null,-30,205,null,0,"Minérale",32,5.19,"Alcor DD ","TEXACO","http://texaco-oil.ru/catalog/category39101/11726.html"]
["ISOVG32",null,null,null,null,null,-33,220,null,0,"Minérale",30.4,5.2,"Rando HD","TEXACO","DOC HUILE\\TEXACO\\Rando HD.pdf"]
["ISOVG32",null,null,null,"875 à 15°C",null,-33,210,null,0,"Minérale",32.700000000000003,5.5,"Azolla DZF","TOTAL ","DOC HUILE\\TOTAL\\Azolla DZF.pdf"]
["ISOVG32",null,null,null,"875 à 15°C",null,-27,227,null,0,"Minérale",32,5.4,"Azolla ZS","TOTAL ","DOC HUILE\\TOTAL\\AZOLLA_ZS.pdf"]
["ISOVG32",null,null,null,"870 à 15°C",null,-39,208,null,0,"Minérale",32.299999999999997,6.5,"Equivis ZS","TOTAL ","DOC HUILE\\TOTAL\\EQUIVIS_ZS.pdf"]
["ISOVG320","DIN 51517",null,null,"0,89à15°C",null,-18,232,null,0,"hydrocarbure",320,23,"MobilGear 632","MOBIL","DOCHUILE\\MOBIL\\MOBILGear632.pdf"]
["ISOVG320","DIN 51517-3",null,null,null,-10,-18,235,130,0,"Minérale",320,null,"Staroil G ","BECHEM","DOC HUILE\\BECHEM\\STAROIL G.docx"]
["ISOVG320","DIN 51517-3",null,null,"892à15°C",null,-15,240,null,0,"Minérale",320,24,"SpartanEP320","ESSO","DOCHUILE\\ESSO\\SpartanEPseries.pdf"]
["ISOVG320","DIN 51517-3",null,null,"0,855g/cm3à15°C",-40,-40,240,145,0,"Synthetic",395,37,"KROILSINTOLUBE320","KRAFFT","DOCHUILE\\KRAFFT\\49067.pdf"]
["ISOVG320","GP000G-20",null,null,"0,908 à 15°C",-20,null,200,100,"000","LITHIUM","320",null,"MOBILUX EP 023","MOBIL","http://www.mobil.com/Australia-English/Lubes/PDS/GLXXENGRSMOMobilux_EP.aspx"]
["ISOVG320","K0G-0",null,null,null,0,-12,220,105,0,"Minérale",320,22.5,"Beslux Gear XP ","BRUGAROLAS","DOC HUILE\\BRUGAROLAS\\lubricantes-brugarolas_aceites_industriales.pdf"]
["ISOVG320","K0K-15",null,null,null,-15,-21,null,120,0,"Minérale",320,null,"Gearmaster CLP","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG320","K0N-20",null,null,null,-20,-33,null,150,0,"Synthétique",320,null,"Gearmaster SYN","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG320","K0N-30",null,null,null,-30,-39,null,150,0,"Synthétique",320,null,"Gearmaster PGP ","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG320","K1N-50",null,null,"0,97à20°C",-50,220,null,150,0,"Lithium/Lithium complex",360,55,"SynthesoGLEP","KLÜBER","DOCGRAISSE\\Klüber\\Syntheso_GLEP_1.pdf"]
["ISOVG320","KP0N-20",null,null,null,-20,270,246,140,"0","LITHIUM COMPLEX","320",null,"MOBILGREASE XHP 320 MINE","MOBIL","DOC GRAISSE\\Mobil\\mobilgrease-xhp-mine-series.pdf"]
["ISOVG320","KP1N-20",null,null,null,-20,270,246,140,"1","LITHIUM COMPLEX","320",null,"MOBILGREASE XHP 321 MINE","MOBIL","DOC GRAISSE\\Mobil\\mobilgrease-xhp-mine-series.pdf"]
["ISOVG320","KP2N-20",null,null,"0,911 à 15°C",-20,270,246,140,"2","LITHIUM COMPLEX","320",null,"MOBILGREASE XHP 322 MINE","MOBIL","DOC GRAISSE\\Mobil\\mobilgrease-xhp-mine-series.pdf"]
["ISOVG320",null,null,null,"1,06 à 15°C",null,-36,250,null,0,"Synthétique",330,60,"Telium VSF","AGIP","DOC HUILE\\AGIP\\Agip Telium VSF 320.pdf"]
["ISOVG320",null,null,null,"0,901 g/cm3 à 15°C",null,-9,298,null,0,"Minérale",null,null,"Degol BG","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG320",null,null,null,"0,895 g/cm3 à 15°C",null,-15,250,null,0,"Minérale",null,null,"Degol BG Plus","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG320",null,null,null,"0,885 g/cm3 à 15°C",null,-48,192,null,0,"Synthétique",null,null,"Degol PAS ","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG320",null,null,null,"1 g/cm3 à 15°C",null,-42,280,null,0,"Synthétique",null,null,"Degol GS","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG320",null,null,null,null,null,null,null,null,0,"Minérale",320,null,"Eco Gear M","BECHEM"]
["ISOVG320",null,null,null,null,null,null,null,null,0,"Synthétique",320,null,"Eco Gear S","BECHEM"]
["ISOVG320",null,null,null,"1,02 g/cm3 à 15°C",null,-33,278,null,0,"Synthétique",326,50,"Berusynth EP ","BECHEM","DOC HUILE\\BECHEM\\BECHEM Berusynth EP_68_1000_9590019(GB).pdf"]
["ISOVG320",null,null,null,"912 à 15°C",null,-15,243,null,0,"Minérale",205,22.7,"Energol GR-XF ","BP","DOC HUILE\\BP\\ENERGOL GR-XF.pdf"]
["ISOVG320",null,null,null,"912 à 15°C",null,-15,243,null,0,"Minérale",320,25,"Energol GR-XP","BP","DOC HUILE\\BP\\ENERGOL GR-XP.pdf"]
["ISOVG320",null,null,null,"0,86 g/cm3 à 15°C",null,-36,230,null,0,"Synthétique",320,33,"Enersyn EP-XF ","BP","DOC HUILE\\BP\\Enersyn EP-XF.pdf"]
["ISOVG320",null,null,null,"1,02 à 15°C",null,-36,280,null,0,"Synthétique",320,null,"Enersyn SG-XP ","BP","DOC HUILE\\BP\\Enersyn SG-XP.pdf"]
["ISOVG320",null,null,null,"0,86 à 15°C",null,-36,230,null,0,"Synthétique",320,33,"Alphasyn EP ","CASTROL","DOC HUILE\\CASTROL\\Alphasyn EP.pdf"]
["ISOVG320",null,null,null,"0,9 à 15°C",null,-15,226,null,0,"Minérale",320,24,"Alpha SP","CASTROL","DOC HUILE\\CASTROL\\Alpha SP.pdf"]
["ISOVG320",null,null,null,"875 à 15°C",null,-30,240,null,0,"Synthétique",320,31.2,"Tribol 1710","CASTROL","DOC HUILE\\CASTROL\\Tribol 1710 .pdf"]
["ISOVG320",null,null,null,"908 à 15°C",null,-21,247,null,0,"Minérale",320,23.6,"Tribol 1100","CASTROL","DOC HUILE\\CASTROL\\Tribol 1100.pdf"]
["ISOVG320",null,null,null,"1,06 à 15°C",null,-36,210,null,0,"Synthétique",320,56,"Alphasyn PG","CASTROL","DOC HUILE\\CASTROL\\Alphasyn PG.pdf"]
["ISOVG320",null,null,null,"1074 à 15°C",null,-30,290,null,0,"Synthétique",320,72,"Tribol 800","CASTROL","DOC HUILE\\CASTROL\\Tribol 800 .pdf"]
["ISOVG320",null,null,null,"892 à 15°C",null,-15,240,null,0,"Minérale",320,24,"Spartan EP series","ESSO","DOC HUILE\\ESSO\\Spartan EP series.pdf"]
["ISOVG320",null,null,null,"860 à 15°C",null,-42,260,null,0,"Synthétique",320,35,"Renolin Unisyn CLP series","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\RENOLIN_UNISYN_CLP.pdf"]
["ISOVG320",null,null,null,"900 à 15°C",null,-14,255,null,0,"Minérale",320,24,"Renolin CLP","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\Renolin CLP.pdf"]
["ISOVG320",null,null,null,null,null,null,null,null,0,"Minérale",320,null,"Renolin CLP Plus","FUCHS EUROPE"]
["ISOVG320",null,null,null,"1075 à 15°C",null,-39,240,null,0,"Synthétique",320,54.4,"Renolin PG","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\RENOLIN_PG.pdf"]
["ISOVG320",null,null,null,"1,05 g/cm3 à 20°C",null,-30,200,null,0,"Synthétique",320,60,"Syntheso D EP","KLÜBER","DOC HUILE\\KLUBER\\Syntheso D EP.pdf"]
["ISOVG320",null,null,null,"0,86 à 15°C",null,-39,240,null,0,"Synthétique",320,37.4,"Mobilgear SHC XMP","MOBIL","DOC HUILE\\MOBIL\\Mobilgear SHC XMP Series pds.pdf"]
["ISOVG320",null,null,null,"1,050 à 15°C",null,-42,290,null,0,"Synthétique",320,54.6,"Glycoyle HE series","MOBIL","DOC HUILE\\MOBIL\\Glygoyle HE Series pds.pdf"]
["ISOVG320",null,null,null,"0,87 à 15°C",null,-39,250,null,0,"Minérale",326,38.6,"Mobil SHC 600 series","MOBIL","DOC HUILE\\MOBIL\\Mobil_SHC_600.pdf"]
["ISOVG320",null,null,null,"0,903 à 15,6°C",null,-18,268,null,0,"Minérale",320,24.1,"Mobilgear XMP series","MOBIL","DOC HUILE\\MOBIL\\mobilgear_xmp_series.pdf"]
["ISOVG320",null,null,null,"1,077 à 15°C",null,-33,265,null,0,"Synthétique",320,55.2,"Mobil glygoyle series","MOBIL","http://www.mobil.com/USA-English/Lubes/PDS/GLXXENINDMOMobil_Glygoyle.aspx"]
["ISOVG320",null,null,null,"855 à 15°C",null,-45,245,null,0,"Synthétique",320,33.4,"Shell Omala HD ","SHELL","DOC HUILE\\SHELL\\Shell Omala HD.pdf"]
["ISOVG320",null,null,null,"892,4 à 20°C",null,-15,205,null,0,"Minérale",320,25,"Shell Omala","SHELL","DOC HUILE\\SHELL\\Shell Omala.pdf"]
["ISOVG320",null,null,null,"0,903 à 15°C",null,-18,202,null,0,"Minérale",320,25,"Shell Omala F","SHELL","DOC HUILE\\SHELL\\Shell Omala F.pdf"]
["ISOVG320",null,null,null,"1,069 à 15°C",null,-37,285,null,0,"Synthétique",320,52.7,"Tivela fluid S","SHELL","DOC HUILE\\SHELL\\TivelaS.pdf"]
["ISOVG320",null,null,null,"0,895 à 15°C",null,-15,250,null,0,"Minérale",320,24.3,"Meropa","TEXACO","DOC HUILE\\TEXACO\\Meropa 320.pdf"]
["ISOVG320",null,null,null,"0,895 à 15°C",null,-18,250,null,0,"Minérale",320,24.4,"Meropa WM ","TEXACO","DOC HUILE\\TEXACO\\Meropa_WM_320.pdf"]
["ISOVG320",null,null,null,"861,7 à 15°C",null,-42,null,null,0,"Synthétique",320,34.6,"Carter SH","TOTAL ","DOC HUILE\\TOTAL\\Carter-SH.pdf"]
["ISOVG320",null,null,null,"0,899 à 15°C",null,-21,270,null,0,"Minérale",320,23.7,"Carter EP","TOTAL ","DOC HUILE\\TOTAL\\CARTER EP.pdf"]
["ISOVG320",null,null,null,"904 à 15°C",null,-18,226,null,0,"Minérale",320,null,"Kassilla GMP","TOTAL ","DOC HUILE\\TOTAL\\Kassilla GMP.pdf"]
["ISOVG320",null,null,null,"1,05 à 25°C",-18,null,302,288,"2","CARBONE","316 à 25°C",null,"MOLYKOTE 41","DOW CORNING","DOC GRAISSE\\DOW CORNING\\TDS_MOLYKOTE_41_eng.pdf"]
["ISOVG4000",null,null,null,"0,91 à 15°C",-10,177,150,35,"00-0","LITHIUM","4000",null,"MOBIL DYNAGEAR 4000","MOBIL","DOC GRAISSE\\Mobil\\mobil_dynagear_4000.pdf"]
["ISOVG46","DIN 51515",null,null,"846à15°C",null,-15,218,null,null,null,46,7.6,"RENOLINETERNA46","FUCHS","DOCHUILE\\FUCHSEUROPE\\RENOLIN_ETERNA.pdf"]
["ISOVG46","K0H-20",null,null,"0,885 g/cm3 à 15°C",-20,-24,190,110,0,"Minérale",46,null,"Fluid Drive HM","BRUGAROLAS","DOC HUILE\\BRUGAROLAS\\lubricantes-brugarolas_aceites_industriales.pdf"]
["ISOVG46","K0K-12",null,null,"0,87 g/cm3 à 20°C",-12,-15,null,120,0,"Minérale",46,null,"Lamora HLP","KLÜBER","http://www.lubebase.com/cgi-bin/ctl/lube/Kluber-LAMORA-HLP-46?id=8321"]
["ISOVG46","K0K-20",null,null,"945 à 15°C",-20,-48,241,120,0,"Synthétique",46,8.6999999999999993,"Biohydran SE 46","TOTAL ","DOC HUILE\\TOTAL\\BIOHYDRAN_SE_32-46-68_ENG.pdf"]
["ISOVG46","K0K-20",null,null,"1000 à 15°C",-20,180,150,120,"0","Lithium/Lithium complex",41.4,null,"CLSGrease","CASTROL","DOCGRAISSE\\castrol\\CLSGrease.pdf"]
["ISOVG46","K1S-20",null,null,"1,43g/cm3à20°C",-40,null,200,1000,1,"Polyglycol+pétrole d'ester",42,10,"HEL46-450","KLÜBER","DOCGRAISSE\\Klüber\\HEL_46_450-en.pdf"]
["ISOVG46",null,null,null,"921 à 15°C",null,-36,370,null,0,"Synthétique",48,9.3000000000000007,"Arnica S ","AGIP","DOC HUILE\\AGIP\\Arnica S.pdf"]
["ISOVG46",null,null,null,"863 à 15°C",null,-30,235,null,0,"Minérale",45.5,7.1,"Oso - D ","AGIP","DOC HUILE\\AGIP\\Oso - D.pdf"]
["ISOVG46",null,null,null,"0,880 à 15°C",null,-27,212,null,0,"Minérale",45,6.8,"Oso","AGIP","DOC HUILE\\AGIP\\oso.pdf"]
["ISOVG46",null,null,null,"923 à 15°C",null,-36,280,null,0,"Synthétique",46,null,"Vitam EHF ","ARAL","http://www.lubebase.com"]
["ISOVG46",null,null,null,"878 à 15°C",null,-24,232,null,0,"Minérale",46,null,"Vitam DE ","ARAL","http://www.lubebase.com"]
["ISOVG46",null,null,null,"877 à 15°C",null,-24,244,null,0,"Minérale",46,null,"Vitam GF ","ARAL","http://www.lubebase.com"]
["ISOVG46",null,null,null,null,null,-36,270,null,0,"Synthétique",46,null,"Hydrostar HEP ","BECHEM","DOC HUILE\\BECHEM\\HYDROSTAR HEP.docx"]
["ISOVG46",null,null,null,null,null,-33,220,null,0,"Minérale",46,null,"Hydrostar D","BECHEM","DOC HUILE\\BECHEM\\BECHEM Hydrostar 46 D.docx"]
["ISOVG46",null,null,null,"0,87 g/cm3 à 15°C",null,-15,250,null,0,"Minérale",46,6.7,"Staroil No. 46","BECHEM","DOC HUILE\\BECHEM\\STAROIL G.docx"]
["ISOVG46",null,null,null,"878 à 15°C",null,-24,225,null,0,"Minérale",46,6.8,"Energol HLP-D ","BP","DOC HUILE\\BP\\Energol HLP-D.pdf"]
["ISOVG46",null,null,null,"0,88 à 15°C",null,-24,215,null,0,"Minérale",46,6.82,"Energol HLP-HM ","BP","DOC HUILE\\BP\\Energol HLP-HM.pdf"]
["ISOVG46",null,null,null,"0,88 à 15°C",null,-42,220,null,0,"Minérale",46,8.32,"Energol SHF-HV","BP","DOC HUILE\\BP\\Energol SHF-HV.pdf"]
["ISOVG46",null,null,null,"0,92 à 20°C",null,-27,270,null,0,"Synthétique",46,9.1199999999999992,"Carelube HES 46","CASTROL","DOC HUILE\\CASTROL\\Carelube HES 46.pdf"]
["ISOVG46",null,null,null,"913 à 15°C",null,-39,212,null,0,"Synthétique",47,9.6,"Tribol Bio Top 1448","CASTROL","DOC HUILE\\CASTROL\\Tribol Bio Top 1448.pdf"]
["ISOVG46",null,null,null,"0,875 à 20°C",null,-21,220,null,0,"Minérale",46,6.65,"Hyspin AWS","CASTROL","DOC HUILE\\CASTROL\\Hyspin AWS.pdf"]
["ISOVG46",null,null,null,"880 à 15°C",null,-30,240,null,0,"Minérale",46,6.8,"Hyspin SP ","CASTROL","DOC HUILE\\CASTROL\\Hyspin SP.pdf"]
["ISOVG46",null,null,null,"855 à 15°C",null,-30,270,null,0,"Minérale",48,7.3,"Tribol 943 AW ","CASTROL","DOC HUILE\\CASTROL\\Tribol 943 AW.pdf"]
["ISOVG46",null,null,null,"880 à 15°C",null,-24,220,null,0,"Minérale",46,6.5,"HLPD-Oel ","ESSO","DOC HUILE\\ESSO\\HLPD-Oel.PDF"]
["ISOVG46",null,null,null,"0,876 à 15°C",null,-24,226,null,0,"Minérale",46,6.7,"NUTO series","ESSO","DOC HUILE\\ESSO\\NUTO series.pdf"]
["ISOVG46",null,null,null,"912 à 15°C",null,-36,230,null,0,"Minérale",45.7,8.1999999999999993,"Eco-Hyd S","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\ECO_HYD_S_PLUS.pdf"]
["ISOVG46",null,null,null,"921 à 15°C",null,-42,304,null,0,"Synthétique",48.8,9.6,"Plantohyd S","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\238_Planto Brochure.pdf"]
["ISOVG46",null,null,null,"870 à 15°C",null,-24,210,null,0,"Minérale",46,6.9,"Renolin B ","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\RENOLIN_B.pdf"]
["ISOVG46",null,null,null,"877 à 15°C",null,-27,220,null,0,"Minérale",46,6.9,"Renolin MR 15","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\RENOLIN MR.pdf"]
["ISOVG46",null,null,null,"0,92 g/cm3 à 20°C",null,-30,310,null,0,"Synthétique",49.5,null,"EAL Hydraulic 46","MOBIL","DOC HUILE\\MOBIL\\mobil-eal-hydraulic-oil-46-424.pdf"]
["ISOVG46",null,null,null,"0,879 à 15°°C",null,-42,216,null,0,"Minérale",46,7.86,"Mobil DTE 10M series","MOBIL","DOC HUILE\\MOBIL\\Mobil_DTE_11M_OIl.pdf"]
["ISOVG46",null,null,null,"0,876 à 15,6°C",null,-27,232,null,0,"Minérale",44.2,6.65,"Mobil DTE 20 series","MOBIL","DOC HUILE\\MOBIL\\Mobil DTE 20 series.pdf"]
["ISOVG46",null,null,null,"0,876 à 15°C",null,-24,226,null,0,"Minérale",46,6.7,"Nuto H series","MOBIL","DOC HUILE\\MOBIL\\Nuto.pdf"]
["ISOVG46",null,null,null,"921 à 15°C",null,-42,322,null,0,"Synthétique",47.2,9.41,"Naturelle HF-E ","SHELL","http://www.lubebase.com/cgi-bin/ctl/lube?id=6435"]
["ISOVG46",null,null,null,"0,879 à 15°°C",null,-30,218,null,0,"Minérale",46,6.7,"Tellus","SHELL","DOC HUILE\\SHELL\\Tellus.pdf"]
["ISOVG46",null,null,null,"877 à 15°C",null,-24,223,null,0,"Minérale",46,7,"Tellus DO","SHELL","DOC HUILE\\SHELL\\Tellus DO(TDS).pdf"]
["ISOVG46",null,null,null,"872 à 15°C",null,-39,225,null,0,"Minérale",46,7.9,"Tellus T","SHELL","DOC HUILE\\SHELL\\Tellus T.pdf"]
["ISOVG46",null,null,null,"0,922 à 15°C",null,-45,252,null,0,"Synthétique",46,9.3000000000000007,"Hydra","TEXACO","DOC HUILE\\TEXACO\\hydra_pds.pdf"]
["ISOVG46",null,null,null,"876 à 15°C",null,-33,238,null,0,"Minérale",46,6.98,"Alcor DD ","TEXACO","http://www.lubebase.com/cgi-bin/ctl/lube?id=3078"]
["ISOVG46",null,null,null,null,null,-30,226,null,0,"Minérale",46,6.5,"Rando HD","TEXACO","DOC HUILE\\TEXACO\\Rando HD.pdf"]
["ISOVG46",null,null,null,"880 à 15°C",null,-33,215,null,0,"Minérale",46.4,6.9,"Azolla DZF","TOTAL ","DOC HUILE\\TOTAL\\Azolla DZF.pdf"]
["ISOVG46",null,null,null,"881 à 15°C",null,-27,232,null,0,"Minérale",45.9,6.8,"Azolla ZS","TOTAL ","DOC HUILE\\TOTAL\\AZOLLA_ZS.pdf"]
["ISOVG46",null,null,null,"874 à 15°C",null,-39,215,null,0,"Minérale",46,8.4,"Equivis ZS","TOTAL ","DOC HUILE\\TOTAL\\EQUIVIS_ZS.pdf"]
["ISOVG46",null,null,null,"922 à 15°C",null,-36,306,null,0,"Synthétique",44,9.6,"PLANTIHYD 40N","VOGELSANG  ","DOC HUILE\\VOGELSANG\\PI_PLANTOHYD-40-N_e.pdf"]
["ISOVG46",null,null,null,"870 à 15°C",null,-24,210,null,0,"Minérale",46,6.9,"RENOLIN B15","VOGELSANG  ","DOC HUILE\\FUCHS EUROPE\\RENOLIN_B.pdf"]
["ISOVG46",null,null,null,"879 à 15°C",null,-30,218,null,0,"Minérale",46,null,"ROTAIR 2000","WORTHINGTON ","DOC HUILE\\WORTHINGTON\\Worthington Creyssensac - Rotair 2000 - GB_en.pdf"]
["ISOVG46",null,null,null,"842à15°C",null,-60,230,null,0,"Synthetic",46,7.9,"Rotor-Xtenddutyfluid","ATLASCOPCO","DOCHUILE\\ATLAS\\Product_Catalogue.pdf"]
["ISOVG46",null,null,null,"1,4 à 25°C",-29,null,101,232,"2","FLUOCARBONE","46",null,"MOLYKOTE 3452","DOW CORNING","DOC GRAISSE\\DOW CORNING\\dow_3451_tds.pdf"]
["ISOVG460"," KPF2P-20",null,null,"0,87 à 15°C",-20,270,93,170,"2","POLYUREA","460","40","MOBIL SHC POLYREX 462","MOBIL","DOC GRAISSE\\Mobil\\mobil_shc_polyrex_series.pdf"]
["ISOVG460"," KPHC2N-40",null,null,"0,874 g/cm3 à 15°C",-40,-27,220,150,"2","LITHIUM COMPLEX","460","46,6","MOBILITH SHC PM 460","MOBIL","DOC GRAISSE\\Mobil\\ss_mobilith_shc_pm.pdf"]
["ISOVG460","DIN 51517-3",null,null,"0,89à15°C",null,-12,275,null,0,"Hydrocarbure",460,29.9,"Mobilgear 634","MOBIL","DOCHUILE\\MOBIL\\MOBILGear632.pdf"]
["ISOVG460","DIN 51519",null,null,"1074à15°C",-25,-25,250,160,0,"Polyglycol",460,71,"Klübersynth-GH6-460","KLÜBER","DOCHUILE\\KLUBER\\KlubersynthGH6.pdf"]
["ISOVG460","DIN 51519",null,null,"1,05 à 20°C",-35,-40,290,150,0,"PolyAlkylene Glycol",460,75,"SynthesoHT460","KLÜBER","DOCHUILE\\KLUBER\\SYNTHESOHT68-T-012010pp.pdf"]
["ISOVG460","GPHC00K-30",null,null,"0,866 à 15°C",-50,null,204,150,"00","LITHIUM COMPLEX","460","46,5","MOBILITH SHC 007","MOBIL","DOC GRAISSE\\Mobil\\MOBILITH SHC serie.pdf"]
["ISOVG460","K00K-20",null,null,"1,076à15°C",-20,-33,265,120,0,"Polyalkylène glycol",460,77.2,"Glygoyle","MOBIL","DOCHUILE\\MOBIL\\gygoyle460.pdf"]
["ISOVG460","K0H-35",null,null,null,-35,-18,302,110,0,"Minérale",460,null,"Staroil G ","BECHEM","DOC HUILE\\BECHEM\\STAROIL G.docx"]
["ISOVG460","K0K-10",null,null,null,-10,-15,230,120,0,"Minérale",460,null,"Gearmaster CLP","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG460","K0K-20",null,null,"0,9g/cm3à20°C",-20,180,285,120,0,"Lithium/Lithium complex",400,25,"MicrolubeGB0","KLÜBER","DOCGRAISSE\\Klüber\\klueberMicrolube_gb0_en.pdf"]
["ISOVG460","K0KN-30",null,null,null,-30,-39,290,150,0,"Minérale",460,null,"Gearmaster PGP ","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG460","K0N-20",null,null,null,-20,-33,280,150,0,"Synthétique",460,null,"Gearmaster SYN","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG460","K0P-25",null,null,"1074à15°C",-25,-25,250,160,0,"Polyglycol",460,71,"KlübersynthGH6-460","KLÜBER","DOCHUILE\\KLUBER\\KlubersynthGH6.pdf"]
["ISOVG460","K1K-15",null,null,"1,07g/cm3à20°C",-15,220,250,120,1,"Minérale",500,null,"Grafloscon","KLÜBER","DOCGRAISSE\\Klüber\\Grafloscon_A_G_1_ULTRA.pdf"]
["ISOVG460","K1N-10",null,null,"0,86g/cm3à20°C",-10,190,300,140,"2/3","Minérale",500,31,"BE31-502","KLÜBER","DOC GRAISSE\\Klüber\\BE 31-502.pdf"]
["ISOVG460","KFK2U-40",null,null,"1,90 à 20°C",-40,null,null,260,2,"Synthetic",400,38,"LGET2","SKF","DOCGRAISSE\\SKF\\12046EN_LGET2.pdf"]
["ISOVG460","KP00K-20",null,null,"1,02 à 15°C",-20,200,204,120,"00-0","LITHIUM","460","30","MOBILGEAR OGL 007","MOBIL","DOC GRAISSE\\Mobil\\Mobil-Gear-OGL-007.pdf"]
["ISOVG460","KP0-20",null,null,null,-20,200,null,120,"1-2","LITHIUM","460",null,"MOBILGEAR OGL 461","MOBIL"]
["ISOVG460","KP1N-20L",null,null,"0,9 à 15°C",-20,null,294,140,"1","LITHIUM COMPLEX","460","16","MOBILGREASE XHP 461","MOBIL","DOC GRAISSE\\Mobil\\MOBILGREASE_XHP_461.PDF"]
["ISOVG460","KP1Q0",null,null,null,0,300,null,170,"1","CLAY","460","31,7","MOBILTEMP 1","MOBIL","DOC GRAISSE\\Mobil\\mobiltemp_serie_pds_2013.pdf"]
["ISOVG460","KP1Q0",null,null,null,0,300,null,170,"1","CLAY","460","31,7","MOBILTEMP 78","MOBIL","DOC GRAISSE\\Mobil\\mobiltemp_serie_pds_2013.pdf"]
["ISOVG460","KP2N-20L",null,null,"0,9 à 15°C",-20,null,294,140,"2","LITHIUM COMPLEX","460","15","MOBILGREASE XHP 462","MOBIL","http://www.mobil.com/USA-English/Lubes/PDS/GLXXENGRSMOMobilgrease_XHP_460.aspx"]
["ISOVG460","KP2Q0",null,null,null,0,300,null,170,"2","CLAY","460","31,7","MOBILTEMP 2","MOBIL","DOC GRAISSE\\Mobil\\mobiltemp_serie_pds_2013.pdf"]
["ISOVG460","KPHC1-2N-40",null,null,"0,9 à 15°C",-40,265,204,150,2,"Lithium",460,47,"Mobilith SHC 460","MOBIL","DOCGRAISSE\\Mobil\\MobilithSHC460.pdf"]
["ISOVG460","KPHC1-2N-40",null,null,"1 à 15°C",-40,275,204,150,1.5,"Lithium",460,46.5,"Mobil SHC PM 460","MOBIL","DOCGRAISSE\\Mobil\\MobilithSHC460.pdf"]
["ISOVG460","KPHC1N-40",null,null,"0,9 à 15°C",-40,null,204,140,"1","LITHIUM COMPLEX","460","47","MOBIL SHC GREASE 460 WT","MOBIL","DOC GRAISSE\\Mobil\\MOBIL_Product_Summary_Juni_2013.pdf"]
["ISOVG460","KPHC1N-40",null,null,"1 à 15°C",-40,265,204,150,"1","LITHIUM COMPLEX","460",null,"MOBILITH SHC 460","MOBIL","DOC GRAISSE\\Mobil\\MOBILITH SHC serie.pdf"]
["ISOVG460","KPHC2N-40",null,null,"0,9 à 15°C",-40,null,204,140,"2","LITHIUM COMPLEX","460","47","MOBIL SHC GREASE 460 WT","MOBIL","DOC GRAISSE\\Mobil\\MOBIL_Product_Summary_Juni_2013.pdf"]
["ISOVG460","KPHC2N-40",null,null,"1 à 15°C",-40,265,204,150,"2","LITHIUM COMPLEX","460",null,"MOBILITH SHC 460","MOBIL","DOC GRAISSE\\Mobil\\MOBILITH SHC serie.pdf"]
["ISOVG460",null,null,null,"0,905 g/cm3 à 15°C",null,-18,300,null,0,"Minérale",460,null,"Degol BG","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG460",null,null,null,"0,902 g/cm3 à 15°C",null,-9,255,null,0,"Minérale",460,null,"Degol BG Plus","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG460",null,null,null,"0,893 g/cm3 à 15°C",null,-39,220,null,0,"Synthétique",460,null,"Degol PAS ","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG460",null,null,null,"1 g/cm3 à 15°C",null,-39,285,null,0,"Synthétique",460,null,"Degol GS","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG460",null,null,null,null,null,null,null,null,0,"Minérale",460,null,"Eco Gear M","BECHEM"]
["ISOVG460",null,null,null,null,null,null,null,null,0,"Synthétique",460,null,"Eco Gear S","BECHEM"]
["ISOVG460",null,null,null,"1,01 g/cm3 à 15°C",null,-33,294,null,0,"Synthétique",464,73,"Berusynth EP ","BECHEM","DOC HUILE\\BECHEM\\BECHEM Berusynth EP_68_1000_9590019(GB).pdf"]
["ISOVG460",null,null,null,"919 à 15°C",null,-9,243,null,0,"Minérale",460,27.2,"Energol GR-XF ","BP","DOC HUILE\\BP\\ENERGOL GR-XF.pdf"]
["ISOVG460",null,null,null,"919 à 15°C",null,-9,243,null,0,"Minérale",425,27.2,"Energol GR-XP","BP","DOC HUILE\\BP\\ENERGOL GR-XP.pdf"]
["ISOVG460",null,null,null,"1,02 à 15°C",null,-39,280,null,0,"Synthétique",460,null,"Enersyn SG-XP ","BP","DOC HUILE\\BP\\Enersyn SG-XP.pdf"]
["ISOVG460",null,null,null,null,null,-9,220,null,0,"Minérale",460,28.7,"Beslux Gear XP ","BRUGAROLAS","DOC HUILE\\BRUGAROLAS\\lubricantes-brugarolas_aceites_industriales.pdf"]
["ISOVG460",null,null,null,"0,9 à 15°C",null,-12,225,null,0,"Minérale",460,30.5,"Alpha SP","CASTROL","DOC HUILE\\CASTROL\\Alpha SP.pdf"]
["ISOVG460",null,null,null,"874 à 15°C",null,-30,240,null,0,"Synthétique",460,42.4,"Tribol 1710","CASTROL","DOC HUILE\\CASTROL\\Tribol 1710 .pdf"]
["ISOVG460",null,null,null,"916 à 15°C",null,-21,248,null,0,"Minérale",464,29.9,"Tribol 1100","CASTROL","DOC HUILE\\CASTROL\\Tribol 1100.pdf"]
["ISOVG460",null,null,null,"1075 à 15°C",null,-30,290,null,0,"Synthétique",460,72,"Tribol 800","CASTROL","DOC HUILE\\CASTROL\\Tribol 800 .pdf"]
["ISOVG460",null,null,null,"895 à 15°C",null,-15,240,null,0,"Minérale",460,30.4,"Spartan EP series","ESSO","DOC HUILE\\ESSO\\Spartan EP series.pdf"]
["ISOVG460",null,null,null,"1007 à 15°C",null,-28,270,null,0,"Synthétique",460,64.7,"Glycolube","ESSO","DOC HUILE\\ESSO\\Esso Glycolube 220, 460.doc"]
["ISOVG460",null,null,null,"856 à 15°C",null,-39,300,null,0,"Synthétique",460,45.6,"Renolin Unisyn CLP series","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\RENOLIN_UNISYN_CLP.pdf"]
["ISOVG460",null,null,null,"901 à 15°C",null,-10,270,null,0,"Minérale",460,30.4,"Renolin CLP","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\Renolin CLP.pdf"]
["ISOVG460",null,null,null,"1075 à 15°C",null,-33,280,null,0,"Synthétique",460,75.099999999999994,"Renolin PG","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\RENOLIN_PG.pdf"]
["ISOVG460",null,null,null,"1,05 g/cm3 à 20°C",null,-30,250,null,0,"Synthétique",460,75,"Syntheso D EP","KLÜBER","DOC HUILE\\KLUBER\\Syntheso D EP.pdf"]
["ISOVG460",null,null,null,"910 à 15°C",null,-10,200,null,0,"Synthétique",460,30,"Klübersynth GEM-4 series","KLÜBER","DOC HUILE\\KLUBER\\Kluberoil GEM 1-series.pdf"]
["ISOVG460",null,null,null,"0,863 à 15°C",null,-36,240,null,0,"Synthétique",460,48.5,"Mobilgear SHC XMP","MOBIL","DOC HUILE\\MOBIL\\Mobilgear SHC XMP Series pds.pdf"]
["ISOVG460",null,null,null,"1,050 à 15°C",null,-40,275,null,0,"Synthétique",460,77.099999999999994,"Glycoyle HE series","MOBIL","DOC HUILE\\MOBIL\\Glygoyle HE Series pds.pdf"]
["ISOVG460",null,null,null,"0,909 à 15°C",null,-12,270,null,0,"Synthétique",460,30.6,"Mobilgear XMP series","MOBIL","DOC HUILE\\MOBIL\\mobilgear_xmp_series.pdf"]
["ISOVG460",null,null,null,"0,87 à 15°C",null,-42,262,null,0,"Minérale",460,48.5,"Mobil SHC 600 series","MOBIL","DOC HUILE\\MOBIL\\Mobil_SHC_600.pdf"]
["ISOVG460",null,null,null,"857 à 15°C",null,-42,245,null,0,"Synthétique",460,45.5,"Shell Omala HD ","SHELL","DOC HUILE\\SHELL\\Shell Omala HD.pdf"]
["ISOVG460",null,null,null,"894,9 à 20°C",null,-12,205,null,0,"Synthétique",460,30.8,"Shell Omala","SHELL","DOC HUILE\\SHELL\\Shell Omala.pdf"]
["ISOVG460",null,null,null,"1,072 à15°C",null,-30,585,null,0,"Minérale",460,73.2,"Tivela fluid S","SHELL","DOC HUILE\\SHELL\\TivelaS.pdf"]
["ISOVG460",null,null,null,"0,903 à 15°C",null,-9,204,null,0,"Synthétique",460,30.8,"Shell Omala F","SHELL","DOC HUILE\\SHELL\\Shell Omala F.pdf"]
["ISOVG460",null,null,null,"0,9 à 15,6°C",null,-15,245,null,0,"Minérale",439,29.8,"Meropa","TEXACO","DOC HUILE\\TEXACO\\Meropa 460.pdf"]
["ISOVG460",null,null,null,"0,903 à 15°C",null,-15,254,null,0,"Minérale",460,30.9,"Meropa WM ","TEXACO","DOC HUILE\\TEXACO\\Meropa WM 460.pdf"]
["ISOVG460",null,null,null,"863,3 à 15°C",null,-30,null,null,0,"Minérale",454.7,46,"Carter SH","TOTAL ","DOC HUILE\\TOTAL\\Carter-SH.pdf"]
["ISOVG460",null,null,null,"0,903 à 15°C",null,-12,256,null,0,"Synthétique",460,29.9,"Carter EP","TOTAL ","DOC HUILE\\TOTAL\\CARTER EP.pdf"]
["ISOVG460",null,null,null,"903 à 15°C",null,-12,256,null,0,"Minérale",460,null,"Carter SP series","TOTAL ","DOC HUILE\\TOTAL\\Carter SP 460.pdf"]
["ISOVG460",null,null,null,"906 à 15°C",null,-9,244,null,0,"Synthétique",460,null,"Kassilla GMP","TOTAL ","DOC HUILE\\TOTAL\\Kassilla GMP.pdf"]
["ISOVG460",null,null,null,null,null,null,null,null,0,null,460,null,"EnergolSGXP","BP"]
["ISOVG460",null,null,null,"1064à20°C",null,-36,308,null,0,"Polyalkylene glycol",460,73.2,"TivelaOilSD","SHELL","DOCHUILE\\SHELL\\tivelaSD.pdf"]
["ISOVG460",null,null,null,"1,9 à 15°C",-20,null,null,240,"2","PTFE","440","42","MOBIL SHC PF 462","MOBIL","http://complyplus.grainger.com/grainger/msds.asp?sheetid=3824322"]
["ISOVG460",null,null,null,null,-40,260,204,180,"1","CLAY","460","45,3","MOBILTEMP SHC 460 SPECIAL","MOBIL","DOC GRAISSE\\Mobil\\Mobiltemp SHC 460 Special pds.pdf"]
["ISOVG660","KP2P-30",null,null,"0,95g/cm3à20°C",-30,null,200,110,2,"Lithium complex",600,null,"AutolTop2000 HighTemp","AGIP","DOCGRAISSE\\AGIP\\AUTOL-TOP-2000-High-Temp.pdf"]
["ISOVG660",null,null,null,"0,92 à 15°C",-37,198,204,10,"00-0","LITHIUM","620","60","MOBIL DYNAGEAR 600 SL","MOBIL","DOC GRAISSE\\Mobil\\mobil_dynagear_600_sl.pdf"]
["ISOVG68","DIN 51524-2",null,null,"0,881à15,6°C",null,-21,236,null,0,"Lithium",71.2,8.5299999999999994,"Mobil DTE 26","MOBIL","DOCHUILE\\MOBIL\\MobilDTE20series.pdf"]
["ISOVG68","K0K-12",null,null,"880 à 15°C",-12,-12,null,120,0,"Minérale",69,null,"Lamora HLP","KLÜBER","http://www.lubebase.com/cgi-bin/ctl/lube/Kluber-LAMORA-HLP-68?id=8322"]
["ISOVG68","K0K-15",null,null,null,-15,-27,239,120,0,"Minérale",68,null,"Gearmaster CLP","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG68","K2R-45",null,null,"0,96g/cm3à20°C",-45,220,null,180,2,"Polyurea+pétrole d'ester",70,9,"KlüberquietBQ72-72","KLÜBER","DOCGRAISSE\\Klüber\\KLUBERQUIETBQ7272.pdf"]
["ISOVG68",null,null,null,"932 à 15°C",null,-30,376,null,0,"Biodégradable",62,11.3,"Arnica S ","AGIP","DOC HUILE\\AGIP\\Arnica S.pdf"]
["ISOVG68",null,null,null,"868 à 15°C",null,-27,240,null,0,"Minérale",68.2,9.1,"Oso - D ","AGIP","DOC HUILE\\AGIP\\Oso - D.pdf"]
["ISOVG68",null,null,null,"0,885 à 15°C",null,-24,220,null,0,"Minérale",68,8.67,"Oso","AGIP","DOC HUILE\\AGIP\\oso.pdf"]
["ISOVG68",null,null,null,"883 à 15°C",null,-24,258,null,0,"Minérale",68,null,"Vitam DE ","ARAL","http://www.lubebase.com/"]
["ISOVG68",null,null,null,"883 à 15°C",null,-24,258,null,0,"Minérale",68,null,"Vitam GF ","ARAL","http://www.lubebase.com/"]
["ISOVG68",null,null,null,null,null,-36,280,null,0,"Biodégradable",68,null,"Hydrostar HEP","BECHEM","DOC HUILE\\BECHEM\\HYDROSTAR HEP.docx"]
["ISOVG68",null,null,null,null,null,null,null,null,0,"Minérale",68,null,"Hydrostar D","BECHEM"]
["ISOVG68",null,null,null,null,null,null,null,null,0,"Minérale",68,null,"Staroil No. 68","BECHEM"]
["ISOVG68",null,null,null,"878 à 15°C",null,-24,230,null,0,"Minérale",68,8.8000000000000007,"Energol HLP-D ","BP","DOC HUILE\\BP\\Energol HLP-D.pdf"]
["ISOVG68",null,null,null,"0,88 à 15°C",null,-24,226,null,0,"Minérale",68,8.77,"Energol HLP-HM ","BP","DOC HUILE\\BP\\Energol HLP-HM.pdf"]
["ISOVG68",null,null,null,"0,88 à 15°C",null,-36,220,null,0,"Minérale",68,11.09,"Energol SHF-HV","BP","DOC HUILE\\BP\\Energol SHF-HV.pdf"]
["ISOVG68",null,null,null,"0,89 g/cm3 à 15°C",null,-21,200,null,0,"Minérale",68,null,"Fluid Drive HM","BRUGAROLAS","DOC HUILE\\BRUGAROLAS\\lubricantes-brugarolas_aceites_industriales.pdf"]
["ISOVG68",null,null,null,"0,936 g/cm3 à 15°C",null,-36,212,null,0,"Biodégradable",66,11,"Tribol Bio Top 1448","CASTROL","http://ukrspecservise.com.ua/castrol/gidravlicheskie-masla/castrol-tribol-biotop-1448-68"]
["ISOVG68",null,null,null,"880 à 15°C",null,-30,245,null,0,"Minérale",68,8.6999999999999993,"Hyspin SP ","CASTROL","DOC HUILE\\CASTROL\\Hyspin SP.pdf"]
["ISOVG68",null,null,null,"0,88 à 20°C",null,-21,220,null,0,"Minérale",68,8.6,"Tribol 943 AW ","CASTROL","DOC HUILE\\CASTROL\\Hyspin AWS.pdf"]
["ISOVG68",null,null,null,"900 à 15°C",null,-24,230,null,0,"Minérale",68,8.6,"HLPD-Oel ","ESSO","DOC HUILE\\ESSO\\HLPD-Oel.PDF"]
["ISOVG68",null,null,null,null,null,null,null,null,0,"Biodégradable",68,null,"Eco-Hyd S","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\ECO_HYD_S_PLUS.pdf"]
["ISOVG68",null,null,null,"928 à 15°C",null,-48,304,null,0,"Biodégradable",69,12,"Plantohyd S","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\238_Planto Brochure.pdf"]
["ISOVG68",null,null,null,"875 à 15°C",null,-24,224,null,0,"Minérale",68,8.6999999999999993,"Renolin B ","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\RENOLIN_B.pdf"]
["ISOVG68",null,null,null,"881 à 15°C",null,-24,225,null,0,"Minérale",68,8.9,"Renolin MR 20","FUCHS EUROPE","DOC HUILE\\FUCHS EUROPE\\RENOLIN_MR.pdf"]
["ISOVG68",null,null,null,"0,884 à 15°C",null,-45,218,null,0,"Minérale",68,10.02,"Mobil DTE 10M series","MOBIL","DOC HUILE\\MOBIL\\Mobil_DTE_11M_OIl.pdf"]
["ISOVG68",null,null,null,"0,881 à 15,6°C",null,-21,236,null,0,"Minérale",71.2,8.5299999999999994,"Mobil DTE 20 series","MOBIL","DOC HUILE\\MOBIL\\Mobil DTE 20 series.pdf"]
["ISOVG68",null,null,null,"0,882 à 15°c",null,-18,234,null,0,"Minérale",68,8.5,"Nuto H series","MOBIL","DOC HUILE\\MOBIL\\Nuto.pdf"]
["ISOVG68",null,null,null,"924 à 15°C",null,-42,320,null,0,"Biodégradable",67.7,12.3,"Naturelle HF-E ","SHELL","DOC HUILE\\SHELL\\Naturelle HF-E 68.pdf"]
["ISOVG68",null,null,null,"0,886 à 15°C",null,-24,223,null,0,"Minérale",68,8.86,"Tellus","SHELL","DOC HUILE\\SHELL\\Tellus.pdf"]
["ISOVG68",null,null,null,"881 à 15°C",null,-24,245,null,0,"Minérale",68,8.8000000000000007,"Tellus DO","SHELL","http://www.expert-oil.com/site.xp/057057124051053054.html"]
["ISOVG68",null,null,null,"877 à 15°C",null,-36,225,null,0,"Minérale",68,10.5,"Tellus T","SHELL","DOC HUILE\\SHELL\\Tellus T.pdf"]
["ISOVG68",null,null,null,"0,889 à 15°C",null,-27,220,null,0,"Minérale",68,8.2799999999999994,"Alcor DD ","TEXACO","http://texaco-oil.ru/catalog/category39101/11728.html"]
["ISOVG68",null,null,null,null,null,-30,235,null,0,"Minérale",68,8.4,"Rando HD","TEXACO","DOC HUILE\\TEXACO\\Rando HD.pdf"]
["ISOVG68",null,null,null,"882 à 15°C",null,-30,230,null,0,"Minérale",68,8.6,"Azolla DZF","TOTAL ","DOC HUILE\\TOTAL\\Azolla DZF.pdf"]
["ISOVG68",null,null,null,"884 à 15°C",null,-27,232,null,0,"Minérale",67.5,6.8,"Azolla ZS","TOTAL ","DOC HUILE\\TOTAL\\AZOLLA_ZS.pdf"]
["ISOVG68",null,null,null,"882 à 15°C",null,-36,220,null,0,"Minérale",68,15.6,"Equivis ZS","TOTAL ","DOC HUILE\\TOTAL\\EQUIVIS_ZS.pdf"]
["ISOVG68",null,null,null,null,null,null,null,null,0,"Blanche",68,null,"WEISSÖL W530","VOGELSANG  "]
["ISOVG68",null,null,null,"878à15°C",null,-33,236,null,null,"Minérale",68,10.85,"Q8","HELLER","DOCHUILE\\HELLER\\Q8.pdf"]
["ISOVG68",null,null,null,"0,89 g/cm3 à 20°C",-30,216,215,150,"0","ALUMINIUM COMPLEX","70",null,"MOLYKOTE G-0050FG","DOW CORNING","DOC GRAISSE\\DOW CORNING\\molykote g-0050 fg3.pdf"]
["ISOVG680","K0K-10",null,null,null,-10,-15,244,120,0,"Minérale",680,null,"Gearmaster CLP","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG680","K0N-20",null,null,null,-20,-33,280,150,0,"Synthétique",680,null,"Gearmaster SYN","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG680","K0N-20",null,null,null,-20,-33,290,150,0,"Synthétique",680,null,"Gearmaster PGP ","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\LUBRICATING-FLUIDS-Fuchs-Lubritech.pdf"]
["ISOVG680","KP1K-30",null,null,"0,909à15°C",-30,215,null,120,1,"Lithium",680,39,"Mobilgrease XTC","MOBIL","DOCGRAISSE\\Mobil\\MobilgreaseXTCpds.pdf"]
["ISOVG680","KP1K-30",null,null,"0,909 à 15°C",-30,215,204,120,"1","LITHIUM","680","39","MOBILGREASE XTC","MOBIL","DOC GRAISSE\\Mobil\\Mobilgrease XTC pds.pdf"]
["ISOVG680","KP1N-10",null,null,null,-10,null,null,140,"1","LITHIUM COMPLEX","680",null,"MOBILGREASE XHP 681 MINE","MOBIL","DOC GRAISSE\\Mobil\\mobilgrease-xhp-mine-series.pdf"]
["ISOVG680",null,null,null,"0,913 à 15°C",null,-12,308,null,0,"Minérale",680,null,"Degol BG","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG680",null,null,null,"0,905 à 15°C",null,-9,255,null,0,"Minérale",680,null,"Degol BG Plus","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG680",null,null,null,"1 à 15°C",null,-36,292,null,0,"Synthétique",680,null,"Degol GS","ARAL","DOC HUILE\\ARAL\\aral-industrieschmierstoffe.pdf"]
["ISOVG680",null,null,null,null,null,null,null,null,0,"Minérale",680,null,"Eco Gear M","BECHEM"]
["ISOVG680",null,null,null,"0,90 g/cm3  15°C",null,-18,256,null,0,"Minérale",658,38,"Staroil G ","BECHEM","DOC HUILE\\BECHEM\\Produktblad DK BECHEM Staroil G 100...680.pdf"]
["ISOVG680",null,null,null,null,null,null,null,null,0,"Synthétique",680,null,"Eco Gear S","BECHEM"]
["ISOVG680",null,null,null,"1,08 g/cm3 à 15°C",null,-30,238,null,0,"Synthétique",680,105,"Berusynth EP ","BECHEM","DOC HUILE\\BECHEM\\BECHEM Berusynth EP_68_1000_9590019(GB).pdf"]
["ISOVG680",null,null,null,"926 à 15°C",null,-9,246,null,0,"Minérale",680,43,"Energol GR-XP","BP","DOC HUILE\\BP\\ENERGOL GR-XP.pdf"]
["ISOVG680",null,null,null,null,null,-9,225,null,0,"Minérale",680,37.799999999999997,"Beslux Gear XP ","BRUGAROLAS","DOC HUILE\\BRUGAROLAS\\lubricantes-brugarolas_aceites_industriales.pdf"]
["ISOVG680",null,null,null,"0,87 à 15°C",null,-33,240,null,0,"Synthétique",680,57,"Alphasyn EP ","CASTROL","DOC HUILE\\CASTROL\\Alphasyn EP.pdf"]
["ISOVG680",null,null,null,"0,92 à 15°C",null,-9,229,null,0,"Minérale",680,37.299999999999997,"Alpha SP","CASTROL","DOC HUILE\\CASTROL\\Alpha SP.pdf"]
["ISOVG680",null,null,null,"923 à 15°C",null,-15,260,null,0,"Minérale",673,35.9,"Tribol 1100","CASTROL","DOC HUILE\\CASTROL\\Tribol 1100.pdf"]
["ISOVG680",null,null,null,"1075 à 15°C",null,-27,290,null,0,"Synthétique",680,112,"Tribol 800","CASTROL","DOC HUILE\\CASTROL\\Tribol 800 .pdf"]
["ISOVG680",null,null,null,"881 à 15°C",null,-9,240,null,0,"Minérale",680,43.8,"Spartan EP series","ESSO","DOC HUILE\\ESSO\\Spartan EP series.pdf"]
["ISOVG680",null,null,null,"858 à 15°C",null,-33,300,null,0,"Synthétique",680,62.2,"Renolin Unisyn CLP series","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\RENOLIN_UNISYN_CLP.pdf"]
["ISOVG680",null,null,null,"918 à 15°C",null,-10,270,null,0,"Minérale",680,36.799999999999997,"Renolin CLP","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\Renolin CLP.pdf"]
["ISOVG680",null,null,null,"1075 à 15°C",null,-33,280,null,0,"Synthétique",680,110.3,"Renolin PG","FUCHS EUROPE ","DOC HUILE\\FUCHS EUROPE\\RENOLIN_PG.pdf"]
["ISOVG680",null,null,null,"1,05 à 20°C",null,-25,250,null,0,"Synthétique",680,110,"Syntheso D EP","KLÜBER","DOC HUILE\\KLUBER\\Syntheso D EP.pdf"]
["ISOVG680",null,null,null,"0,866 à 15°C",null,-30,240,null,0,"Synthétique",680,64.599999999999994,"Mobilgear SHC XMP","MOBIL","DOC HUILE\\MOBIL\\Mobilgear SHC XMP Series pds.pdf"]
["ISOVG680",null,null,null,null,null,-6,232,null,0,"Minérale",680,34.700000000000003,"Mobil gear 600 series  ","MOBIL","DOC HUILE\\MOBIL\\Mobilgear 600 Series pds.pdf"]
["ISOVG680",null,null,null,"1,051 à 15°C",null,-37,280,null,0,"Synthétique",680,114,"Glycoyle HE series","MOBIL","DOC HUILE\\MOBIL\\Glygoyle HE Series pds.pdf"]
["ISOVG680",null,null,null,"0,917 à 15°C",null,-9,272,null,0,"Minérale",680,36.9,"Mobilgear XMP series","MOBIL","36,9DOC HUILE\\MOBIL\\mobilgear_xmp_series.pdf"]
["ISOVG680",null,null,null,"918,4 à 20°C",null,-9,205,null,0,"Minérale",680,38,"Shell Omala","SHELL","DOC HUILE\\SHELL\\Shell Omala.pdf"]
["ISOVG680",null,null,null,null,null,-12,260,null,0,"Minérale",680,36.5,"Meropa","TEXACO","DOC HUILE\\TEXACO\\Meropa680.pdf"]
["ISOVG680",null,null,null,"864,9 à 15°C",null,-21,237,null,0,"Synthétique",676,64,"Carter SH","TOTAL ","DOC HUILE\\TOTAL\\Carter-SH.pdf"]
["ISOVG680",null,null,null,"0,92 à 15°C",null,-12,258,null,0,"Minérale",665.6,34.5,"Carter EP","TOTAL ","DOC HUILE\\TOTAL\\CARTER EP.pdf"]
["ISOVG680",null,null,null,"0,91 à 15°C",-40,175,158,10,"00-0","LITHIUM","680","60","MOBIL DYNAGEAR 800 EXTRA","MOBIL","DOC GRAISSE\\Mobil\\mobil_dynagear_800_extra.pdf"]
["ISOVG80","KP2S-20",null,null,"1000à20°C",-20,230,150,200,2,"Lithium complex",80,null,"Urethyn MP2","FUCHSEUROPE","DOCGRAISSE\\FUCHSEUROPE\\URETHYN_E2.pdf"]
["ISOVG800","KPF2N-30",null,null,null,-30,null,null,140,"2","LITHIUM","800",null,"ARALUB 4320","ARAL"]
["L-XBCEB 0","MP0K-25",null,null,"0,9 à 15°C",-25,351,null,120,"0","LITHIUM-CALCIUM","150","17","MULTIS EP 0","ELF","http://www.onshoreoils.com.au/utto__universal_tractor_transmission_oil_.php?catid=8"]
["L-XBCEB 1","KP1K-30",null,null,"0,9 à 15°C",-30,354,null,120,"1","LITHIUM-CALCIUM","150","17","MULTIS EP 1","ELF","http://www.onshoreoils.com.au/utto__universal_tractor_transmission_oil_.php?catid=8"]
["L-XBCEB 2","KP2K-25",null,null,"0,9 à 15°C",-25,361,null,120,"2","LITHIUM-CALCIUM","150","17","MULTIS EP 2","ELF","http://www.onshoreoils.com.au/utto__universal_tractor_transmission_oil_.php?catid=8"]
["L-XBCEB 3","KP3K-20",null,null,null,-20,null,null,120,"3","LITHIUM-CALCIUM","150","17","MULTIS EP 3","ELF","http://www.onshoreoils.com.au/utto__universal_tractor_transmission_oil_.php?catid=8"]
["L-XCBEB 00","GP00G-30",null,null,"0,9 à 15°C",-30,343,null,100,"00","LITHIUM-CALCIUM","150","15","MULTIS EP 00","ELF","DOC GRAISSE\\ELF\\MULTIS-EP-00.pdf"]
["L-XCBEB 000","GP000G-30",null,null,null,-30,null,null,100,"000","LITHIUM-CALCIUM","150",null,"MULTIS EP 000","ELF","DOC GRAISSE\\ELF\\MULTIS EP 000 FR.pdf"]
["SOVG120",null,null,null,"0,89 g/cm3 à 20°C",-30,null,246,150,"2","ALUMINIUM COMPLEX","115",null,"MOLYKOTE G-0052FG","DOW CORNING","DOC GRAISSE\\DOW CORNING\\molykote g-0050 fg3.pdf"]