{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["PV","Calculs","Synthèse","exemple"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":78,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"PV","index":0,"n_rows":745,"n_cols":14,"rows_kept":745,"cut":false,"hidden":false,"merged":[]}
["RESULTATS","DE","MESURES"]
["Site","de","Douvrin"]
["DESIGNATION",":","CULASSE"]
["Type",":","DV5R"]
["Ligne",":","L3"]
["N°","Piece",":"]
["N°","Adaptateur",":",14]
["Opération",":",120]
["N°","Meteor",":",3]
["N°","Demande","ou","de","Commande",":"]
["METROLOGUE",":","Date","de","rédaction",":"]
["Nbre","de","pièces","mesurées",":"]
["Incertitude","de","mesure",":","U","=","±2.1","+","L","/",333,"Repère",":"]
["Equipement(s)","utilisé(s)",":","DEA","09-15-08","Logiciel",":","METROLOG","XG12"]
["DEMANDEUR",":","Service",":"]
["Tél",":"]
["Tél",":",8,3804]
["Le","classement","et","l'archivage"]
["de","ce","document","sont","à","la"]
["charge","du","demandeur."]
["Interprétation","des","écarts","dans","le","secteur","mécanique",":"]
["Les","cotes","mesurées","et","les","écarts","relevés","sont","donnés","par","rapport","au(x)","référentiel(s)","pièce."]
["RESPONSABLE",":","EVERLET.E","Visa","métrologue",":"]
["date","de","mod.",":","2015-10-12","13:06:56"]
["Version",":"]
["Indice","modif.",":","m00"]
["DVR-120-man.gm2"]
["XG","14.004","HF4"]
["2016-02-09","20:12:09"]
["(","Facultatif","pour","demande","DMB",")"]
[1,"/",11]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["Fraisage","finition","face","combustion."]
["Pour","info","coordonnées","des","points","de","palpage."]
["X+","de","LG01","vers","LG02"]
["Z+","de","LG01","vers","face","admission."]
["PLA_FACE_F","Planéité","planéité","face","combustion"]
["PLAN","0.000","0.019","0.030","0.019"]
["INFO_PT5","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.008","0.008"]
["INFO_PT6","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.009","0.009"]
["INFO_PT7","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.009","0.009"]
["INFO_PT8","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.012","0.012"]
["INFO_PT9","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.012","0.012"]
["INFO_PT10","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.007","0.007"]
["INFO_PT11","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.006","0.006"]
["INFO_PT12","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.005","0.005"]
["INFO_PT13","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.004","0.004"]
["INFO_PT14","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.002","0.002"]
["INFO_PT15","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.002","0.002"]
["INFO_PT16","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.002","0.002"]
["INFO_PT17","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.004","0.004"]
["INFO_PT18","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.001","0.001"]
["INFO_PT19","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.000","-0.000"]
["INFO_PT20","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.000","0.000"]
["INFO_PT21","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.001","0.001"]
["INFO_PT22","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.006","0.006"]
["INFO_PT23","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.008","0.008"]
["INFO_PT24","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.002","0.002"]
["INFO_PT25","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.002","0.002"]
["INFO_PT26","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.000","-0.000"]
["INFO_PT27","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.000","0.000"]
["INFO_PT28","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.000","-0.000"]
["INFO_PT29","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.000","0.000"]
["INFO_PT30","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.003","0.003"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[14]
[3]
["Ligne",":"]
["Opération",":"]
["L3"]
[120]
[2,"/",11]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["INFO_PT31","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.002","0.002"]
["INFO_PT32","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.002","-0.002"]
["INFO_PT33","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.002","-0.002"]
["INFO_PT34","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT35","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT36","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.001","0.001"]
["INFO_PT37","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.001","0.001"]
["INFO_PT38","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.004","-0.004"]
["INFO_PT39","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.002","-0.002"]
["INFO_PT40","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.001","-0.001"]
["INFO_PT41","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.005","-0.005"]
["INFO_PT42","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT43","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.002","-0.002"]
["INFO_PT44","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT45","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.000","0.000"]
["INFO_PT46","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT47","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.005","-0.005"]
["INFO_PT48","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT49","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT50","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT51","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.006","-0.006"]
["INFO_PT52","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.002","-0.002"]
["INFO_PT53","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.000","-0.000"]
["INFO_PT54","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.005","0.005"]
["INFO_PT55","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.002","-0.002"]
["INFO_PT56","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.006","-0.006"]
["INFO_PT57","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.009","-0.009"]
["INFO_PT58","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.002","-0.002"]
["INFO_PT59","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.004","-0.004"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[14]
[3]
["Ligne",":"]
["Opération",":"]
["L3"]
[120]
[3,"/",11]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["INFO_PT60","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.004","-0.004"]
["INFO_PT61","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.001","-0.001"]
["INFO_PT62","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.000","0.000"]
["INFO_PT63","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.005","-0.005"]
["INFO_PT64","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.006","-0.006"]
["INFO_PT65","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.007","-0.007"]
["INFO_PT66","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.007","-0.007"]
["INFO_PT67","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.006","-0.006"]
["INFO_PT68","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.005","-0.005"]
["INFO_PT69","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.004","-0.004"]
["INFO_PT70","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.000","-0.000"]
["INFO_PT71","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.003","0.003"]
["INFO_PT72","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.002","-0.002"]
["INFO_PT73","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.001","-0.001"]
["INFO_PT74","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.008","-0.008"]
["INFO_PT75","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.006","-0.006"]
["INFO_PT76","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.005","-0.005"]
["INFO_PT77","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.008","0.008"]
["INFO_PT78","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.001","0.001"]
["INFO_PT79","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT80","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.005","-0.005"]
["INFO_PT81","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.007","-0.007"]
["INFO_PT82","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.000","0.000"]
["INFO_PT83","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.001","0.001"]
["INFO_PT84","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT85","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.002","0.002"]
["INFO_PT86","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.003","0.003"]
["INFO_PT87","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.005","-0.005"]
["INFO_PT88","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.004","-0.004"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[14]
[3]
["Ligne",":"]
["Opération",":"]
["L3"]
[120]
[4,"/",11]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["INFO_PT89","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.005","-0.005"]
["INFO_PT90","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.004","-0.004"]
["INFO_PT91","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.004","-0.004"]
["INFO_PT92","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.004","-0.004"]
["INFO_PT93","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.001","0.001"]
["INFO_PT94","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.002","0.002"]
["INFO_PT95","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT96","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.004","-0.004"]
["INFO_PT97","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.004","-0.004"]
["INFO_PT98","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.005","0.005"]
["INFO_PT99","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT100","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.007","-0.007"]
["INFO_PT101","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.005","0.005"]
["INFO_PT102","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.002","-0.002"]
["INFO_PT103","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.006","-0.006"]
["INFO_PT104","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.006","-0.006"]
["INFO_PT105","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.001","-0.001"]
["INFO_PT106","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT107","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.001","-0.001"]
["INFO_PT108","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.007","-0.007"]
["INFO_PT109","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.005","-0.005"]
["INFO_PT110","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.002","0.002"]
["INFO_PT111","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.001","0.001"]
["INFO_PT112","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.002","-0.002"]
["INFO_PT113","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.005","-0.005"]
["INFO_PT114","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.004","-0.004"]
["INFO_PT115","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.004","-0.004"]
["INFO_PT116","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.005","-0.005"]
["INFO_PT117","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.007","-0.007"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[14]
[3]
["Ligne",":"]
["Opération",":"]
["L3"]
[120]
[5,"/",11]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["INFO_PT118","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.002","-0.002"]
["INFO_PT119","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT120","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT121","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.002","-0.002"]
["INFO_PT122","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.000","-0.000"]
["INFO_PT123","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.005","-0.005"]
["INFO_PT124","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.006","-0.006"]
["INFO_PT125","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.008","-0.008"]
["INFO_PT126","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT127","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.002","0.002"]
["INFO_PT128","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.002","0.002"]
["INFO_PT129","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.001","-0.001"]
["INFO_PT130","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.001","-0.001"]
["INFO_PT131","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.002","-0.002"]
["INFO_PT132","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.002","0.002"]
["INFO_PT133","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.003","-0.003"]
["INFO_PT134","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.001","-0.001"]
["INFO_PT135","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.004","-0.004"]
["INFO_PT136","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.003","0.003"]
["INFO_PT137","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.004","-0.004"]
["INFO_PT138","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.001","0.001"]
["INFO_PT139","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.004","-0.004"]
["INFO_PT140","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.002","-0.002"]
["INFO_PT141","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.001","0.001"]
["INFO_PT142","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.001","0.001"]
["INFO_PT143","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.008","0.008"]
["INFO_PT144","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.009","0.009"]
["INFO_PT145","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.003","0.003"]
["INFO_PT146","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.002","0.002"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[14]
[3]
["Ligne",":"]
["Opération",":"]
["L3"]
[120]
[6,"/",11]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["INFO_PT147","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.002","0.002"]
["INFO_PT148","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.001","-0.001"]
["INFO_PT149","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.003","0.003"]
["INFO_PT150","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.001","-0.001"]
["INFO_PT151","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","-0.001","-0.001"]
["INFO_PT152","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.003","0.003"]
["INFO_PT153","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.001","0.001"]
["INFO_PT154","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.001","0.001"]
["INFO_PT155","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.002","0.002"]
["INFO_PT156","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.006","0.006"]
["INFO_PT157","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.006","0.006"]
["INFO_PT158","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.008","0.008"]
["INFO_PT159","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.003","0.003"]
["INFO_PT160","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.008","0.008"]
["INFO_PT161","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.005","0.005"]
["INFO_PT162","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.007","0.007"]
["INFO_PT163","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.005","0.005"]
["INFO_PT164","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.006","0.006"]
["INFO_PT166","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.001","0.001"]
["INFO_PT167","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.005","0.005"]
["INFO_PT168","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.008","0.008"]
["INFO_PT169","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.009","0.009"]
["INFO_PT170","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.010","0.010"]
["INFO_PT171","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.010","0.010"]
["INFO_PT172","Distance","Sect.","+","extérieur","matière"]
["Y","0.000","0.010","0.010"]
["DI_F_APP_1","Distance","Position","face","comb","face","à","l'appui",1,"de","AAC"]
["Y","88.430","88.449","-0.050","0.050","0.019"]
["DI_F_APP_2","Distance","Position","face","comb","face","à","l'appui",2,"de","AAC"]
["Y","88.430","88.445","-0.050","0.050","0.015"]
["DI_F_APP_3","Distance","Position","face","comb","face","à","l'appui",3,"de","AAC"]
["Y","88.430","88.445","-0.050","0.050","0.015"]
["DI_F_APP_4","Distance","Position","face","comb","face","à","l'appui",4,"de","AAC"]
["Y","88.430","88.457","-0.050","0.050","0.027"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[14]
[3]
["Ligne",":"]
["Opération",":"]
["L3"]
[120]
[7,"/",11]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["LOC_FACE_F","Localis.","Localisation","calculée","sur","les",4,"points"]
["LOCA","0.000","0.054","0.100","0.054"]
["DI_F_RETRAIT_1","Distance","Coté","BV","vers","LG01"]
["Y","0.000","-0.196","-0.500","0.000","-0.196"]
["DI_F_RETRAIT_2","Distance","Coté","BV","et","ADM."]
["Y","0.000","-0.196","-0.500","0.000","-0.196"]
["DI_F_RETRAIT_3","Distance","Coté","Dist.","et","ADM."]
["Y","0.000","-0.186","-0.500","0.000","-0.186"]
["Perçage","profond","et","alésage","CH01."]
["ALE_CH01_1","Cercle","Pour","info"]
["DIAM","12.650","12.869","0.219"]
["X","353.450","353.454","-0.200","0.200","0.004"]
["Z","82.500","82.512","-0.200","0.200","0.012"]
["E.F.","0.016","0.016"]
["ALE_CH01_2","Cercle","Pour","info"]
["DIAM","12.650","12.884","0.234"]
["X","353.450","353.448","-0.200","0.200","-0.002"]
["Z","82.500","82.506","-0.200","0.200","0.006"]
["E.F.","0.003","0.003"]
["ALE_CH01_3","Cercle","Pour","info"]
["DIAM","12.000","12.020","0.020"]
["X","353.450","353.447","-0.200","0.200","-0.003"]
["Z","82.500","82.505","-0.200","0.200","0.005"]
["E.F.","0.003","0.003"]
["ALE_CH01_4","Cercle","Pour","info"]
["DIAM","12.000","12.016","0.016"]
["X","353.450","353.448","-0.200","0.200","-0.002"]
["Z","82.500","82.507","-0.200","0.200","0.007"]
["E.F.","0.006","0.006"]
["ANG_ALE_CH01_1","Angle","Pour","info","alésage","12.65"]
["XoY","1.000","0.908","-0.580","0.580","-0.092"]
["ANG_ALE_CH01_2","Angle","Pour","info","alésage",12]
["XoY","1.000","1.003","-0.580","0.580","0.003"]
["PER_PRO_CH01_E","Cercle"]
["DIAM","8.000","8.196","0.196"]
["E.F.","0.002","0.002"]
["PER_PRO_CH01_F","Cercle"]
["DIAM","8.000","8.161","0.161"]
["E.F.","0.000","0.000"]
["ANG_PER_CH01_HE","Angle","Pour","info","alésage","12.65"]
["XoY","1.000","1.001","-0.580","0.580","0.001"]
["PT_CH01_PRO_E","Point","Pour","info","localisation"]
["X","353.450","353.440","-0.250","0.250","-0.010"]
["Z","82.500","82.509","-0.250","0.250","0.009"]
["PT_CH01_PRO_F","Point","Pour","info","localisation"]
["X","353.450","353.440","-0.250","0.250","-0.010"]
["Z","82.500","82.467","-0.250","0.250","-0.033"]
["LOC_CH01_HE","Localis."]
["LOCA","0.000","0.069","0.500","0.069"]
["COA_CH01_1","Coaxialité","Diam.","12.65","/","HE"]
["COAX","0.000","0.040","0.400","0.040"]
["COA_CH01_2","Coaxialité","Diam.",12,"/","HE"]
["COAX","0.000","0.030","0.400","0.030"]
["Perçage","profond","descente","d'huile","DH01."]
["PER_PRO_DH01_E","Cercle"]
["DIAM","8.000","8.207","0.207"]
["E.F.","0.001","0.001"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[14]
[3]
["Ligne",":"]
["Opération",":"]
["L3"]
[120]
[8,"/",11]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["PER_PRO_DH01_F","Cercle"]
["DIAM","8.000","8.165","0.165"]
["E.F.","0.004","0.004"]
["ANG_PER_DH01","Angle","Pour","info"]
["YoZ","83.500","83.459","-0.580","0.580","-0.041"]
["PT_DH01_PRO_E","Point","Pour","info","localisation"]
["X","168.000","167.999","-0.250","0.250","-0.001"]
["Z","115.750","115.696","-0.250","0.250","-0.054"]
["PT_DH01_PRO_F","Point","Pour","info","localisation"]
["X","168.000","167.951","-0.250","0.250","-0.049"]
["Z","115.750","115.746","-0.250","0.250","-0.004"]
["LOC_DH01_PRO","Localis."]
["LOCA","0.000","0.108","0.500","0.108"]
["Perçage","passage","trou","d'eau","PE01."]
["PER_PE01_E","Cercle"]
["DIAM","12.000","11.995","-0.005"]
["E.F.","0.001","0.001"]
["PER_PE01_F","Cercle"]
["DIAM","12.000","11.996","-0.004"]
["E.F.","0.010","0.010"]
["ANG_PER_PE01_1","Angle","Pour","info"]
["ZoX","11.350","11.214","-0.580","0.580","-0.136"]
["ANG_PER_PE01_2","Angle","Pour","info"]
["ESP","54.500","54.470","-0.580","0.580","-0.030"]
["PT_PE01_E","Point","Pour","info","localisation"]
["Y","109.020","109.013","-0.250","0.250","-0.007"]
["Z","43.050","43.105","-0.250","0.250","0.055"]
["PT_PE01_F","Point","Pour","info","localisation"]
["Y","109.020","109.094","-0.250","0.250","0.074"]
["Z","43.050","43.073","-0.250","0.250","0.023"]
["LOC_PE01","Localis."]
["LOCA","0.000","0.156","0.500","0.156"]
["Chanfreinage","sortie","d'injecteur."]
["PL_IJ01","Plan"]
["E.F.","0.001","0.001"]
["CE_IJ01","Cercle","Pour","info"]
["DIAM","8.093","8.275","0.182"]
["X","42.000","42.001","0.001"]
["Y","45.500","45.505","0.005"]
["E.F.","0.001","0.001"]
["CHANF_IJ01","Cône"]
["ANGL","90.000","91.088","1.088"]
["E.F.","0.005","0.005"]
["PJ_IJ01","Point"]
["Z","0.250","0.337","-0.100","0.100","0.087"]
["PL_IJ02","Plan"]
["E.F.","0.001","0.001"]
["CE_IJ02","Cercle","Pour","info"]
["DIAM","8.093","8.277","0.184"]
["X","126.000","125.993","-0.007"]
["Y","45.500","45.506","0.006"]
["E.F.","0.001","0.001"]
["CHANF_IJ02","Cône"]
["ANGL","90.000","90.889","0.889"]
["E.F.","0.007","0.007"]
["PJ_IJ02","Point"]
["Z","0.250","0.335","-0.100","0.100","0.085"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[14]
[3]
["Ligne",":"]
["Opération",":"]
["L3"]
[120]
[9,"/",11]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["PL_IJ03","Plan"]
["E.F.","0.001","0.001"]
["CE_IJ03","Cercle","Pour","info"]
["DIAM","8.093","8.275","0.182"]
["X","210.000","209.990","-0.010"]
["Y","45.500","45.507","0.007"]
["E.F.","0.000","0.000"]
["CHANF_IJ03","Cône"]
["ANGL","90.000","90.947","0.947"]
["E.F.","0.006","0.006"]
["PJ_IJ03","Point"]
["Z","0.250","0.330","-0.100","0.100","0.080"]
["PL_IJ04","Plan"]
["E.F.","0.000","0.000"]
["CE_IJ04","Cercle","Pour","info"]
["DIAM","8.093","8.286","0.193"]
["X","294.000","293.987","-0.013"]
["Y","45.500","45.509","0.009"]
["E.F.","0.001","0.001"]
["CHANF_IJ04","Cône"]
["ANGL","90.000","91.023","1.023"]
["E.F.","0.007","0.007"]
["PJ_IJ04","Point"]
["Z","0.250","0.341","-0.100","0.100","0.091"]
["Fraisage","passage","échangeur","DG01","et","DG02."]
["DI_DG01","Distance","Pour","info","localisation"]
["Z","80.500","80.603","-0.250","0.250","0.103"]
["LOC_DG01","Localis."]
["LOCA","0.000","0.205","0.500","0.205"]
["DI_DG02","Distance","Pour","info","localisation"]
["Y","10.000","10.174","-0.250","0.250","0.174"]
["LOC_DG02","Localis."]
["LOCA","0.000","0.348","0.500","0.348"]
["Fraisage","face","FW02."]
["DI_FW02_1","Distance","Pour","info","localisation","coté","BV-Comb"]
["Z","79.500","79.602","-0.250","0.250","0.102"]
["DI_FW02_2","Distance","Pour","info","localisation","milieu","vers","PAAC"]
["Z","79.500","79.436","-0.250","0.250","-0.064"]
["DI_FW02_3","Distance","Pour","info","localisation","coté","Dist-Comb"]
["Z","79.500","79.436","-0.250","0.250","-0.064"]
["LOC_FW02","Localis."]
["LOCA","0.000","0.203","0.500","0.203"]
["Fraisage","ébavurage","montage","PP","HP","DG09."]
["DI_PP","HP_1","Distance","Pour","info","localisation"]
["Z","10.000","9.858","-0.250","0.250","-0.142"]
["LOC_PP","HP_1","Localis."]
["LOCA","0.000","0.284","0.500","0.284"]
["DI_PP","HP_2","Distance","Pour","info","localisation"]
["X","186.470","186.349","-0.250","0.250","-0.121"]
["LOC_PP","HP_2","Localis."]
["LOCA","0.000","0.242","0.500","0.242"]
["Défonçage","sortie","EGR","SEGR"]
["SEGR","Cercle","Pour","info","localisation"]
["DIAM","25.000","25.018","0.018"]
["X","22.000","22.009","-0.100","0.100","0.009"]
["Y","31.000","31.090","-0.100","0.100","0.090"]
["E.F.","0.006","0.006"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[14]
[3]
["Ligne",":"]
["Opération",":"]
["L3"]
[120]
[10,"/",11]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["LOC_SEGR","Localis."]
["LOCA","0.000","0.180","0.300","0.180"]
["Alésage","chanfreinage","logt.","plugg","BC01","-","BC02."]
["PL_BC01","Plan"]
["E.F.","0.000","0.000"]
["ALE_BC01","Cercle","Pour","info","localisation"]
["DIAM","20.000","20.017","-0.050","0.050","0.017"]
["X","15.500","15.590","-0.250","0.250","0.090"]
["Y","78.000","77.951","-0.250","0.250","-0.049"]
["E.F.","0.016","0.016"]
["LOC_BC01","Localis."]
["LOCA","0.000","0.205","0.500","0.205"]
["PL_BC02","Plan"]
["E.F.","0.001","0.001"]
["ALE_BC02","Cercle","Pour","info","localisation"]
["DIAM","20.000","20.020","-0.050","0.050","0.020"]
["X","15.500","15.564","-0.250","0.250","0.064"]
["Y","258.000","257.952","-0.250","0.250","-0.048"]
["E.F.","0.012","0.012"]
["LOC_BC02","Localis."]
["LOCA","0.000","0.160","0.500","0.160"]
["DUREE-PROG","Texte/Valeur","Durée","du","programme","en","Minutes"]
["VAL","0.000","26.685","0.000","120.000","26.685"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[14]
[3]
["Ligne",":"]
["Opération",":"]
["L3"]
[120]
[11,"/",11]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]

{"sheet":"Calculs","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Synthèse","index":2,"n_rows":4,"n_cols":5,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
[]
[null,{"$f":"\"Désignation : \"&PV!C3","v":"Désignation : CULASSE"},null,null,{"$f":"\"OP : \"&PV!C8&\".\"&PV!D9","v":"OP : 120.3"}]
[null,{"$f":"\"Type : \"&PV!C4","v":"Type : DV5R"},null,null,{"$f":"\"N° adaptateur : \"&PV!D7","v":"N° adaptateur : 14"}]
[null,{"$f":"\"Ligne : \"&PV!C5","v":"Ligne : L3"},null,null,{"$f":"\"Date : \"&TEXT(INDEX(PV!A:A,MATCH(\"Metrologic\",PV!A:A,0)-3,1),\"JJ/MM/AAAA\")","v":"Date : 09/02/2016"}]

{"sheet":"exemple","index":3,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["aaaaaa"]