**ERA 4**

|  |
| --- |
| Apollo 40 PR |
| Traction PR 15 |
| Speed ​​9 + 7 = 16 PR |
| Total 71 PR |
| ARES 45 PR |
| A path | path B | path C |
| 6 PR accelerator | Speed ​​16 PR | Reliability 8 PR |
|  | Wagons 20 PR |  |
| Total 51 PR | Total 81 PR | Total 53 PR |
| NEPTUNE 25 PR | Horus 60 PR | HERMES 60 PR |
| Acceleration 7 + 3 = 10 PR | Speed ​​7 PR | Wagons 13 + 12 = 25 PR |
| Wagons 15 PR | Wagons 16 PR | Speed ​​25 +15 = 40 PR |
|  | Reliability 5 + 5 = 10 PR |  |
|  |  | Full options (recommended) |
|  |  | Acceleration 6+ 4 = 10 PR |
|  |  | Reliability 5 + 5 = 10 PR |
| Total 50 PR | Total 93 PR | PR Total 125 (145 Full PR) |
| THOR 40 PR |
| Wagons 20 + 18 = 38 PR |
| Acceleration 12 + 7 = 19 PR |
| Speed ​​15 + 7 = 22 PR |
| Reliability 6 + 13 = 19 PR |
| Total 138 PR |
| POSEIDON 50 PR |
| Wagons 25 PR |
| Acceleration 18 + 8 = 26 PR |
| Speed ​​16 + 20 = 36 PR |
| Reliability 13 PR |
| Total 146 PR |
| Hook 80 PR |
| TOTAL | TOTAL B | TOTAL C (BIS) |
| 536 PR | 609 PR | 613 PR (PR 633) |

Note :

It is for everyone to choose their own path. This is an indication but, it is to consider making the loco V priority with FULL OPTIONS and continue to THOR when you have finished with V.

Good game to all.