{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["waste management","Feuille principale"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"waste management","index":0,"n_rows":56,"n_cols":3,"rows_kept":56,"cut":false,"hidden":false,"merged":[]}
[null,"Pareto Analysis: Waste ","Perte"]
[null,"causes des Pertes ","Perte"]
[null,"Huile hydraulique",4237]
[null,"Perte Transpalette ",1487]
[null,"TCA21",1184]
[null,"Perte Préparation ",875]
[null,"Boucle libre vide URA",801]
[null,"Echantillonneur",789]
[null,"Air stérile",785]
[null,"Défaut traitement",500]
[null,"Pulvérisation",489]
[null,"Nettoyage Intermédiare ",458]
[null,"Chambre aseptique",456]
[null,"Température armoire électrique",456]
[null,"Servomoteur",452]
[null,"Four",394]
[null,"Languette ouverture",375]
[null,"Perte Echantillon en cours de Production ",369]
[null,"Autre Perte Partie superieure ",320]
[null,"Hélix ",258]
[null,"Autre Perte DE",245]
[null,"Toboggan",242]
[null,"Changement du tank",238]
[null,"Autre Perte Logistique ",196]
[null,"Surcharge poste de sortie",189]
[null,"Débit eau soudure bas",178]
[null,"Roue à godets",147]
[null,"Dispatcheur  ",147]
[null,"Fin Bobine Patch",145]
[null,"Couronne de Formation ",142]
[null,"Changement de format",125]
[null,"Perte Retourneur Bobine ",123]
[null,"Système de nettoyage",123]
[null,"Raccord Film",117]
[null,"Laisser passer TLS",111]
[null,"Absence Opérateur",91]
[null,"Décors hors limites",85]
[null,"Non Respect du standard",81]
[null,"Stérilisateur",78]
[null,"Languette intérieure",74]
[null,"température d'eau de refroidissement",63]
[null,"Raccord Papier",60]
[null," Perte Chariot logistique ",50]
[null,"Peroxyde",48]
[null,"Surcharge moteur",47]
[null,"Rupture Papier URA",41]
[null,"Convoyeur",26]
[null,"Système lecture de niveau ",20]
[null,"correction Volume",17]
[null,"Reservoire de Peroxyde  ",16]
[null,"Echangeur de chaleur",14]
[null,"Fin Bobine Aluminium",12]
[null,"Batterie de chauffe",12]
[null," Nettoyage Complet",5]
[null,"Perte (Humidité)",5]
[null,"Autre Perte organisationnelProduction ",1]

{"sheet":"Feuille principale","index":1,"n_rows":14,"n_cols":3,"rows_kept":14,"cut":false,"hidden":false,"merged":[[13,2,15,7]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Je souhaite exécuter l'opération de filtration à partir de cette feuille "]