{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Accuel","Consommation","ModulePV","Batterie"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Accuel","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Consommation","index":1,"n_rows":10,"n_cols":27,"rows_kept":10,"cut":false,"hidden":false,"merged":[[2,3,2,26]]}
[]
[]
[null,null,null,"Repartition journalière de l'utilisation"]
["Noms","Puissance (W)","Quantité","00:00:00","01:00:00","02:00:00","03:00:00","04:00:00","05:00:00","06:00:00","07:00:00","08:00:00","09:00:00","10:00:00","11:00:00","12:00:00","13:00:00","14:00:00","15:00:00","16:00:00","17:00:00","18:00:00","19:00:00","20:00:00","21:00:00","22:00:00","23:00:00"]
["A",1,2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Z",1,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["E",4,3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["R",3,1,3,3,3,0,3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["H",2,1,2,26,26,8,18,0,0,0,0,0,0,0,8,8,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,58,58,16,42,0,0,0,0,0,0,0,16,16,0,0,0,0,0,0,0,0,0,0]

{"sheet":"ModulePV","index":2,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":false,"merged":[[2,0,2,2],[16,0,16,2]]}
[]
[]
["Paramètres du module PV choisi"]
["Puissance crête",140,"W"]
["Tension Vmp",20,"V"]
["Courant Imp",7.78,"A"]
["Tension Voc",21.6,"V"]
["Courant Isc",8.85,"A"]
["Tension nominale",12,"V"]
["K t° de Voc",-0.35,"/°C"]
["K t° de Isc",3.6999999999999998E-2,"/°C"]
["K t° de Pmpp",-0.48,"/°C"]
["Longuer",1480,"mm"]
["Largeur",673,"mm"]
[]
[]
["Module PV par défaut"]
["Puissance crête",140,"W"]
["Tension Vmp",20,"V"]
["Courant Imp",7.78,"A"]
["Tension Voc",21.6,"V"]
["Courant Isc",8.85,"A"]
["Tension nominale",12,"V"]
["K t° de Voc",-0.35,"/°C"]
["K t° de Isc",3.6999999999999998E-2,"/°C"]
["K t° de Pmpp",-0.48,"/°C"]
["Longuer",1480,"mm"]
["Largeur",673,"mm"]

{"sheet":"Batterie","index":3,"n_rows":13,"n_cols":3,"rows_kept":13,"cut":false,"hidden":false,"merged":[[2,0,2,2]]}
[]
[]
["Paramètres de la Batterie choisie"]
["Rendement","é"]
["Jours d'autonomie",null,"jrs"]
["t° la plus basse",null,"°C"]
["Capacité",null,"Ah"]
["Tension nominale",null,"V"]
["Profondeur de décharge",null,"%"]
["K t° de la batterie"]
["Exposant de Peukert"]
["Facteur de recharge"]
["Temps de recharge",null,"heure(s)"]