{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["ancien","nouveau","niveaux","statistiques"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":3,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ancien","index":0,"n_rows":41,"n_cols":6,"rows_kept":41,"cut":false,"hidden":false,"merged":[[27,5,28,5],[25,5,26,5],[21,2,22,2],[23,2,24,2],[27,2,28,2],[27,4,28,4],[23,4,24,4],[21,4,22,4],[23,5,24,5],[27,0,28,0],[27,3,28,3],[25,1,26,1],[27,1,28,1],[25,2,26,2],[25,3,26,3],[40,0,41,1],[36,0,37,5],[29,0,30,0],[29,1,30,1],[29,2,30,2],[32,0,34,5],[29,3,30,3],[29,4,30,4],[29,5,30,5],[40,2,41,5],[23,0,24,0],[4,0,5,0],[19,0,20,0],[25,4,26,4],[25,0,26,0],[23,3,24,3],[19,1,20,1],[19,2,20,2],[19,3,20,3],[23,1,24,1],[4,5,5,5],[19,5,20,5],[0,0,1,0],[21,0,22,0],[0,5,1,5],[0,1,1,4],[21,5,22,5],[21,3,22,3],[19,4,20,4],[21,1,22,1],[2,0,3,5]]}
["RHODIA Chalampé     Service Incendie","SUIVI DU STOCK EMULSEUR",null,null,null,"180 IT 008    "]
[]
["NE PLUS UTILISER"]
[]
["Lieu ou Véhicule","Capacité","Quantité","Référence :","Date ","Analyse ou N° de Lot"]
[null,"du stockage","en stock","Emulseur / Classe","d'achat"]
[]
["Station Mousse","1- 8000 L",0,"Polypétrofilm / 1","27/17/1998"," 12/03/2002"]
[null,"2- 8000 L",7500,"MOUSSOL APS 3%","10/2012"]
[null,"3- 8000 L",1550,"MOUSSOL APS 3%","2013-07-01"]
[null,"4- 8000 L"]
[]
[null,32000,{"$f":"SUM(C8:C11)","v":9050}]
["RESERVE   LOCAL",null,null,"         "]
["    INCENDIE","***  0 "]
["Aux Garages  n°2 et 3",3000,0]
["Emulseur stocké dans  ",null,31000,"Uniseral AF 22","2015/2016"]
["     Containers de ",null,1000,"Polypétrofilm / 1"]
["     1000 Litres       ",null,"   ",null,"   ","   "]
["V.M.R. 60",3000,3000,"Uniseral AF 22","2015/2016"]
[]
["V.M.R. 105",10000,10000,"Uniseral AF 22","2015/2016"]
[]
["V.M.R. 100",10000,10000,"Moussol APS 3%","10/2011"]
[]
["C.C.EM. 1",8000,8000,"Moussol APS 3%","10/2011"]
[]
["C.C.EM. 2",8000,8000,"Uniseral AF 22","2015/2016"]
[]
["TOTAL",71000,{"$f":"SUM(C13,C15,C16,C17,C20,C22,C24,C26,C28)","v":79050},"Différence :",{"$f":"SUM(C30-B30)","v":8050},"Litres"]
[]
[]
["Date du dernier recensement :    03/06/2019       "]
[]
[]
[]
["NOM :               Equipe :    A"]
[]
[]
[]
["VERSION 2",null,"Date d'application : FEVRIER 2012"]

{"sheet":"nouveau","index":1,"n_rows":66,"n_cols":10,"rows_kept":66,"cut":false,"hidden":false,"merged":[[0,1,1,3],[2,1,2,4],[27,0,27,4],[30,0,30,3],[32,0,32,4],[0,0,1,0],[12,0,12,4],[15,0,15,3],[9,0,9,4],[10,0,10,3],[20,0,20,3],[17,0,17,4],[22,0,22,4],[0,4,1,4],[5,0,5,3],[3,0,3,4],[60,0,60,3],[4,0,4,3],[35,0,35,3],[37,0,37,4],[40,0,40,3],[42,0,42,4],[45,0,45,3],[47,0,47,4],[25,0,25,3],[50,0,50,3],[52,0,52,4],[55,0,55,3],[57,0,57,4]]}
["SOLVAY Chalampé\nService Incendie","SUIVI DU STOCK EMULSEUR",null,null,"180 IT 008    "]
[]
["VERSION 3","Date d'application : JUILLET 2019"]
[]
["TOTAL EMULSEUR SUR SITE",null,null,null,{"$f":"E16+E21+E26+E31+E36+E41+E46+E51+E56+E61","v":69900}]
["TOTAL EMULSEUR OPERATIONNEL",null,null,null,{"$f":"E11+E41+E46+E51+E56+E61","v":54700}]
[null,null,null,null,null,"Date","Date","Date","Date","Date"]
[null,null,null,null,null,"2019-07-17","2019-07-17","2019-07-17","2019-06-30","2019-06-29"]
[null,null,null,null,null,"Motif d'utilisation","Motif d'utilisation","Motif d'utilisation","Motif d'utilisation","Motif d'utilisation"]
["TOTAL STATION MOUSSE",null,null,null,null,"Intervention","Intervention","Essai","Relevés","Relevés"]
["STOCK TOTAL EN COURS",null,null,null,{"$f":"E16+E21+E26+E31","v":17200}]
[]
["STATION MOUSSE - n°1"]
["Capacité",8000,"Date achat","27/17/1998","Utilisé",null,null,null,null,6600]
["Type émulseur","Polypétrofilm / 1","Date analyse","2002-03-12","Appointé"]
["STOCK EN COURS",null,null,null,1400]
[]
["STATION MOUSSE - n°2"]
["Capacité",8000,"Date achat","2012-10-01","Utilisé",null,null,null,null,500]
["Type émulseur","Moussol","Date analyse",null,"Appointé"]
["STOCK EN COURS",null,null,null,7500]
[]
["STATION MOUSSE - n°3"]
["Capacité",8000,"Date achat","2013-07-01","Utilisé",null,null,null,null,4700]
["Type émulseur","Moussol","Date analyse",null,"Appointé",3000]
["STOCK EN COURS",null,null,null,6300]
[]
["STATION MOUSSE - n°4"]
["Capacité",8000,"Date achat",null,"Utilisé",null,null,null,null,8000]
["Type émulseur",null,"Date analyse",null,"Appointé",null,2000]
["STOCK EN COURS",null,null,null,2000]
[]
["CONTAINERS 1000L"]
["Capacité",31600,"Date achat","2015/2016","Utilisé",3000,2000,1800,1600,8000]
["Type émulseur","Uniseral AF 22","Date analyse",null,"Appointé"]
["STOCK EN COURS",null,null,null,15200]
[]
["VMR60"]
["Capacité",3000,"Date achat","2015/2016","Utilisé",null,null,1800,null,1600]
["Type émulseur","Uniseral AF 22","Date analyse",null,"Appointé",null,null,1800,1600]
["STOCK EN COURS",null,null,null,3000]
[]
["VMR105"]
["Capacité",10000,"Date achat","2015/2016","Utilisé",null,null,null,null,900]
["Type émulseur","Uniseral AF 22","Date analyse",null,"Appointé"]
["STOCK EN COURS",null,null,null,9100]
[]
["VMR100"]
["Capacité",10000,"Date achat","2011-10-01","Utilisé"]
["Type émulseur","Moussol","Date analyse",null,"Appointé"]
["STOCK EN COURS",null,null,null,10000]
[]
["CEEM1"]
["Capacité",8000,"Date achat","2011-10-01","Utilisé"]
["Type émulseur","Moussol","Date analyse",null,"Appointé"]
["STOCK EN COURS",null,null,null,8000]
[]
["CEEM2"]
["Capacité",8000,"Date achat","2015/2016","Utilisé",null,null,null,null,600]
["Type émulseur","Uniseral AF 22","Date analyse",null,"Appointé"]
["STOCK EN COURS",null,null,null,7400]
[]
[null,null,null,null,"TOTAL Relevés",null,null,null,1600]
[null,null,null,null,"TOTAL Formation"]
[null,null,null,null,"TOTAL Intervention",3000,2000]
[null,null,null,null,"TOTAL Essai",null,null,1800]

{"sheet":"niveaux","index":2,"n_rows":17,"n_cols":34,"rows_kept":17,"cut":false,"hidden":false,"merged":[[4,5,4,6],[0,0,0,4],[1,5,1,6],[3,5,3,6],[2,5,2,6],[0,5,0,6]]}
["CALCULS AUTOMATIQUES POUR NIVEAUX EMULSEURS",null,null,null,null,"Liste déroulante"]
[null,null,null,null,null,"Intervention"]
["VMR60",null,null,null,null,"Formation"]
["Niveau collerette / produit (en cm)",85,null,null,null,"Relevés"]
["Volume émulseur restant (en littres)",{"$f":"(143-B4)*3000/136","v":1279.4117647058824},null,null,null,"Essai"]
[]
["VMR105"]
["Niveau lu (en %)",91]
["Volume émulseur restant (en littres)",{"$f":"B8*10000/100","v":9100}]
[]
["VMR100"]
["Niveau collerette / produit (en cm)",0,5,10,15,20,25,30,35,40,45,50,55,60,65,70,75,80,85,90,95,100,105,110,115,120]
["Volume émulseur restant (en littres)",0,1448,4044,7330,11130,15335,19863,24651,29646,34800,40070,45416,50799,56183,61529,66800,71953,76948,81736,86265,90469,94269,97555,100151,101599]
[]
["CEEM"]
["Niveau collerette / produit (en cm)",0,5,10,15,20,25,30,35,40,45,50,55,60,65,70,75,80,85,90,95,100,105,110,115,120,125,130,135,140,145,150,155,160]
["Volume émulseur restant (en littres)",0,70,210,380,580,800,1040,1300,1570,1850,2150,2450,2750,3070,3380,3700,4020,4340,4660,4980,5290,5590,5900,6190,6470,6740,7000,7240,7460,7660,7830,7970,8040]

{"sheet":"statistiques","index":3,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":false,"merged":[[2,0,2,1]]}
[]
[]
["Année de statistiques",null,2019]
[]
["Relevés"]
["Intervention",3000]
["Formation"]
["Essai"]