{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Feuil1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Feuil1","index":0,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
[]
["CAP-CERM 10nF,20%,200V,X7R,Poly T",{"$f":"capa(A2)","v":"10n"},{"$f":"tol(A2)","v":20}]
["CAP-CERM 2.2UF,20%,16V,X5R,,0603",{"$f":"capa(A3)","v":"2.2U"},{"$f":"tol(A3)","v":20}]
["RES-TF 4.7k,5%,63.0mW,200ppm/C,155","4.7k",5]
["RES-TF 100R,0.5%,63.0mW,200ppm/C,15","100",0.5]