{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["selección","datas","test"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":56,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"selección","index":0,"n_rows":9,"n_cols":10,"rows_kept":9,"cut":false,"hidden":false,"merged":[[2,7,2,9],[1,7,1,9]]}
[]
[null,null,"Equipment Category","Equipment Type","Shaft Power Kw and other","RPM","Floor Span","Results"]
[null,"Click on a cell to see the choices","Piping.and.ducts","all.7","all",42,"Up.to.6.m","Slab on Grade"]
[null,null,"Air.Compressors.and.Vacuum.Pumps2","Centrifugal..scroll2",null,null,null,"Base Type","Isolator Type","Min Defl. Min"]
[]
[null,null,null,null,null,null,null,null,"Floor Span"]
[null,null,null,null,null,null,null,"Base Type","Isolator Type","Min Defl. Min"]
[]
[null,null,null,null,null,null,null,null,"Reference Notes"]

{"sheet":"datas","index":1,"n_rows":40,"n_cols":19,"rows_kept":40,"cut":false,"hidden":false,"merged":[]}
[]
["Type","Equipment_Category","Refrigeration.Machines.and.Chillers","Air.Compressors.and.Vacuum.Pumps","Pumps","Cooling.Tower","Bollers","Axial.Fans..Plenum.Fans..Cabinet.Fans..Fan.sections..Centrifugal.Inline.Fans","Centrifugal.Fans","Propeller.Fans","Heat.Pumps..Fan.Colls..Computer.Room.units","Condensing.units","Packaged.AH..AC..H.and.V.Units","Packaged.Rooftop.Equipment","Ducted.Rotating.Equipment","Engine.Driven.Generators","Piping.and.ducts",null,"Floor_span"]
["Equipment_Category","Refrigeration.Machines.and.Chillers","Reciprocating","Tank.mounted..horizontal","Close.coupled","all.1","Fire.tubed","Up.to.560.mm.diameter","Up.to.560.mm.diameter2","Wall.mouted","all.2","all.3","all.4","all.5","Small.fans..fan.powered","all.6","all.7",null,"Up.to.6.m"]
["Equipment_type","Air.Compressors.and.Vacuum.Pumps","Centrifugal..scroll","Tank.mounted.vert","Large.inline",null,"Water.tubed..copper.fin","from.610.mm.diameter.and.up","from.610.mm.diameter.and.up2","Roof.mouted",null,null,null,null,null,null,null,null,"6.to.9.m"]
["Shaft","Pumps","Screw","Base.mounted","End.suction.and.split.case",null,null,null,null,null,null,null,null,null,null,null,null,null,"9.to.12.m"]
["RPM","Cooling.Tower","Absorbtion","Larg.reciprocating","Packaged.pump.systems"]
["Slab","Bollers","Air.cooled recip..scroll"]
["Floor _span","Axial.Fans..Plenum.Fans..Cabinet.Fans..Fan.sections..Centrifugal.Inline.Fans","Air.cooled screw"]
["Reference_note","Centrifugal.Fans"]
[null,"Propeller.Fans"]
[null,"Heat.Pumps..Fan.Colls..Computer.Room.units"]
[null,"Condensing.units"]
[null,"Packaged.AH..AC..H.and.V.Units"]
[null,"Packaged.Rooftop.Equipment"]
[null,"Ducted.Rotating.Equipment"]
[null,"Engine.Driven.Generators"]
[null,"Piping.and.ducts"]
[]
[]
[null,"Reciprocating","Centrifugal..scroll","Screw","Absorbtion","Air.cooled.recip..scroll","Air.cooled.screw"]
["Shaft..Power..kW.and.Other","all","all","all","all","all","all"]
[null,null,null,null,null,null,"Centrifugal Vans","Up.to.560.mm.diameter2","from.610.mm.diameter.and.up2"]
[null,"Tank.mounted.horizontal","Tank.mounted.vert","Base.mounted","Large.reciprocating",null,null,"all","<=30",null,"Piping.and.ducts","all.7"]
["Shaft..Power..kW.and.Other","<=7,5","all","all","all",null,null,null,">=37",null,null,"seen section on Isolating Vibration and noise in Piping Systems"]
[null,">=11"]
[null,null,null,null,null,null,"Propellers fans","Wall.mouted","Roof.mouted"]
[null,"Close.coupled","Large.inline","End.suction.and.split.case","Packaged.pump.systems",null,null,"all","all"]
["Shaft..Power..kW.and.Other","<=5,6","3,7 to 19","<=30","all"]
[null,">=7,5",">=22","37 to 93",null,null,"Heat.Pumps..Fan.Colls..Computer.Room.units","all.2",null,"Packaged.Rooftop.Equipment","all.5"]
["Cooling tower","all.1",null,">=110",null,null,null,"all",null,null,"all"]
["Shaft..Power..kW.and.Other","all"]
[null,null,null,null,null,null,"Condensing.units","all.3",null,"Ducted.Rotating.Equipment","Small.fans..fan.powered"]
[null,"Fire.tubed","Water.tubed..copper.fin",null,null,null,null,"all",null,null,"<=300 L/s"]
["Shaft..Power..kW.and.Other","all","all",null,null,null,null,null,null,null,">=301 l/s"]
[null,null,null,null,null,null,"Packaged.AH..AC..H.and.V.Units","all.4"]
["axial fans","Up.to.560.mm.diameter","from.610.mm.diameter.and.up",null,null,null,null,"<=7,5",null,"Engine.Driven.Generators","all.6"]
["Shaft..Power..kW.and.Other","all","<=500 Pa SP",null,null,null,null,"<=11",null,null,"all"]
[null,null,">501 Pa SP",null,null,null,null,"<=1 kPa SP"]
[null,null,null,null,null,null,null,">1 kPa SP11"]
[null,null,null,null,null,null,null,">1 kPa SP"]

{"sheet":"test","index":2,"n_rows":23,"n_cols":16,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
["Equipment_Category2","Refrigeration.Machines.and.Chillers2","Air.Compressors.and.Vacuum.Pumps2","Pumps","Cooling.Tower","Bollers","Axial.Fans..Plenum.Fans..Cabinet.Fans..Fan.sections..Centrifugal.Inline.Fans","Centrifugal.Fans","Propeller.Fans","Heat.Pumps..Fan.Colls..Computer.Room.units","Condensing.units","Packaged.AH..AC..H.and.V.Units","Packaged.Rooftop.Equipment","Ducted.Rotating.Equipment","Engine.Driven.Generators","Piping.and.ducts"]
["Refrigeration.Machines.and.Chillers2","Reciprocating2","Tank.mounted..horizontal2","Close.coupled","all","Fire.tubed","Up.to.560.mm.diameter","Up.to.560.mm.diameter","Wall.mouted","all","all","all","all","Small.fans..fan.powered","all","all"]
["Air.Compressors.and.Vacuum.Pumps2","Centrifugal..scroll2","Tank.mounted.vert2","Large.inline",null,"Water.tubed..copper.fin","610.mm.diameter.and.up","610.mm.diameter.and.up","Roof.mouted",null,null,null,null,"Boxes"]
["Pumps","Screw2","Base.mounted2","End.suction.and.split.case"]
["Cooling.Tower","Absorbtion2","Larg.reciprocating2","Packaged.pump.systems"]
["Bollers","Air.cooled recip..scroll2"]
["Axial.Fans..Plenum.Fans..Cabinet.Fans..Fan.sections..Centrifugal.Inline.Fans","Air.cooled screw2"]
["Centrifugal.Fans"]
["Propeller.Fans"]
["Heat.Pumps..Fan.Colls..Computer.Room.units"]
["Condensing.units"]
["Packaged.AH..AC..H.and.V.Units"]
["Packaged.Rooftop.Equipment"]
["Ducted.Rotating.Equipment"]
["Engine.Driven.Generators"]
["Piping.and.ducts"]
[]
[]
[null,"Reciprocating2","Centrifugal..scroll2","Screw2","Absorbtion2","Air.cooled recip..scroll2","Air.cooled.screw2"]
["RPM",42,"all","all","all","all","all"]
[null,12]
[null,"Tank.mounted.horizontal","Tank.mounted.vert","Base.mounted","Larg.reciprocating"]
["RPM","all","all","all","all"]