{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["PV","Calculs","exemple"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"PV","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Calculs","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"exemple","index":2,"n_rows":853,"n_cols":14,"rows_kept":853,"cut":false,"hidden":false,"merged":[]}
["RESULTATS","DE","MESURES"]
["Site","de","Douvrin"]
["DESIGNATION",":","CULASSE"]
["Type",":","DV5R"]
["Ligne",":","L3"]
["N°","Piece",":"]
["N°","Adaptateur",":",119]
["Opération",":",30]
["N°","Meteor",":",2]
["N°","Demande","ou","de","Commande",":"]
["METROLOGUE",":","Date","de","rédaction",":"]
["Nbre","de","pièces","mesurées",":"]
["Incertitude","de","mesure",":","U","=","±2.1","+","L","/",333,"Repère",":"]
["Equipement(s)","utilisé(s)",":","DEA","09-15-08","Logiciel",":","METROLOG","XG12"]
["DEMANDEUR",":","Service",":"]
["Tél",":"]
["Tél",":",8,3804]
["Le","classement","et","l'archivage"]
["de","ce","document","sont","à","la"]
["charge","du","demandeur."]
["Interprétation","des","écarts","dans","le","secteur","mécanique",":"]
["Les","cotes","mesurées","et","les","écarts","relevés","sont","donnés","par","rapport","au(x)","référentiel(s)","pièce."]
["RESPONSABLE",":","EVERLET.E","Visa","métrologue",":"]
["date","de","mod.",":","2015-10-12","13:05:01"]
["Version",":"]
["Indice","modif.",":","m00"]
["DVR-030-man.gm2"]
["XG","14.004","HF4"]
["2016-01-25","18:33:27"]
["(","Facultatif","pour","demande","DMB",")"]
[1,"/",12]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["Palpage","des","références","brutes","pour","balançage."]
["CONDUIT_A1","Cercle","Pour","controle","fonderie"]
["DIAM","17.500","18.675","1.175"]
["X","-18.700","-18.725","-0.025"]
["Y","-15.000","-15.075","-0.075"]
["E.F.","0.071","0.071"]
["CONDUIT_A2","Cercle","Pour","controle","fonderie"]
["DIAM","17.500","18.726","1.226"]
["X","65.300","65.100","-0.200"]
["Y","-15.000","-15.163","-0.163"]
["E.F.","0.026","0.026"]
["CONDUIT_A3","Cercle","Pour","controle","fonderie"]
["DIAM","17.500","18.747","1.247"]
["X","149.300","148.965","-0.335"]
["Y","-15.000","-15.144","-0.144"]
["E.F.","0.067","0.067"]
["CONDUIT_A4","Cercle","Pour","controle","fonderie"]
["DIAM","17.500","18.724","1.224"]
["X","233.300","232.797","-0.503"]
["Y","-15.000","-14.985","0.015"]
["E.F.","0.089","0.089"]
["PT_17","Point","Pour","controle","fonderie"]
["Z","30.800","31.084","0.284"]
["PT_27","Point","Pour","controle","fonderie"]
["Z","30.800","31.019","0.219"]
["PT_37","Point","Pour","controle","fonderie"]
["Z","30.800","30.977","0.177"]
["PT_47","Point","Pour","controle","fonderie"]
["Z","30.800","31.046","0.246"]
["YA1","Distance","CONDUIT_A1","-","ORIGINE","/","X_REF_Y_REF"]
["Y","0.000","0.000","0.000"]
["YA2","Distance","CONDUIT_A2","-","ORIGINE","/","X_REF_Y_REF"]
["Y","0.000","0.118","0.118"]
["YA3","Distance","CONDUIT_A3","-","ORIGINE","/","X_REF_Y_REF"]
["Y","0.000","0.129","0.129"]
["YA4","Distance","CONDUIT_A4","-","ORIGINE","/","X_REF_Y_REF"]
["Y","0.000","0.000","0.000"]
["XR1","Distance","CONDUIT_A2","-","ORIGINE","/","X_REF_Y_REF"]
["X","84.000","83.825","-0.175"]
["XR2","Distance","CONDUIT_A3","-","ORIGINE","/","X_REF_Y_REF"]
["X","168.000","167.689","-0.311"]
["XR3","Distance","CONDUIT_A4","-","ORIGINE","/","X_REF_Y_REF"]
["X","252.000","251.522","-0.478"]
["ZA1","Distance","PT_17","-","ORIGINE","/","Z_REF"]
["Z","0.000","0.000","0.000"]
["ZA2","Distance","PT_27","-","ORIGINE","/","Z_REF"]
["Z","0.000","-0.066","-0.066"]
["ZA3","Distance","PT_37","-","ORIGINE","/","Z_REF"]
["Z","0.000","-0.107","-0.107"]
["ZA4","Distance","PT_47","-","ORIGINE","/","Z_REF"]
["Z","0.000","-0.039","-0.039"]
["Position","face","combustion","au","niveaux","des","appuis","platine."]
["Zone",1,"au","niveau","de","FC06","Impossible","à","palper","(","emcombrement","montage",")"]
["Zone",2,"au","niveau","de","FC04"]
["Zone",3,"au","niveau","de","FC02"]
["Zone",4,"au","niveau","de","FC10"]
["ZONE_1_DF","Plan","en",16,"élément(s)"]
["E.F.","0.005","0.005"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[119]
[2]
["Ligne",":"]
["Opération",":"]
["L3"]
[30]
[2,"/",12]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["POS_Z1","Point","Position","zone",1,"face","comb.","ébauche"]
["Z","0.620","0.649","0.029"]
["INFO_Z1_PT1","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","0.000","0.001","0.001"]
["INFO_Z1_PT2","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.000","-0.000"]
["INFO_Z1_PT3","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.003","0.003"]
["INFO_Z1_PT4","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.000","0.000"]
["INFO_Z1_PT5","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.003","-0.003"]
["INFO_Z1_PT6","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.003","-0.003"]
["INFO_Z1_PT7","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.001","0.001"]
["INFO_Z1_PT8","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.003","0.003"]
["INFO_Z1_PT9","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.000","0.000"]
["INFO_Z1_PT10","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.002","0.002"]
["INFO_Z1_PT11","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.001","0.001"]
["INFO_Z1_PT12","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.005","-0.005"]
["INFO_Z1_PT13","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.004","-0.004"]
["INFO_Z1_PT14","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.000","-0.000"]
["INFO_Z1_PT15","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.002","0.002"]
["INFO_Z1_PT16","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.001","0.001"]
["ZONE_2_DF","Plan","en",16,"élément(s)"]
["E.F.","0.003","0.003"]
["POS_Z2","Point","Position","zone",2,"face","comb.","ébauche"]
["Z","0.620","0.655","0.035"]
["INFO_Z2_PT1","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.000","-0.000"]
["INFO_Z2_PT2","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.004","0.004"]
["INFO_Z2_PT3","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.001","0.001"]
["INFO_Z2_PT4","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.000","-0.000"]
["INFO_Z2_PT5","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.001","-0.001"]
["INFO_Z2_PT6","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.001","-0.001"]
["INFO_Z2_PT7","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.001","-0.001"]
["INFO_Z2_PT8","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.001","-0.001"]
["INFO_Z2_PT9","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.001","0.001"]
["INFO_Z2_PT10","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.001","-0.001"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[119]
[2]
["Ligne",":"]
["Opération",":"]
["L3"]
[30]
[3,"/",12]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["INFO_Z2_PT11","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.002","-0.002"]
["INFO_Z2_PT12","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.001","-0.001"]
["INFO_Z2_PT13","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.002","-0.002"]
["INFO_Z2_PT14","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.001","0.001"]
["INFO_Z2_PT15","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.002","0.002"]
["INFO_Z2_PT16","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.002","0.002"]
["ZONE_3_DF","Plan","en",16,"élément(s)"]
["E.F.","0.005","0.005"]
["POS_Z3","Point","Position","zone",3,"face","comb.","ébauche"]
["Z","0.620","0.646","0.026"]
["INFO_Z3_PT1","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.000","-0.000"]
["INFO_Z3_PT2","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.001","0.001"]
["INFO_Z3_PT3","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.000","0.000"]
["INFO_Z3_PT4","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.000","-0.000"]
["INFO_Z3_PT5","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.001","0.001"]
["INFO_Z3_PT6","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.002","0.002"]
["INFO_Z3_PT7","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.001","0.001"]
["INFO_Z3_PT8","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.001","-0.001"]
["INFO_Z3_PT9","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.000","0.000"]
["INFO_Z3_PT10","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.003","-0.003"]
["INFO_Z3_PT11","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.001","-0.001"]
["INFO_Z3_PT12","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.001","-0.001"]
["INFO_Z3_PT13","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.000","-0.000"]
["INFO_Z3_PT14","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.000","-0.000"]
["INFO_Z3_PT15","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.001","0.001"]
["INFO_Z3_PT16","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.002","0.002"]
["ZONE_4_DF","Plan","en",16,"élément(s)"]
["E.F.","0.003","0.003"]
["POS_Z4","Point","Position","zone",4,"face","comb.","ébauche"]
["Z","0.620","0.642","0.022"]
["INFO_Z4_PT1","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.001","-0.001"]
["INFO_Z4_PT2","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.000","0.000"]
["INFO_Z4_PT3","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.001","0.001"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[119]
[2]
["Ligne",":"]
["Opération",":"]
["L3"]
[30]
[4,"/",12]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["INFO_Z4_PT4","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.002","0.002"]
["INFO_Z4_PT5","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.000","0.000"]
["INFO_Z4_PT6","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.001","0.001"]
["INFO_Z4_PT7","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.000","0.000"]
["INFO_Z4_PT8","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.002","-0.002"]
["INFO_Z4_PT9","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.003","-0.003"]
["INFO_Z4_PT10","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.002","-0.002"]
["INFO_Z4_PT11","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.001","-0.001"]
["INFO_Z4_PT12","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","-0.000","-0.000"]
["INFO_Z4_PT13","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.001","0.001"]
["INFO_Z4_PT14","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.003","0.003"]
["INFO_Z4_PT15","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.001","0.001"]
["INFO_Z4_PT16","Distance","à","titre","info","Secteur","+","extérieur","matière"]
["Z","-0.000","0.000","0.000"]
["PLA_Z1_A_Z4","Planéité","Zones",1,"à",4]
["PLAN","0.000","0.009","0.050","0.009"]
["POS_Z","Point","Position","zone",4,"face","comb.","ébauche"]
["Z","0.620","0.645","-0.120","0.120","0.025"]
["Alésage","finition","locatings","LG01","et","LG02"]
["LG01_D14.03","Cercle"]
["DIAM","14.030","14.049","0.019"]
["E.F.","0.017","0.017"]
["LG01_D12.7","Cercle"]
["DIAM","12.700","12.731","0.031"]
["E.F.","0.002","0.002"]
["LG01_D14_INFO","Distance","Position","loc.","cyl.","LG01"]
["X","42.000","41.993","-0.150","0.150","-0.007"]
["Y","46.500","46.587","-0.150","0.150","0.087"]
["LG01_D12.7_INFO","Distance","Position","loc.","cyl.","LG01"]
["X","42.000","42.000","-0.150","0.150","0.000"]
["Y","46.500","46.590","-0.150","0.150","0.090"]
["LOC_LG01_D14","Localis.","Locating","LG01","diam",14]
["LOCA","0.000","0.174","0.300","0.174"]
["LG02_D14.03_1","Cercle"]
["DIAM","14.030","14.066","0.036"]
["E.F.","0.002","0.002"]
["LG02_D14.03_2","Cercle"]
["DIAM","14.030","14.064","0.034"]
["E.F.","0.002","0.002"]
["LG02_D12.7_1","Cercle"]
["DIAM","12.700","12.732","0.032"]
["LG02_D12.7_2","Cercle"]
["DIAM","12.700","12.730","0.030"]
["E.F.","0.002","0.002"]
["ALE_LG02_1_D14.03","Distance","LG02","/","LG01","diam.14.03"]
["Y","335.750","335.746","-0.125","0.125","-0.004"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[119]
[2]
["Ligne",":"]
["Opération",":"]
["L3"]
[30]
[5,"/",12]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["ALE_LG02_2_D14.03","Distance","LG02","/","LG01","diam.14.03"]
["Y","336.250","336.246","-0.125","0.125","-0.004"]
["ALE_LG02_1_D12.7","Distance","LG02","/","LG01","diam.12.7"]
["Y","335.750","335.746","-0.125","0.125","-0.004"]
["ALE_LG02_2_D12.7","Distance","LG02","/","LG01","diam.12.7"]
["Y","336.250","336.246","-0.125","0.125","-0.004"]
["INFO_LG02_D14.03","Distance","/","PY","-","PX","(","336-42)=294"]
["X","294.000","294.003","-0.150","0.150","0.003"]
["Y","46.500","46.570","-0.150","0.150","0.070"]
["LOC_LG02_D14.03","Localis.","Des","arcs","de","cercle","de","LG02","D14.03"]
["LOCA","0.000","0.140","0.300","0.140"]
["Lamage","appuis","vis","FC01","à","FC10"]
["POS_APP_FC01_INFO","Point","A","titre","info","loca"]
["Z","65.620","65.678","-0.125","0.125","0.058"]
["LOC_APP_VIS_FC01","Localis."]
["LOCA","0.000","0.116","0.250","0.116"]
["PAR_FC01","Parallél."]
["PARA","0.000","0.019","0.150","0.019"]
["PLA_FC01","Planéité"]
["PLAN","0.000","0.018","0.050","0.018"]
["POS_APP_FC02_INFO","Point","A","titre","info","loca"]
["Z","65.620","65.670","-0.125","0.125","0.050"]
["LOC_APP_VIS_FC02","Localis."]
["LOCA","0.000","0.100","0.250","0.100"]
["PAR_FC02","Parallél."]
["PARA","0.000","0.018","0.150","0.018"]
["PLA_FC02","Planéité"]
["PLAN","0.000","0.017","0.050","0.017"]
["POS_APP_FC03_INFO","Point","A","titre","info","loca"]
["Z","65.620","65.668","-0.125","0.125","0.048"]
["LOC_APP_VIS_FC03","Localis."]
["LOCA","0.000","0.097","0.250","0.097"]
["PAR_FC03","Parallél."]
["PARA","0.000","0.017","0.150","0.017"]
["PLA_FC03","Planéité"]
["PLAN","0.000","0.017","0.050","0.017"]
["POS_APP_FC04_INFO","Point","A","titre","info","loca"]
["Z","65.620","65.675","-0.125","0.125","0.055"]
["LOC_APP_VIS_FC04","Localis."]
["LOCA","0.000","0.110","0.250","0.110"]
["PAR_FC04","Parallél."]
["PARA","0.000","0.032","0.150","0.032"]
["PLA_FC04","Planéité"]
["PLAN","0.000","0.031","0.050","0.031"]
["POS_APP_FC05_INFO","Point","A","titre","info","loca"]
["Z","65.620","65.718","-0.125","0.125","0.098"]
["LOC_APP_VIS_FC05","Localis."]
["LOCA","0.000","0.195","0.250","0.195"]
["PAR_FC05","Parallél."]
["PARA","0.000","0.089","0.150","0.089"]
["PLA_FC05","Planéité"]
["PLAN","0.000","0.076","0.050","0.076","0.026"]
["POS_APP_FC06_INFO","Point","A","titre","info","loca"]
["Z","65.620","65.655","-0.125","0.125","0.035"]
["LOC_APP_VIS_FC06","Localis."]
["LOCA","0.000","0.071","0.250","0.071"]
["PAR_FC06","Parallél."]
["PARA","0.000","0.015","0.150","0.015"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[119]
[2]
["Ligne",":"]
["Opération",":"]
["L3"]
[30]
[6,"/",12]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["PLA_FC06","Planéité"]
["PLAN","0.000","0.015","0.050","0.015"]
["POS_APP_FC07_INFO","Point","A","titre","info","loca"]
["Z","65.620","65.651","-0.125","0.125","0.031"]
["LOC_APP_VIS_FC07","Localis."]
["LOCA","0.000","0.062","0.250","0.062"]
["PAR_FC07","Parallél."]
["PARA","0.000","0.013","0.150","0.013"]
["PLA_FC07","Planéité"]
["PLAN","0.000","0.013","0.050","0.013"]
["POS_APP_FC08_INFO","Point","A","titre","info","loca"]
["Z","65.620","65.655","-0.125","0.125","0.035"]
["LOC_APP_VIS_FC08","Localis."]
["LOCA","0.000","0.070","0.250","0.070"]
["PAR_FC08","Parallél."]
["PARA","0.000","0.014","0.150","0.014"]
["PLA_FC08","Planéité"]
["PLAN","0.000","0.013","0.050","0.013"]
["POS_APP_FC09_INFO","Point","A","titre","info","loca"]
["Z","65.620","65.670","-0.125","0.125","0.050"]
["LOC_APP_VIS_FC09","Localis."]
["LOCA","0.000","0.101","0.250","0.101"]
["PAR_FC09","Parallél."]
["PARA","0.000","0.030","0.150","0.030"]
["PLA_FC09","Planéité"]
["PLAN","0.000","0.028","0.050","0.028"]
["POS_APP_FC10_INFO","Point","A","titre","info","loca"]
["Z","65.620","65.662","-0.125","0.125","0.042"]
["LOC_APP_VIS_FC10","Localis."]
["LOCA","0.000","0.084","0.250","0.084"]
["PAR_FC10","Parallél."]
["PARA","0.000","0.012","0.150","0.012"]
["PLA_FC10","Planéité"]
["PLAN","0.000","0.012","0.050","0.012"]
["Perçage","passages","de","vis","coté","face","combustion"]
["CE_FC01_S","Cercle","A","la","sortie"]
["DIAM","12.100","12.313","0.213"]
["E.F.","0.004","0.004"]
["CE_FC01_E","Cercle","A","l'entrée"]
["DIAM","12.100","12.311","0.211"]
["E.F.","0.000","0.000"]
["PT_FC01_E","Point","A","titre","info","loca","Sect.+","vers","FC06"]
["X","0.000","-0.077","-0.200","0.200","-0.077"]
["Y","0.000","0.006","-0.200","0.200","0.006"]
["PT_FC01_S","Point","A","titre","info","loca","Sect.+","vers","FC06"]
["X","0.000","-0.079","-0.200","0.200","-0.079"]
["Y","0.000","0.001","-0.200","0.200","0.001"]
["LOC_FC01","Localis."]
["LOCA","0.000","0.158","0.400","0.158"]
["CE_FC02_S","Cercle","A","la","sortie"]
["DIAM","12.100","12.313","0.213"]
["E.F.","0.005","0.005"]
["CE_FC02_E","Cercle","A","l'entrée"]
["DIAM","12.100","12.311","0.211"]
["E.F.","0.000","0.000"]
["PT_FC02_E","Point","A","titre","info","loca","Sect.+","vers","FC06"]
["X","84.000","83.942","-0.200","0.200","-0.058"]
["Y","0.000","-0.022","-0.200","0.200","-0.022"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[119]
[2]
["Ligne",":"]
["Opération",":"]
["L3"]
[30]
[7,"/",12]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["PT_FC02_S","Point","A","titre","info","loca","Sect.+","vers","FC06"]
["X","84.000","83.907","-0.200","0.200","-0.093"]
["Y","0.000","0.008","-0.200","0.200","0.008"]
["LOC_FC02","Localis."]
["LOCA","0.000","0.187","0.400","0.187"]
["CE_FC03_S","Cercle","A","la","sortie"]
["DIAM","12.100","12.316","0.216"]
["E.F.","0.001","0.001"]
["CE_FC03_E","Cercle","A","l'entrée"]
["DIAM","12.100","12.304","0.204"]
["E.F.","0.009","0.009"]
["PT_FC03_E","Point","A","titre","info","loca","Sect.+","vers","FC06"]
["X","168.000","167.914","-0.200","0.200","-0.086"]
["Y","0.000","-0.040","-0.200","0.200","-0.040"]
["PT_FC03_S","Point","A","titre","info","loca","Sect.+","vers","FC06"]
["X","168.000","167.918","-0.200","0.200","-0.082"]
["Y","0.000","0.009","-0.200","0.200","0.009"]
["LOC_FC03","Localis."]
["LOCA","0.000","0.190","0.400","0.190"]
["CE_FC04_S","Cercle","A","la","sortie"]
["DIAM","12.100","12.312","0.212"]
["E.F.","0.004","0.004"]
["CE_FC04_E","Cercle","A","l'entrée"]
["DIAM","12.100","12.306","0.206"]
["E.F.","0.009","0.009"]
["PT_FC04_E","Point","A","titre","info","loca","Sect.+","vers","FC06"]
["X","252.000","251.904","-0.200","0.200","-0.096"]
["Y","0.000","-0.001","-0.200","0.200","-0.001"]
["PT_FC04_S","Point","A","titre","info","loca","Sect.+","vers","FC06"]
["X","252.000","251.924","-0.200","0.200","-0.076"]
["Y","0.000","0.001","-0.200","0.200","0.001"]
["LOC_FC04","Localis."]
["LOCA","0.000","0.193","0.400","0.193"]
["CE_FC05_S","Cercle","A","la","sortie"]
["DIAM","12.100","12.315","0.215"]
["E.F.","0.007","0.007"]
["CE_FC05_E","Cercle","A","l'entrée"]
["DIAM","12.100","12.303","0.203"]
["E.F.","0.007","0.007"]
["PT_FC05_E","Point","A","titre","info","loca","Sect.+","vers","FC06"]
["X","336.000","335.873","-0.200","0.200","-0.127"]
["Y","0.000","-0.028","-0.200","0.200","-0.028"]
["PT_FC05_S","Point","A","titre","info","loca","Sect.+","vers","FC06"]
["X","336.000","335.895","-0.200","0.200","-0.105"]
["Y","0.000","0.009","-0.200","0.200","0.009"]
["LOC_FC05","Localis."]
["LOCA","0.000","0.259","0.400","0.259"]
["CE_FC06_S","Cercle","A","la","sortie"]
["DIAM","12.100","12.311","0.211"]
["E.F.","0.005","0.005"]
["CE_FC06_E","Cercle","A","l'entrée"]
["DIAM","12.100","12.313","0.213"]
["E.F.","0.000","0.000"]
["PT_FC06_E","Point","A","titre","info","loca"]
["X","336.000","335.911","-0.200","0.200","-0.089"]
["Y","93.000","92.965","-0.200","0.200","-0.035"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[119]
[2]
["Ligne",":"]
["Opération",":"]
["L3"]
[30]
[8,"/",12]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["PT_FC06_S","Point","A","titre","info","loca"]
["X","336.000","335.888","-0.200","0.200","-0.112"]
["Y","93.000","93.024","-0.200","0.200","0.024"]
["LOC_FC06","Localis."]
["LOCA","0.000","0.228","0.400","0.228"]
["CE_FC07_S","Cercle","A","la","sortie"]
["DIAM","12.100","12.307","0.207"]
["E.F.","0.002","0.002"]
["CE_FC07_E","Cercle","A","l'entrée"]
["DIAM","12.100","12.311","0.211"]
["E.F.","0.005","0.005"]
["PT_FC07_E","Point","A","titre","info","loca"]
["X","252.000","251.922","-0.200","0.200","-0.078"]
["Y","93.000","92.998","-0.200","0.200","-0.002"]
["PT_FC07_S","Point","A","titre","info","loca"]
["X","252.000","251.899","-0.200","0.200","-0.101"]
["Y","93.000","93.003","-0.200","0.200","0.003"]
["LOC_FC07","Localis."]
["LOCA","0.000","0.203","0.400","0.203"]
["CE_FC08_S","Cercle","A","la","sortie"]
["DIAM","12.100","12.306","0.206"]
["E.F.","0.004","0.004"]
["CE_FC08_E","Cercle","A","l'entrée"]
["DIAM","12.100","12.308","0.208"]
["E.F.","0.005","0.005"]
["PT_FC08_E","Point","A","titre","info","loca"]
["X","168.000","167.928","-0.200","0.200","-0.072"]
["Y","93.000","92.989","-0.200","0.200","-0.011"]
["PT_FC08_S","Point","A","titre","info","loca"]
["X","168.000","167.898","-0.200","0.200","-0.102"]
["Y","93.000","92.995","-0.200","0.200","-0.005"]
["LOC_FC08","Localis."]
["LOCA","0.000","0.205","0.400","0.205"]
["CE_FC09_S","Cercle","A","la","sortie"]
["DIAM","12.100","12.308","0.208"]
["E.F.","0.004","0.004"]
["CE_FC09_E","Cercle","A","l'entrée"]
["DIAM","12.100","12.307","0.207"]
["E.F.","0.002","0.002"]
["PT_FC09_E","Point","A","titre","info","loca"]
["X","84.000","83.936","-0.200","0.200","-0.064"]
["Y","93.000","93.007","-0.200","0.200","0.007"]
["PT_FC09_S","Point","A","titre","info","loca"]
["X","84.000","83.884","-0.200","0.200","-0.116"]
["Y","93.000","92.985","-0.200","0.200","-0.015"]
["LOC_FC09","Localis."]
["LOCA","0.000","0.234","0.400","0.234"]
["CE_FC10_S","Cercle","A","la","sortie"]
["DIAM","12.100","12.309","0.209"]
["E.F.","0.008","0.008"]
["CE_FC10_E","Cercle","A","l'entrée"]
["DIAM","12.100","12.297","0.197"]
["E.F.","0.013","0.013"]
["PT_FC10_E","Point","A","titre","info","loca","Sect.+","vers","FC06"]
["X","0.000","-0.100","-0.200","0.200","-0.100"]
["Y","93.000","92.954","-0.200","0.200","-0.046"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[119]
[2]
["Ligne",":"]
["Opération",":"]
["L3"]
[30]
[9,"/",12]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["PT_FC10_S","Point","A","titre","info","loca","Sect.+","vers","FC06"]
["X","0.000","-0.085","-0.200","0.200","-0.085"]
["Y","93.000","93.014","-0.200","0.200","0.014"]
["LOC_FC10","Localis."]
["LOCA","0.000","0.220","0.400","0.220"]
["Perçage","logements","injecteurs","coté","face","PAAC"]
["CE_IJ01_E","Cercle","A","l'entrée"]
["DIAM","12.100","12.310","0.210"]
["E.F.","0.012","0.012"]
["CE_IJ01_F","Cercle","Au","fond"]
["DIAM","12.100","12.309","0.209"]
["E.F.","0.001","0.001"]
["PT_IJ01_E","Point","A","titre","info","loca"]
["X","42.000","41.932","-0.200","0.200","-0.068"]
["Y","45.540","45.526","-0.200","0.200","-0.014"]
["PT_IJ01_F","Point","A","titre","info","loca"]
["X","42.000","41.930","-0.200","0.200","-0.070"]
["Y","45.540","45.497","-0.200","0.200","-0.043"]
["LOC_IJ01","Localis."]
["LOCA","0.000","0.164","0.400","0.164"]
["CE_IJ02_E","Cercle","A","l'entrée"]
["DIAM","12.100","12.312","0.212"]
["E.F.","0.002","0.002"]
["CE_IJ02_F","Cercle","Au","fond"]
["DIAM","12.100","12.313","0.213"]
["E.F.","0.004","0.004"]
["PT_IJ02_E","Point","A","titre","info","loca"]
["X","126.000","125.933","-0.200","0.200","-0.067"]
["Y","45.540","45.511","-0.200","0.200","-0.029"]
["PT_IJ02_F","Point","A","titre","info","loca"]
["X","126.000","125.948","-0.200","0.200","-0.052"]
["Y","45.540","45.520","-0.200","0.200","-0.020"]
["LOC_IJ02","Localis."]
["LOCA","0.000","0.146","0.400","0.146"]
["CE_IJ03_E","Cercle","A","l'entrée"]
["DIAM","12.100","12.306","0.206"]
["E.F.","0.014","0.014"]
["CE_IJ03_F","Cercle","Au","fond"]
["DIAM","12.100","12.306","0.206"]
["E.F.","0.002","0.002"]
["PT_IJ03_E","Point","A","titre","info","loca"]
["X","210.000","209.928","-0.200","0.200","-0.072"]
["Y","45.540","45.511","-0.200","0.200","-0.029"]
["PT_IJ03_F","Point","A","titre","info","loca"]
["X","210.000","209.977","-0.200","0.200","-0.023"]
["Y","45.540","45.509","-0.200","0.200","-0.031"]
["LOC_IJ03","Localis."]
["LOCA","0.000","0.155","0.400","0.155"]
["CE_IJ04_E","Cercle","A","l'entrée"]
["DIAM","12.100","12.305","0.205"]
["E.F.","0.007","0.007"]
["CE_IJ04_F","Cercle","Au","fond"]
["DIAM","12.100","12.309","0.209"]
["E.F.","0.003","0.003"]
["PT_IJ04_E","Point","A","titre","info","loca"]
["X","294.000","293.932","-0.200","0.200","-0.068"]
["Y","45.540","45.526","-0.200","0.200","-0.014"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[119]
[2]
["Ligne",":"]
["Opération",":"]
["L3"]
[30]
[10,"/",12]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["PT_IJ04_F","Point","A","titre","info","loca"]
["X","294.000","293.928","-0.200","0.200","-0.072"]
["Y","45.540","45.520","-0.200","0.200","-0.020"]
["LOC_IJ04","Localis."]
["LOCA","0.000","0.150","0.400","0.150"]
["Lamage","et","taraudage","logements","de","bouchon","BC03","et","BC04"]
["TAR_BC03","Cylindre"]
["E.F.","0.099","0.099"]
["PT_BC03_E","Point","A","titre","info","localisation"]
["X","84.000","83.932","-0.250","0.250","-0.068"]
["Y","67.500","67.437","-0.250","0.250","-0.063"]
["PT_BC03_F","Point","A","titre","info","localisation"]
["X","84.000","83.944","-0.250","0.250","-0.056"]
["Y","67.500","67.472","-0.250","0.250","-0.028"]
["LOC_BC03","Localis."]
["LOCA","0.000","0.185","0.500","0.185"]
["KA_BC03","Plan"]
["E.F.","0.001","0.001"]
["POS_KA_BC03_INFO","Point","A","titre","info","loca"]
["Z","69.620","69.712","-0.150","0.150","0.092"]
["LOC_KA_BC03","Localis."]
["LOCA","0.000","0.184","0.300","0.184"]
["PERP_BC03","Perpendic."]
["PERP","0.000","0.036","0.100","0.036"]
["TAR_BC04","Cylindre"]
["E.F.","0.114","0.114"]
["PT_BC04_E","Point","A","titre","info","localisation"]
["X","252.000","251.963","-0.250","0.250","-0.037"]
["Y","67.500","67.404","-0.250","0.250","-0.096"]
["PT_BC04_F","Point","A","titre","info","localisation"]
["X","252.000","251.918","-0.250","0.250","-0.082"]
["Y","67.500","67.500","-0.250","0.250","-0.000"]
["LOC_BC04","Localis."]
["LOCA","0.000","0.205","0.500","0.205"]
["KA_BC04","Plan"]
["E.F.","0.002","0.002"]
["POS_KA_BC04_INFO","Point","A","titre","info","loca"]
["Z","69.620","69.707","-0.150","0.150","0.087"]
["LOC_KA_BC04","Localis."]
["LOCA","0.000","0.175","0.300","0.175"]
["PERP_BC04","Perpendic."]
["PERP","0.000","0.106","0.100","0.106","0.006"]
["Lamage","logements","de","bouchon","BC03","et","BC04","à","titre","indicatif"]
["LAM_BC03","Cercle","A","titre","info"]
["DIAM","24.000","25.847","1.847"]
["X","84.000","83.945","-0.250","0.250","-0.055"]
["Y","67.500","67.454","-0.250","0.250","-0.046"]
["E.F.","0.002","0.002"]
["COA_BC03","Coaxialité"]
["COAX","0.000","0.043","0.250","0.043"]
["LAM_BC04","Cercle","A","titre","info"]
["DIAM","24.000","25.876","1.876"]
["X","252.000","251.946","-0.250","0.250","-0.054"]
["Y","67.500","67.469","-0.250","0.250","-0.031"]
["E.F.","0.009","0.009"]
["COA_BC04","Coaxialité"]
["COAX","0.000","0.134","0.250","0.134"]
["Perçage","logements","injecteurs","coté","face","comb."]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[119]
[2]
["Ligne",":"]
["Opération",":"]
["L3"]
[30]
[11,"/",12]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]
["NOMINAL","MESURE","TOL-","TOL+","ECART","TENDANCE"]
["PER_IJ01_E","Cercle","A","l'entrée"]
["DIAM","6.780","6.785","0.005"]
["E.F.","0.006","0.006"]
["PER_IJ01_F","Cercle","Au","fond"]
["DIAM","6.780","6.781","0.001"]
["E.F.","0.001","0.001"]
["PT_PER_IJ01_E","Point","A","titre","info","loca"]
["X","42.000","42.006","-0.200","0.200","0.006"]
["Y","45.540","45.524","-0.200","0.200","-0.016"]
["PT_PER_IJ01_F","Point","A","titre","info","loca"]
["X","42.000","41.992","-0.200","0.200","-0.008"]
["Y","45.540","45.519","-0.200","0.200","-0.021"]
["LOC_PER_IJ01","Localis."]
["LOCA","0.000","0.046","0.400","0.046"]
["PER_IJ02_E","Cercle","A","l'entrée"]
["DIAM","6.780","6.786","0.006"]
["E.F.","0.005","0.005"]
["PER_IJ02_F","Cercle","Au","fond"]
["DIAM","6.780","6.781","0.001"]
["E.F.","0.000","0.000"]
["PT_PER_IJ02_E","Point","A","titre","info","loca"]
["X","126.000","126.012","-0.200","0.200","0.012"]
["Y","45.540","45.541","-0.200","0.200","0.001"]
["PT_PER_IJ02_F","Point","A","titre","info","loca"]
["X","126.000","126.009","-0.200","0.200","0.009"]
["Y","45.540","45.540","-0.200","0.200","-0.000"]
["LOC_PER_IJ02","Localis."]
["LOCA","0.000","0.025","0.400","0.025"]
["PER_IJ03_E","Cercle","A","l'entrée"]
["DIAM","6.780","6.783","0.003"]
["E.F.","0.002","0.002"]
["PER_IJ03_F","Cercle","Au","fond"]
["DIAM","6.780","6.781","0.001"]
["E.F.","0.000","0.000"]
["PT_PER_IJ03_E","Point","A","titre","info","loca"]
["X","210.000","210.002","-0.200","0.200","0.002"]
["Y","45.540","45.537","-0.200","0.200","-0.003"]
["PT_PER_IJ03_F","Point","A","titre","info","loca"]
["X","210.000","210.000","-0.200","0.200","-0.000"]
["Y","45.540","45.544","-0.200","0.200","0.004"]
["LOC_PER_IJ03","Localis."]
["LOCA","0.000","0.008","0.400","0.008"]
["PER_IJ04_E","Cercle","A","l'entrée"]
["DIAM","6.780","6.788","0.008"]
["E.F.","0.000","0.000"]
["PER_IJ04_F","Cercle","Au","fond"]
["DIAM","6.780","6.780","0.000"]
["E.F.","0.000","0.000"]
["PT_PER_IJ04_E","Point","A","titre","info","loca"]
["X","294.000","294.005","-0.200","0.200","0.005"]
["Y","45.540","45.528","-0.200","0.200","-0.012"]
["PT_PER_IJ04_F","Point","A","titre","info","loca"]
["X","294.000","294.005","-0.200","0.200","0.005"]
["Y","45.540","45.528","-0.200","0.200","-0.012"]
["LOC_PER_IJ04","Localis."]
["LOCA","0.000","0.026","0.400","0.026"]
["DUREE-PROG","Texte/Valeur","Durée","du","programme","en","Minutes"]
["VAL","0.000","29.411","0.000","120.000","29.411"]
["DESIGNATION",":"]
["Type",":"]
["N°","Piece",":"]
["N°","Adaptateur",":"]
["N°","Meteor",":"]
["CULASSE"]
["DV5R"]
[119]
[2]
["Ligne",":"]
["Opération",":"]
["L3"]
[30]
[12,"/",12]
["Metrologic","Group","-","M8.1250.XG",14]
["\f"]