{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Cuve soude","Cuve acide","Récap NEP","Recettelavage","Récap lavages"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":8,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cuve soude","index":0,"n_rows":2,"n_cols":17,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Date","Paramètre principal modifié","Paramètre 2ndaire","Situation avant modification","Motif de modification","Situation après modification","Courbes","pH -1","Nitrates -1","DCO -1","Entero -1","pH -2","Nitrates -2","DCO -2","Entero -2","FMA -2","Validation"]
["2016-12-13","Température","Mini"]

{"sheet":"Cuve acide","index":1,"n_rows":2,"n_cols":17,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Date","Paramètre principal modifié","Paramètre 2ndaire","Situation avant modification","Motif de modification","Situation après modification","Courbes","pH -1","Nitrates -1","DCO -1","Entero -1","pH -2","Nitrates -2","DCO -2","Entero -2","FMA -2","Validation"]
["2016-12-15","Température","Mini"]

{"sheet":"Récap NEP","index":2,"n_rows":6,"n_cols":13,"rows_kept":6,"cut":false,"hidden":false,"merged":[[2,2,2,4],[2,5,2,7],[2,8,2,12]]}
["Date de maj",{"$f":"MAX(MAX('Cuve soude'!A2:A1827),MAX('Cuve acide'!A2:A1827),MAX(Recettelavage!B4:B1829))","v":"2016-12-22"}]
[]
[null,null,"Température",null,null,"Conductivité",null,null,"Matériel"]
[null,"Produit chimique","Mini","Consigne","Maxi","Mini","Consigne","Maxi","Cuve","Tuyauterie","Vanne","Sonde t°","Sonde conductivité"]
["Cuve soude"]
["Cuve acide"]

{"sheet":"Recettelavage","index":3,"n_rows":30,"n_cols":40,"rows_kept":30,"cut":false,"hidden":false,"merged":[]}
["Date de maj",{"$f":"MAX(Recettelavage!B4:B1829)","v":"2016-12-22"}]
[]
["Date prévue","Date réalisée","N° Lavage","Equipement","Paramètre principal modifié","Paramètre 2ndaire","Situation avant modification","Motif","Situation après modification","T° ENR","Conductivité ENR","Débits ENR","Temps ENR","Date","Temps depuis dernier lavage","pH -1","Nitrates -1","DCO -1","Entero -1","Date","Temps depuis dernier lavage","pH -2","Nitrates -2","DCO -2","Entero -2","FMA 30°C -2","Date","Temps depuis dernier lavage","pH -3","Nitrates -3","DCO -3","Entero -3","FMA 30°C -3","Validation"]
[null,"2016-12-15",2,null,"Temps","Temps de Pousse envoi station vers boule de lavage",300,"Pas assez long pour diminuer la charge",360,"C/NC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Noir si entero1 NC",null,null,null,null,null,null,null,"oui/non"]
[null,"2016-12-16",3,null,"Matériel","Tuyauterie",63,"Trop de raccords",51]
[null,"2016-12-17",2,null,"Temps","Temps de Pousse envoi station vers boule de lavage",360,"Besoin d'économiser de l'eau propre",330]
[null,"2016-12-18",1,null,"Débit","Envoi",31000,"Pas en accord avec les préco",25000]
[null,"2016-12-19",3,null,"Temps","Temps de circulation soude",600,"Objectif 900s",900]
[null,"2016-12-20",1,null,"Matériel","Boule de lavage","RS400","Sous-dimmensionnée","RS500"]
[null,"2016-12-21",2,null,"Temps","Temps de circulation soude",600,"Objectif 900s",900]
[null,"2016-12-22",1,null,"Débit","Retour",18000,"Pas en accord avec les préco",25000]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temps","Matériel","Débit","Conductivité","Température"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temps Prélavage","Tuyauterie","Envoi","Seuil de décompte temps","Seuil de décompte temps"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temps de Pousse envoi station vers boule de lavage","Pompe d'envoi","Retour","Seuil de tri","Seuil de tri"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temps Mini vidange tank après envoi vers boule","Pompe de retour"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temps Maxi vidange tank après envoi vers boule","Boule de lavage"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temps max retour produit vers station"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temps de circulation soude"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temps de trempage soude"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temps pour éliminer queue de dilution soude"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temps de rinçage intermédiaire après soude"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temps de circulation acide"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temps de trempage acide"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temps pour éliminer queue de dilution acide"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temps de dernier rinçage"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Temps d'égouttage"]

{"sheet":"Récap lavages","index":4,"n_rows":9,"n_cols":27,"rows_kept":9,"cut":false,"hidden":false,"merged":[[1,19,1,20],[1,21,1,22],[1,23,1,26],[1,3,1,16],[1,17,1,18]]}
["Date de maj",{"$f":"MAX(Recettelavage!B4:B1829)","v":"2016-12-22"}]
[null,null,null,"Temps",null,null,null,null,null,null,null,null,null,null,null,null,null,"Conductivité",null,"Température",null,"Débit",null,"Matériel"]
["N° lavage","Equipement","NEP","Temps Prélavage","Temps de Pousse envoi station vers boule de lavage","Temps Mini vidange tank après envoi vers boule","Temps Maxi vidange tank après envoi vers boule","Temps max retour produit vers station","Temps de circulation soude","Temps de trempage soude","Temps pour éliminer queue de dilution soude","Temps de rinçage intermédiaire après soude","Temps de circulation acide","Temps de trempage acide","Temps pour éliminer queue de dilution acide","Temps de dernier rinçage","Temps d'égouttage","Seuil de décompte temps","Seuil de tri","Seuil de décompte temps","Seuil de tri","Envoi","Retour","Tuyauterie","Pompe d'envoi","Pompe de retour","Boule de lavage"]
[1,"Tank 31",4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25000,25000,null,null,null,"RS500"]
[2,"Tank 32",4,null,330,null,null,null,900]
[3,"Tank 33",3,null,null,null,null,null,900,null,null,null,null,null,null,null,null,null,null,null,null,null,null,51]
[]
[]
[null,null,null,null,"En jaune ce que je souhaiterai voir apparaître"]