{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Feuil1"],"not_rendered":{"charts":1,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Feuil1","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[[9,0,10,1],[1,4,2,5],[3,4,4,5],[5,4,6,5],[7,4,8,5],[9,4,10,5],[9,2,10,3],[0,0,0,5],[1,0,2,1],[3,0,4,1],[5,0,6,1],[7,0,8,1],[1,2,2,3],[3,2,4,3],[5,2,6,3],[7,2,8,3]]}
["Indicateur de passage de vitesse en fonction des tours moteur"]
["Sous-régime",null,"1200-1800"]
[]
["léger sous-régime",null,"1800-2800"]
[]
["régime parfait",null,"2800-4900"]
[]
["léger sur-régime",null,"4900-5900"]
[]
["Sur-régime",null,"5900-6500"]
[]
[]
[]
[]
[null,null,"blanche",1200]
[null,null,"Bleu marine",600,null,null,null,1]
[null,null,"Bleu ciel",1000,null,null,null,2]
[null,null,"Vert",2100,null,null,null,2200]
[null,null,"Jaune",1000]
[null,null,"Rouge",600]
[null,null,"Invisible",{"$f":"SUM(D16:D20)-D15","v":4100}]
[]
[null,null,"aiguille",0]
[null,null,"largeur",40]
[null,null,"invisible",{"$f":"SUM(D15:D21)-(D24+D23)","v":10560}]