{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Feuil1","Feuil2","Feuil3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Feuil1","index":0,"n_rows":210,"n_cols":6,"rows_kept":210,"cut":false,"hidden":false,"merged":[[207,3,208,5],[209,3,209,5],[210,3,216,5],[205,4,206,4],[205,0,205,2],[206,0,206,2],[193,0,193,2],[194,0,194,2],[195,0,195,2],[196,0,196,2],[197,0,197,2],[198,0,198,2],[199,0,199,2],[200,0,200,2],[201,0,201,2],[202,0,202,2],[203,0,203,2],[204,0,204,2],[184,0,184,2],[185,0,185,2],[186,0,186,2],[187,0,187,2],[188,0,188,2],[189,0,189,2],[190,0,190,2],[191,0,191,2],[192,0,192,2],[175,0,175,2],[176,0,176,2],[177,0,177,2],[178,0,178,2],[179,0,179,2],[180,0,180,2],[181,0,181,2],[182,0,182,2],[183,0,183,2],[166,0,166,2],[167,0,167,2],[168,0,168,2],[169,0,169,2],[170,0,170,2],[171,0,171,2],[172,0,172,2],[173,0,173,2],[174,0,174,2],[157,0,157,2],[158,0,158,2],[159,0,159,2],[160,0,160,2],[161,0,161,2],[162,0,162,2],[163,0,163,2],[164,0,164,2],[165,0,165,2],[205,5,206,5],[5,0,5,2],[128,0,128,2],[129,0,129,2],[130,0,130,2],[131,0,131,2],[125,0,125,2],[134,0,134,2],[136,0,136,2],[112,0,112,2],[114,0,114,2],[115,0,115,2],[119,0,119,2],[120,0,120,2],[121,0,121,2],[123,0,123,2],[124,0,124,2],[113,0,113,2],[116,0,116,2],[117,0,117,2],[118,0,118,2],[132,0,132,2],[133,0,133,2],[135,0,135,2],[122,0,122,2],[127,0,127,2],[79,0,79,2],[22,0,22,2],[85,0,85,2],[61,0,61,2],[60,0,60,2],[105,0,105,2],[106,0,106,2],[107,0,107,2],[108,0,108,2],[86,0,86,2],[87,0,87,2],[88,0,88,2],[89,0,89,2],[90,0,90,2],[80,0,80,2],[81,0,81,2],[82,0,82,2],[83,0,83,2],[84,0,84,2],[75,0,75,2],[76,0,76,2],[77,0,77,2],[98,0,98,2],[99,0,99,2],[101,0,101,2],[102,0,102,2],[103,0,103,2],[104,0,104,2],[91,0,91,2],[92,0,92,2],[93,0,93,2],[95,0,95,2],[96,0,96,2],[97,0,97,2],[94,0,94,2],[52,0,52,2],[53,0,53,2],[54,0,54,2],[55,0,55,2],[56,0,56,2],[57,0,57,2],[46,0,46,2],[47,0,47,2],[48,0,48,2],[49,0,49,2],[50,0,50,2],[51,0,51,2],[78,0,78,2],[66,0,66,2],[67,0,67,2],[71,0,71,2],[72,0,72,2],[73,0,73,2],[74,0,74,2],[58,0,58,2],[59,0,59,2],[62,0,62,2],[63,0,63,2],[64,0,64,2],[65,0,65,2],[70,0,70,2],[68,0,68,2],[69,0,69,2],[42,0,42,2],[43,0,43,2],[44,0,44,2],[45,0,45,2],[29,0,29,2],[35,0,35,2],[36,0,36,2],[37,0,37,2],[38,0,38,2],[39,0,39,2],[32,0,32,2],[34,0,34,2],[30,0,30,2],[31,0,31,2],[33,0,33,2],[12,0,12,2],[13,0,13,2],[14,0,14,2],[4,0,4,2],[23,0,23,2],[16,0,16,2],[24,0,24,2],[40,0,40,2],[41,0,41,2],[111,0,111,2],[7,0,7,2],[8,0,8,2],[9,0,9,2],[1,0,2,2],[6,0,6,2],[1,3,2,3],[1,4,2,4],[25,0,25,2],[26,0,26,2],[27,0,27,2],[28,0,28,2],[1,5,2,5],[17,0,17,2],[18,0,18,2],[19,0,19,2],[20,0,20,2],[21,0,21,2],[10,0,10,2],[11,0,11,2],[126,0,126,2],[141,0,141,2],[137,0,137,2],[138,0,138,2],[100,0,100,2],[156,0,156,2],[146,0,146,2],[147,0,147,2],[148,0,148,2],[149,0,149,2],[150,0,150,2],[151,0,151,2],[139,0,139,2],[140,0,140,2],[142,0,142,2],[143,0,143,2],[144,0,144,2],[145,0,145,2],[152,0,152,2],[153,0,153,2],[154,0,154,2],[155,0,155,2],[109,0,109,2],[110,0,110,2]]}
[]
["NOMENCLATURE",null,null,"Pds","Qtté","Pds total"]
[]
[]
["cale bois",null,null,1,null,{"$f":"D5*E5","v":0}]
["cale de pied jaune",null,null,0.2,null,{"$f":"D6*E6","v":0}]
["socle réglable 0,50m",null,null,3.47,null,{"$f":"D7*E7","v":0}]
["socle réglable 0,80m",null,null,7,null,{"$f":"D8*E8","v":0}]
["socle orientable",null,null,5,null,{"$f":"D9*E9","v":0}]
["embase",null,null,1.7,null,{"$f":"D10*E10","v":0}]
["poteau 0,50m",null,null,2.9,null,{"$f":"D11*E11","v":0}]
["poteau 1,00m",null,null,5.12,null,{"$f":"D12*E12","v":0}]
["poteau 1,50m",null,null,7.34,null,{"$f":"D13*E13","v":0}]
["poteau 2,00m",null,null,9.5500000000000007,null,{"$f":"D14*E14","v":0}]
["poteau 3,00m",null,null,11.73,null,{"$f":"D15*E15","v":0}]
["goupille",null,null,0.1,null,{"$f":"D16*E16","v":0}]
["Cadre 2 x 0,75",null,null,18,null,{"$f":"D17*E17","v":0}]
["poteau sans goujon 0,50m",null,null,2,null,{"$f":"D18*E18","v":0}]
["poteau sans goujon 1,00m",null,null,4.5999999999999996,null,{"$f":"D19*E19","v":0}]
["poteau sans goujon 1,50m",null,null,6.9,null,{"$f":"D20*E20","v":0}]
["poteau sans goujon 2,00m",null,null,9,null,{"$f":"D21*E21","v":0}]
["poteau sans goujon 3,00m",null,null,13.5,null,{"$f":"D22*E22","v":0}]
["double clavette",null,null,1,null,{"$f":"D23*E23","v":0}]
["lisse 0,40m",null,null,2.35,null,{"$f":"D24*E24","v":0}]
["lisse 0,70m",null,null,3.19,null,{"$f":"D25*E25","v":0}]
["lisse 1,00m",null,null,4.22,null,{"$f":"D26*E26","v":0}]
["lisse 1,50m",null,null,5.94,null,{"$f":"D27*E27","v":0}]
["lisse 2,00m",null,null,7.67,null,{"$f":"D28*E28","v":0}]
["lisse 2,50m",null,null,9.39,null,{"$f":"D29*E29","v":0}]
["lisse 3,00m",null,null,11.11,null,{"$f":"D30*E30","v":0}]
["garde-corps 0,70m",null,null,7.5,null,{"$f":"D31*E31","v":0}]
["garde-corps 1,00m",null,null,8.5,null,{"$f":"D32*E32","v":0}]
["garde-corps 1,50m",null,null,9,null,{"$f":"D33*E33","v":0}]
["garde-corps 2,00m",null,null,10,null,{"$f":"D34*E34","v":0}]
["garde-corps 3,00m",null,null,15.5,null,{"$f":"D35*E35","v":0}]
["lisse renforcée 1,00m",null,null,8,null,{"$f":"D36*E36","v":0}]
["lisse renforcée 1,50m",null,null,11.39,null,{"$f":"D37*E37","v":0}]
["lisse renforcée 2,00m",null,null,18.010000000000002,null,{"$f":"D38*E38","v":0}]
["lisse renforcée 2,50m",null,null,21.91,null,{"$f":"D39*E39","v":0}]
["lisse renforcée 3,00m",null,null,19.7,null,{"$f":"D40*E40","v":0}]
["console 0,40m",null,null,3.4,null,{"$f":"D41*E41","v":0}]
["console 0,70m",null,null,6,null,{"$f":"D42*E42","v":0}]
["console 1,00m",null,null,12,null,{"$f":"D43*E43","v":0}]
["diagonale 2,00 x 0,70m",null,null,8.6,null,{"$f":"D44*E44","v":0}]
["diagonale 2,00 x 1,00m",null,null,9,null,{"$f":"D45*E45","v":0}]
["diagonale 2,00 x 1,50m",null,null,9.6999999999999993,null,{"$f":"D46*E46","v":0}]
["diagonale 2,00 x 2,00m",null,null,10.8,null,{"$f":"D47*E47","v":0}]
["diagonale 2,00 x 2,50m",null,null,12.1,null,{"$f":"D48*E48","v":0}]
["diagonale 2,00 x 3,00m",null,null,13.5,null,{"$f":"D49*E49","v":0}]
["poutre acier avec piquage 4,00m",null,null,51.9,null,{"$f":"D50*E50","v":0}]
["poutre acier avec piquage 5,00m",null,null,63.1,null,{"$f":"D51*E51","v":0}]
["poutre acier avec piquage 6,00m",null,null,71.8,null,{"$f":"D52*E52","v":0}]
["poutre acier sans piquage 4,00m",null,null,40,null,{"$f":"D53*E53","v":0}]
["poutre acier sans piquage 5,00m",null,null,50,null,{"$f":"D54*E54","v":0}]
["poutre acier sans piquage 6,00m",null,null,60,null,{"$f":"D55*E55","v":0}]
["poutre aluminium 3,00m",null,null,18,null,{"$f":"D56*E56","v":0}]
["poutre aluminium 4,00m",null,null,24,null,{"$f":"D57*E57","v":0}]
["poutre aluminium 5,00m",null,null,30,null,{"$f":"D58*E58","v":0}]
["poutre aluminium 6,00m",null,null,36,null,{"$f":"D59*E59","v":0}]
["poutre aluminium 8,00m",null,null,50,null,{"$f":"D60*E60","v":0}]
["liaison poutre",null,null,2.5,null,{"$f":"D61*E61","v":0}]
["liaison faitière",null,null,3,null,{"$f":"D62*E62","v":0}]
["plancher acier 0,30 x 0,70m",null,null,7.7149999999999999,null,{"$f":"D63*E63","v":0}]
["plancher acier 0,30 x 1,00m",null,null,10.44,null,{"$f":"D64*E64","v":0}]
["plancher acier 0,30 x 1,50m",null,null,13.73,null,{"$f":"D65*E65","v":0}]
["plancher acier 0,30 x 2,00m",null,null,17.02,null,{"$f":"D66*E66","v":0}]
["plancher acier 0,30 x 2,50m",null,null,20.309999999999999,null,{"$f":"D67*E67","v":0}]
["plancher acier 0,30 x 3,00m",null,null,23.6,null,{"$f":"D68*E68","v":0}]
["plancher alu/bois 0,60 x 1,50m",null,null,12.3,null,{"$f":"D69*E69","v":0}]
["plancher alu/bois 0,60 x 2,00m",null,null,16,null,{"$f":"D70*E70","v":0}]
["plancher alu/bois 0,60 x 3,00m",null,null,18.600000000000001,null,{"$f":"D71*E71","v":0}]
["couvre plancher 0,75m",null,null,7.5,null,{"$f":"D72*E72","v":0}]
["couvre plancher 1,05m",null,null,6.1,null,{"$f":"D73*E73","v":0}]
["couvre plancher 1,50m",null,null,8.9,null,{"$f":"D74*E74","v":0}]
["couvre plancher 2,00m",null,null,11.2,null,{"$f":"D75*E75","v":0}]
["couvre plancher 2,50m",null,null,14.9,null,{"$f":"D76*E76","v":0}]
["couvre plancher 3,00m",null,null,17.899999999999999,null,{"$f":"D77*E77","v":0}]
["plancher trappe 0,60 x 1,50m",null,null,23,null,{"$f":"D78*E78","v":0}]
["plancher trappe 0,60 x 2,00m",null,null,25,null,{"$f":"D79*E79","v":0}]
["plancher trappe 0,60 x 2,50m avec échelle",null,null,27,null,{"$f":"D80*E80","v":0}]
["plancher trappe 0,60 x 3,00m avec échelle",null,null,29,null,{"$f":"D81*E81","v":0}]
["échelle 2,00m",null,null,5,null,{"$f":"D82*E82","v":0}]
["échelle 3,00m",null,null,7,null,{"$f":"D83*E83","v":0}]
["échelle 4,00m",null,null,10,null,{"$f":"D84*E84","v":0}]
["échelle",null,null,null,null,{"$f":"D85*E85","v":0}]
["plinthe 0,70m",null,null,2,null,{"$f":"D86*E86","v":0}]
["plinthe 1,00m",null,null,3.1,null,{"$f":"D87*E87","v":0}]
["plinthe 1,50m",null,null,4.95,null,{"$f":"D88*E88","v":0}]
["plinthe 2,00m",null,null,6.2,null,{"$f":"D89*E89","v":0}]
["plinthe 2,50m",null,null,7.4,null,{"$f":"D90*E90","v":0}]
["plinthe 3,00m",null,null,8.6,null,{"$f":"D91*E91","v":0}]
["rack de stockage",null,null,49,null,{"$f":"D92*E92","v":0}]
["rack de stockage grillagé",null,null,80,null,{"$f":"D93*E93","v":0}]
["raccord angle droit 49mm",null,null,1.32,null,{"$f":"D94*E94","v":0}]
["crapaud",null,null,1.5,null,{"$f":"D95*E95","v":0}]
["raccord angle variable 49mm",null,null,1.42,null,{"$f":"D96*E96","v":0}]
["raccord angle droit 49 / 60mm",null,null,1.7,null,{"$f":"D97*E97","v":0}]
["raccord angle variable 49 / 60mm",null,null,1.6,null,{"$f":"D98*E98","v":0}]
["collier de jonction",null,null,1.41,null,{"$f":"D99*E99","v":0}]
["cale cp pour vérin d'amarrage",null,null,0.5,null,{"$f":"D100*E100","v":0}]
["clavette sur 1/2 collier",null,null,1.3,null,{"$f":"D101*E101","v":0}]
["vérin d'amarrage",null,null,2.9,null,{"$f":"D102*E102","v":0}]
["goujon sur collier",null,null,2.2999999999999998,null,{"$f":"D103*E103","v":0}]
["roue sur vérin 300kg",null,null,9,null,{"$f":"D104*E104","v":0}]
["roue sur vérin 700kg",null,null,12,null,{"$f":"D105*E105","v":0}]
["barre d'ancrage 0,50m",null,null,3,null,{"$f":"D106*E106","v":0}]
["barre d'ancrage 1,00m",null,null,5,null,{"$f":"D107*E107","v":0}]
["barre d'ancrage 1,50m",null,null,6,null,{"$f":"D108*E108","v":0}]
["piton 120mm",null,null,0.1,null,{"$f":"D109*E109","v":0}]
["piton 160mm",null,null,0.15,null,{"$f":"D110*E110","v":0}]
["piton 300mm",null,null,0.2,null,{"$f":"D111*E111","v":0}]
["cheville 70 x 14mm",null,null,0.01,null,{"$f":"D112*E112","v":0}]
["fourreau 2,00m",null,null,8,null,{"$f":"D113*E113","v":0}]
["fourreau 1,00m",null,null,4,null,{"$f":"D114*E114","v":0}]
["contreplaqué 1,20 x 2,50m ep 18mm",null,null,12,null,{"$f":"D115*E115","v":0}]
["contreplaqué découpé  ep 18mm",null,null,4,null,{"$f":"D116*E116","v":0}]
["polyfoam 2,50 x 1,20m",null,null,2,null,{"$f":"D117*E117","v":0}]
["polyfoam 1,25  x 1,20m",null,null,1,null,{"$f":"D118*E118","v":0}]
["polyfoam 2,50 x 0,60m",null,null,1,null,{"$f":"D119*E119","v":0}]
["planche 38 x 200mm lg 1,00m",null,null,3,null,{"$f":"D120*E120","v":0}]
["planche 38 x 200mm lg 1,50m",null,null,4.5,null,{"$f":"D121*E121","v":0}]
["planche 38 x 200mm lg 2,00m",null,null,6,null,{"$f":"D122*E122","v":0}]
["planche 38 x 200mm lg 2,50m",null,null,7.5,null,{"$f":"E123*D123","v":0}]
["planche 38 x 200mm lg 3,00m",null,null,9,null,{"$f":"D124*E124","v":0}]
["planche 38 x 200mm lg 4,00m",null,null,12,null,{"$f":"D125*E125","v":0}]
["tube<0,70m",null,null,2,null,{"$f":"D126*E126","v":0}]
["tube 0,70m",null,null,2.2400000000000002,null,{"$f":"D127*E127","v":0}]
["tube 1,20m",null,null,3.84,null,{"$f":"D128*E128","v":0}]
["tube 1,70m",null,null,5.44,null,{"$f":"D129*E129","v":0}]
["tube 2,20m",null,null,7.04,null,{"$f":"D130*E130","v":0}]
["tube 2,70m",null,null,8.64,null,{"$f":"D131*E131","v":0}]
["tube 3,20m",null,null,10.24,null,{"$f":"D132*E132","v":0}]
["tube 4,50m",null,null,14.4,null,{"$f":"D133*E133","v":0}]
["tube 5,20m",null,null,16.64,null,{"$f":"D134*E134","v":0}]
["tube 6,40m",null,null,20.48,null,{"$f":"D135*E135","v":0}]
["Platine"]
["pince à tole petite",null,null,0.5,null,{"$f":"D137*E137","v":0}]
["pince à tole grande",null,null,0.6,null,{"$f":"D138*E138","v":0}]
["tôle 0,90 x 2,00m",null,null,8,null,{"$f":"D139*E139","v":0}]
["tôle 0,90 x 2,10m",null,null,8.5,null,{"$f":"D140*E140","v":0}]
["bâche 170gr/m² 3,00m  le ml",null,null,0.16500000000000001,null,{"$f":"D141*E141","v":0}]
["bâche 170gr/m² 2.50m  le ml",null,null,0.16500000000000001,null,{"$f":"D142*E142","v":0}]
["colson les 100",null,null,0.1,null,{"$f":"D143*E143","v":0}]
["limon avec palier 0,90 x 3,00m",null,null,25,null,{"$f":"D144*E144","v":0}]
["garde corps de limon",null,null,7,null,{"$f":"D145*E145","v":0}]
["garde corps de palier",null,null,2.5,null,{"$f":"D146*E146","v":0}]
["limon droit 0,90 x 2,50m",null,null,20,null,{"$f":"D147*E147","v":0}]
["limon droit 0,90 x 1,50m",null,null,15,null,{"$f":"D148*E148","v":0}]
["limon droit 0,90 x 1,00m",null,null,10,null,{"$f":"D149*E149","v":0}]
["étais SN80 - 0,55/0,80m",null,null,5,null,{"$f":"D150*E150","v":0}]
["étais SN120 - 0,75/1,20m",null,null,6,null,{"$f":"D151*E151","v":0}]
["étais SN175 - 1,00/1,75m",null,null,7.2,null,{"$f":"D152*E152","v":0}]
["étais SE300 - 1,70/3,00m",null,null,16,null,{"$f":"D153*E153","v":0}]
["étais SE400 - 2,20/4,00m",null,null,17.5,null,{"$f":"D154*E154","v":0}]
["sécurétai - 1,50/1,50m",null,null,12,null,{"$f":"D155*E155","v":0}]
["échelle ASE 0,70m",null,null,10.6,null,{"$f":"D156*E156","v":0}]
["échelle ASE 1,40m",null,null,19.899999999999999,null,{"$f":"D157*E157","v":0}]
["garde corps ASE 1,80m",null,null,11.8,null,{"$f":"D158*E158","v":0}]
["croisillon ASE 0,70m",null,null,4.25,null,{"$f":"D159*E159","v":0}]
["vérin de pied ASE",null,null,6.2,null,{"$f":"D160*E160","v":0}]
["vérin de tête ASE",null,null,6,null,{"$f":"D161*E161","v":0}]
["plancher trappe ASE 0,60 x 1,80m",null,null,20.6,null,{"$f":"D162*E162","v":0}]
["plancher acier ASE 0,30 x 1,80m",null,null,14.8,null,{"$f":"D163*E163","v":0}]
["fourche double entrée",null,null,2.5,null,{"$f":"D164*E164","v":0}]
["fourche réglable",null,null,6,null,{"$f":"D165*E165","v":0}]
["trapéze T28.100P",null,null,7.8,null,{"$f":"D166*E166","v":0}]
["trapéze T28.100G",null,null,9.0500000000000007,null,{"$f":"D167*E167","v":0}]
["trapéze T28.150P",null,null,9.5,null,{"$f":"D168*E168","v":0}]
["trapéze T28.150G",null,null,11.15,null,{"$f":"D169*E169","v":0}]
["raccord d'extrémité T28 RE.100",null,null,3.13,null,{"$f":"D170*E170","v":0}]
["raccord d'extrémité T28 RE.150",null,null,4.3,null,{"$f":"D171*E171","v":0}]
["diagonale horizontale T28 DH.100 x 100",null,null,3.5,null,{"$f":"D172*E172","v":0}]
["diagonale horizontale T28 DH.100 x 150",null,null,4.3499999999999996,null,{"$f":"D173*E173","v":0}]
["diagonale horizontale T28 DH.150 x 150",null,null,5.01,null,{"$f":"D174*E174","v":0}]
["socle réglable T28 SR. Ø34",null,null,6.8,null,{"$f":"D175*E175","v":0}]
["fourche réglable T28 FR. Ø34 2M",null,null,9.1999999999999993,null,{"$f":"D176*E176","v":0}]
["fourche réglable T28 FR. Ø34 3M",null,null,10.5,null,{"$f":"D177*E177","v":0}]
["trapéze T40.60P",null,null,8.4,null,{"$f":"D178*E178","v":0}]
["trapéze T40.60G",null,null,10.3,null,{"$f":"D179*E179","v":0}]
["trapéze T40.100P",null,null,9.6999999999999993,null,{"$f":"D180*E180","v":0}]
["trapéze T40.100G",null,null,13.4,null,{"$f":"D181*E181","v":0}]
["raccord d'extrémité T40 RE.60",null,null,3.05,null,{"$f":"D182*E182","v":0}]
["raccord d'extrémité T40 RE.100",null,null,3.9,null,{"$f":"D183*E183","v":0}]
["diagonale horizontale T40 DH.60 x 60",null,null,3,null,{"$f":"D184*E184","v":0}]
["diagonale horizontale T40 DH.60 x 100",null,null,3.1,null,{"$f":"D185*E185","v":0}]
["diagonale horizontale T40 DH.100 x 100",null,null,3.75,null,{"$f":"D186*E186","v":0}]
["socle réglable T40 SR. Ø42",null,null,9.4499999999999993,null,{"$f":"D187*E187","v":0}]
["fourche réglable T40 FR. Ø40 3M",null,null,14.2,null,{"$f":"D188*E188","v":0}]
["poutrelle H20 lg 1,00m",null,null,5,null,{"$f":"D189*E189","v":0}]
["poutrelle H20 lg 2,45m",null,null,12.25,null,{"$f":"D190*E190","v":0}]
["poutrelle H20 lg 2,90m",null,null,14.5,null,{"$f":"D191*E191","v":0}]
["poutrelle H20 lg 3,30m",null,null,16.5,null,{"$f":"D192*E192","v":0}]
["poutrelle H20 lg 3,90m",null,null,19.5,null,{"$f":"D193*E193","v":0}]
["tube GC diam.40 lg 1.00m",null,null,null,null,{"$f":"D194*E194","v":0}]
["Poutrelle AL200 3,60",null,null,23.76,null,{"$f":"D195*E195","v":0}]
["tête d'étai",null,null,4.5999999999999996,null,{"$f":"D196*E196","v":0}]
["poutrelle primaire 200",null,null,14.5,null,{"$f":"D197*E197","v":0}]
["poutrelle primaire 170",null,null,13.2,null,{"$f":"D198*E198","v":0}]
["poutrelle primaire 150",null,null,11.6,null,{"$f":"D199*E199","v":0}]
["poutrelle primaire 115",null,null,8.8000000000000007,null,{"$f":"D200*E200","v":0}]
["poutrelle primaire 90",null,null,7,null,{"$f":"D201*E201","v":0}]
["poutrelle secondaire 170",null,null,6.1,null,{"$f":"D202*E202","v":0}]
["poutrelle secondaire 150",null,null,5.4,null,{"$f":"D203*E203","v":0}]
["poutrelle secondaire 115",null,null,4.2,null,{"$f":"D204*E204","v":0}]
["trépied",null,null,null,null,{"$f":"D205*E205","v":0}]
[null,null,null,null,null,{"$f":"SUM(F5:F205)","v":0}]
[]
[null,null,null,"CLIENT"]
[]
[null,null,null,"NOM et SIGNATURE"]

{"sheet":"Feuil2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Feuil3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}